{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Kurzwaffen","Langwaffen"],"not_rendered":{"external_links":2,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Kurzwaffen","index":0,"n_rows":53,"n_cols":22,"rows_kept":53,"flags":["formulas_cached_only"]}
["Hersteller","Modell","Kaliber","Lauf","Schusszahl","Antrieb","Abzug","Spannsystem","Laden","Lauflänge","Gewicht","Lauf","Laufmantel","Oberteil/System","Griffstück","Griffschalen","Sicherung","Visierung","Bemerkung 1","Bemerkung 2","Vorbild","Zustand/Schäden"]
["Baikal",null,"4,5/.177","gezogen","1","Federdruck",null,"Knicklauf","Kipplauf-Hinterlader","22",null,"Stahl",null,"Stahl","Kunststoff rot",null,"Rastsicherung gegen Aufschnappen beim Spannen","offen,einstellbar",{"$nulls":3},"gebraucht gur"]
["BSA","Scorpion","4,5/.177","gezogen",1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader","20",null,"Stahl",null,"Stahl","Kunststoff schwarz",null,"Abzug, Drehflügel","offen,einstellbar",{"$nulls":3},"gebraucht"]
["Crosman","137","4,5/.177","gezogen","1","CO2","SA","Zugknopf","Kammerlader","21,5",null,"Stahl",null,"Stahl","Druckguss","Kunststoff schwarz","Abzug, Schubstift","offen, seitlich einstellbar","Spannschieber",null,null,"gebraucht"]
["Crosman","150","5,5/.22","gezogen","1","CO2","SA","Zugknopf","Kammerlader","15",null,"Stahl",null,"Stahl","Druckguss","Kunststoff braun","Abzug, Schubstift","offen, seitlich einstellbar","Spannschieber",null,null,"stark gebraucht"]
["Copperhead/Crosman","Black Venom","4,5/.177","gezogen","1/17","Federdruck",null,"Zugspanner","Kipplauf-Hinterlader/Magazin","12",null,"Stahl","Kunststoff","Kunststoff","Kunststoff schwarz",null,"Abzug, Schubstift","offen, fest",{"$nulls":3},"neu"]
["Crosman","357","4,5/.177","gezogen","6/10","CO2","SA/DA","Revolver","Wechseltrommel","20",null,"Stahl","Druckguss","Druckguss","Druckguss","Kunststoff braun","Hahn, Schubstift","offen, einstellbar",null,null,"Colt Python","stark gebraucht"]
["Crosman","357BB","4,5/.177 BB","glatt","6","CO2","SA/DA","Revolver","Wechseltrommel","15",null,"Stahl","Kunststoff","Druckguss","Druckguss","Kunststoff braun","Hahn, Schubstift","offen, einstellbar",null,null,"Colt Python","neu"]
["Crosman","1200","4,5/.177 BB","glatt",">20","CO2","SA","Spannschieber","Kugelreservoir",null,null,"Stahl","Druckguss","Druckguss","Druckguss","Kunststoff braun",null,"offen, einstellbar","Spannschieber unter dem Lauf",null,null,"neuwertig"]
["Crosman","38C","4,5/.177","gezogen","6","CO2","SA/DA","Revolver","Trommel","10",null,"Stahl","Druckguss","Druckguss","Druckguss","Kunststoff braun","keine","offen, einstellbar",{"$nulls":3},"gebraucht"]
["Crosman","1377","4,5/.177","gezogen","1","vorkomprimiert","SA","Spannschieber mit Verschluss kombiniert","Kammerlader","26",null,"Stahl",null,null,"Druckguss","Kunststoff","Abzug, Schubstift","offen, einstellbar",{"$nulls":3},"neuwertig"]
["Crosman","Peacemaker 44","4,5/.177","gezogen","6","CO2","SA","Revolver","Trommel","12",null,"Stahl","Druckguss","Druckguss","Druckguss","Kunststoff braun","keine","offen, fest",null,null,"Colt SAA","gebraucht"]
["Crosman","1861 Shiloh","4,5/.177","gezogen","6","CO2","SA","Revolver","Trommel","17",null,"Stahl","Druckguss","Druckguss","Druckguss","Kunststoff braun","Abzug, Schubstift","offen, fest",null,null,"Remington Army","gebraucht"]
["Daisy","717","4,5/.177","gezogen","1","vorkomprimiert",null,"Spannschieber mit Verschluss kombiniert","Kammerlader",null,null,"Stahl",null,"Messing","Druckguss","Kunststoff braun","Abzug, Schubstift","offen, einstellbar",{"$nulls":3},"gebraucht"]
["Daisy","44 Magnum","4,5/.177","gezogen","6","CO2","SA/DA","Revolver","Wechseltrommel","20",null,"Stahl","Druckguss","Druckguss","Druckguss","Kunststoff braun","Hahn, Schubstift","offen, einstellbar",{"$nulls":3},"gebraucht gur"]
["Daisy","44 Magnum","4,5/.177","gezogen","6","CO2","SA/DA","Revolver","Wechseltrommel","20",null,"Stahl","Druckguss","Druckguss","Druckguss","Kunststoff schwarz","Hahn, Schubstift","offen, einstellbar","glanzchrom",null,null,"gebraucht gur"]
["Daisy","44 Magnum","4,5/.177","gezogen","6","CO2","SA/DA","Revolver","Wechseltrommel","10",null,"Stahl","Druckguss","Druckguss","Druckguss","Kunststoff braun","Hahn, Schubstift","offen, einstellbar",{"$nulls":3},"gebraucht gur"]
["Daisy","PowerLine 92","4,5/.177","gezogen","12","CO2","SA/DA","SA/DA","Magazin","~12",null,"Stahl","Kunststoff","Kunststoff schwarz","Kunststoff schwarz","Kunststoff schwarz","Hahn, Drehflügel","offen, einstellbar",null,null,"Beretta 92","gebraucht sehr gut"]
["Daisy","PowerLine 93","4,5/.177 BB","glatt","15","CO2","DAO","DAO","Magazin",null,null,"Stahl",null,"Kunststoff schwarz","Kunststoff schwarz","Kunststoff braun","keine","offen, einstellbar",{"$nulls":3},"gebraucht, fehlende Kleinteile"]
["Daisy","PowerLine 200","4,5/.177 BB","glatt",">20Reservoir/6Magazin","CO2",null,"halbautomatisch","Kugelreservoir","18",null,"Stahl","Druckguss","Druckguss","Druckguss","Kunststoff braun","Abzug, Schubstift","offen, einstellbar",{"$nulls":3},"neuwertig"]
["Diana",2,"4,5/.177","glatt",1,"Federdruck",null,"Einschublauf","Laufschraube","18",null,"Stahl","Stahl","Stahl","Holz",null,"keine","offen, fest",{"$nulls":3},"gebraucht gut"]
["Diana",5,"4,5/.177","gezogen",1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader","18",null,"Stahl",null,"Stahl","Kunststoff grau",null,"keine","offen, einstellbar","Abzug einstellbar",null,null,"gebraucht"]
["Condor/Drulov","DU-10","4,5/.177","gezogen","5","CO2","SA","Spannschieber/halbautomatisch","Magazin","~15",null,"Stahl","Druckguss","Stahl","Stahl","Holz","Schlagstück, Schubknopf","offen, einstellbar",{"$nulls":3},"gebraucht sehr gut"]
["Em-Ge","LP3","4,5/.177","gezogen","1","Federdruck",null,"Knicklauf","Kipplauf-Hinterlader","15",null,"Stahl","Druckguss","Druckguss","Druckguss","Kunststoff braun","keine","offen, einstellbar",{"$nulls":3},"stark gebraucht"]
["Falke","33","4,5/.177","gezogen","1","Federdruck",null,"Hebelspanner","Kipplauf-Hinterlader","13",null,"Stahl",null,"Stahl","Holz",null,"keine",null,"Lauf kippt beim Spannen automaitsch",null,null,"gebraucht gut"]
["FEG","GPM-D2","4,5/.177","gezogen","1","CO2","SA","Hebelspanner","Kammerlader","26,5",null,"Stahl",null,"Aluguss","Holz",null,"keine","offen, einstellbar","wahlweise 2 8g-Kapseln oder 33g-Füllung im Tank",null,null,"gebraucht gut"]
["Gamo","AF10","4,5/.177 BB","glatt","20","vorkomprimiert",null,"Laufspanner","Unterlaufmagazin",null,null,"Stahl",null,"Kunststoff schwarz/Stahl","Kunststoff schwarz",null,"Abzug, Schubstift","offen, einstellbar",{"$nulls":3},"gebraucht gut"]
["Hämmerli","CO2 Single","4,5/.177","gezogen","1","CO2","SA","Spannschieber","Ladeschieber","11",null,"Stahl",null,"Stahl","Druckguss","Kunststoff braun","keine","offen, einstellbar",{"$nulls":3},"gebraucht gut"]
["Harrington&Son","The Gat","4,5/.177","glatt","1","Federdruck",null,"Einschublauf","Laufschraube","18",null,"Stahl","Kunststoff","Druckguss","Druckguss",null,"Abzug, Drehflügel","offen, fest",{"$nulls":3},"neuwertig"]
["Healthways/Perfecta","Plainsmaster","4,45/.175","glatt",">20","CO2","DAO","DAO","Kugelreservoir","~22",null,"Stahl","Druckguss","Druckguss","Druckguss","Kunststoff braun","Abzug, Schieber","offen, fest",{"$nulls":3},"neuwertig"]
["Heym",null,"4,5/.177","glatt",1,"Federdruck",null,"Einschublauf","Laufschraube","15",null,"Stahl","Stahl","Druckguss","Druckguss","Kunststoff schwarz","keine","offen, fest",{"$nulls":3},"stark gebraucht, Griffschale gebrochen"]
["Heym?",null,"4,5/.177","glatt","1","Federdruck",null,"Zugspanner","Einschraublauf","10,5",null,"Messing",null,"Stahl","Holz",null,"keine","offen, fest",{"$nulls":3},"stark gebraucht"]
["HyScore",null,"4,5/.177","gezogen","1","Federdruck",null,"Laufspanner","Drehverschluss-Hinterlader","19",null,"Stahl",null,"Stahl","Kunststoff schwarz",null,"keine","offen, einstellbar","Lauf geht durch Kolbenraum","Schalldämpfergewinde, Wechselläufe verschiedener Kaliber möglich",null,"gebraucht sehr gut"]
["HS","9","4,5/.177","glatt",1,"Federdruck",null,"Einschublauf","Laufschraube","15",null,"Stahl","Stahl","Stahl","Bakelit",null,"keine","offen, fest",{"$nulls":3},"stark gebraucht, Griffstück geklebt"]
["HS","9a","4,5/.177","glatt",1,"Federdruck",null,"Einschublauf","Laufschraube","15",null,"Stahl","Stahl","Bakelit","Bakelit",null,"keine","offen, fest",{"$nulls":3},"gebraucht sehr gut"]
["HS","71","4,5/.177","gezogen",">20","Federdruck",null,"Seitenspanner","Kugelreservoir","~11",null,"Stahl",null,"Druckguss","Kunststoff braun",null,"keine","offen, einstellbar",{"$nulls":3},"gebraucht"]
["Lucznik/AKAH",null,"4,5/.177","gezogen","1","Federdruck",null,"Knicklauf","Kipplauf-Hinterlader","23,5",null,"Stahl",null,"Druckguss","Stahl","Kunststoff schwarz","keine","offen, einstellbar",null,null,"Kopie der Walther LP53","gebraucht"]
["Marksman","Repeater","4,5/.177","glatt","1/~10","Federdruck",null,"Zugspanner","Kipplauf-Hinterlader/Magazin","6",null,"Messing","Druckguss","Druckguss","Druckguss",null,"Abzug, Schubstift","offen, fest",{"$nulls":3},"stark gebraucht"]
["Mondial","Oklahoma","4,5/.177","glatt","1","Federdruck",null,"Knicklauf","Kipplauf-Hinterlader","16",null,"Messing","Druckguss","Druckguss","Druckguss","Kunststoff braun","keine","offen, fest","Arretierhebel für den Lauf",null,null,"stark gebraucht"]
["Mondial","Zip","4,5/.177","gezogen","1","Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Stahl","Druckguss","Druckguss","Druckguss","Kunststoff braun","keine","offen",{"$nulls":3},"stark gebraucht"]
["Rekord","Champion","4,5/.177","gezogen","12","Federdruck",null,"Seitenspanner","Magazin","19",null,"Stahl",null,"Druckguss","Druckguss","Kunststoff braun","Abzug, Schieber","offen, einstellbar","Lauf geht durch Kolbenraum",null,null,"gebraucht gur"]
["Rekord","Jumbo","4,5/.177","gezogen",1,"Federdruck",null,"Hebelspanner","Hinterlader","15",null,"Stahl",null,"Druckguss","Druckguss","Holz","Abzug, Drehflügel","offen, fest","Lauf geht durch Kolbenraum",null,null,"stark gebraucht"]
["Rekord","Mod. 2","4,5/.177","gezogen","1","Federdruck",null,"Knicklauf","Kipplauf-Hinterlader","13",null,"Stahl","Druckguss","Druckguss","Druckguss","Kunststoff weiss","keine","offen, einstellbar",{"$nulls":3},"stark gebraucht"]
["Relum",null,"5,5/.22","gezogen","1","Federdruck",null,"Unterlaufspanner","Ladeklappe","19",null,"Stahl",null,"Stahl","Holz",null,"keine","offen, einstellbar","einsteckbarer Anschlagbügel aus Stahldraht",null,null,"gebraucht gut, Holzgriff angerissen"]
["RWS","C225","4,5/.177","gezogen","8","CO2","SA/DA","Revolver","Trommelmagazin","15",null,"Stahl","Druckguss","Druckguss","Druckguss","Kunststoff schwarz","Hahnrast/Entspannhebel","offen, einstellbar",null,null,"SigSauer 225","in Gebrauch"]
["Sheridan","E9A EB20","5,0/.20","gezogen","1","CO2","SA","Spannschieber mit Verschluss kombiniert","Kammerlader","16",null,"Messing",null,"Messing","Druckguss","Holz","Abzug, Schubstift","offen, einstellbar",{"$nulls":3},"gebraucht gut"]
["Slavia","APP661","4,5/.177 BB","glatt","7","CO2","SA","Spannhebel/halbautomatisch","Stangenmagazin","11",null,"Stahl",null,"Druckguss","Druckguss","Kunststoff schwarz","Schlagstück, Drehflügel","offen, einstellbar",{"$nulls":3},"gebraucht"]
["Smith&Wesson","79G","4,5/.177","gezogen","1","CO2","SA","Spannschieber","Kammerlader","20",null,"Stahl","Druckguss","Druckguss","Druckguss","Kunststoff braun","Abzug, Schubstift","offen, einstellbar","Abzug einstellbar",null,null,"gebraucht"]
["UMA","SP50","4,5/.177","glatt",1,"Federdruck",null,"Einschublauf","Laufschraube","17",null,"Messing","Kunststoff","Druckguss","Druckguss",null,"keine","offen, fest",{"$nulls":3},"stark gebraucht"]
["Webley","Junior","4,5/.177","glatt","1","Federdruck",null,"Laufspanner","Kipplauf-Hinterlader","15",null,"Stahl",null,"Stahl","Stahl","Kunststoff schwarz","keine","offen, einstellbar","Lauf oberhalb des Druckzylinders",null,null,"gebraucht"]
["Webley","Mark I","4,5/.177","gezogen",1,"Federdruck",null,"Laufspanner","Kipplauf-Hinterlader","18",null,"Stahl",null,"Stahl","Stahl","Holz","Abzug, Drehknopf","offen, einstellbar","Lauf oberhalb des Druckzylinders",null,null,"stark gebraucht"]
["Weihrauch","HW45","5,5/.22","gezogen",1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader","20",null,"Stahl",null,"Druckguss","Druckguss","Holz","Abzug, Drehflügel","offen, einstellbar",{"$nulls":3},"gebraucht"]
["Weihrauch","HW70","4,5/.177","gezogen",1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader","16",null,"Stahl","Druckguss","Druckguss","Kunststoff braun",null,"keine","offen, einstellbar",{"$nulls":3},"gebraucht gut"]

{"sheet":"Langwaffen","index":1,"n_rows":40,"n_cols":21,"rows_kept":40,"flags":["formulas_cached_only"]}
["Hersteller","Modell","Kaliber","Lauf","Schusszahl","Antrieb","Abzug","Spannsystem","Laden","Lauflänge","Gewicht","Lauf","Laufmantel","System","Schaft","Sicherung","Visierung","Bemerkung 1","Bemerkung 2","Vorbild","Zustand/Schäden"]
["?",null,"6,35/.25","glatt",1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Stahl",null,"Stahl","Holz",null,"offen, fest","System Quackenbush",null,null,"sehr stark gebraucht"]
["Anschütz","250","4,5/.177","gezogen","1","Federdruck",null,"Seitenspanner","Ladeschacht",null,null,"Stahl",null,"Stahl","Holz",null,"Diopter","Doppelkolbensystem, pneumatisch gedämpft",null,null,"gebraucht gut"]
["Armigas Comega",null,"4,4 BRK","gezogen","~60","CO2","SA","Spannschieber/halbautomatisch","Magazin",null,null,"Stahl",null,"Stahl","Holz",null,"offen, einstellbar",{"$nulls":3},"stark gebraucht"]
["Crosman",262,"4,5/.177","gezogen",1,"CO2","SA","Zugknopf","Schwenkkammer",null,null,"Stahl","Stahl","Stahl/Druckguss","Holz","Abzug, Schubstift","offen, einstellbar",{"$nulls":3},"gebraucht"]
["Crosman","400","5,5/.22","gezogen","12","CO2","SA","Zugknopf","Kammerlader",null,null,"Stahl",null,"Stahl","Holz",null,"offen, einstellbar",{"$nulls":3},"gebraucht gut"]
["Crosman","622 PellClip Repeater","5,5/.177","gezogen",6,"CO2","SA","Vorderschaftrepetierer","Trommelmagazin",null,null,"Stahl",null,"Druckguss","Holz",null,"offen, einstellbar","seitliches Einsteck-Trommelmagazin",null,"Vorderschaftrepetierflinte","stark gebraucht"]
["Crosman",1077,"4,5/.177","gezogen",12,"CO2","DAO","Revolver","Trommelmagazin",null,null,"Stahl","Stahlblech","Kunststoff","Holz",null,"RedDot","Kastenförmiger Trommelträger",null,"Ruger 1022","gebraucht gut"]
["Diana/MGR","Diana-Luft-Gewehr","4,5/.177",null,1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Stahl",null,"Stahl","Holz",null,"offen, fest",{"$nulls":3},"stark gebraucht, narbig, Schaft gerissen"]
["Diana/MGR",1,"4,5/.177","glatt",1,"Federdruck",null,"Knicksystem","Einstecklauf",null,null,"Messing","Stahlblech","Stahlblech","Holz",null,"offen, fest","Lauf wird zum Laden vorne aus dem Laufrohr gezogen",null,null,"sehr stark gebraucht"]
["Diana",15,"4,5/.177","glatt",1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Stahl","Stahlblech","Stahlblech","Holz",null,"offen, Höhe einstellbar","Gesamte Waffe aus Stahlblech gefertigt",null,null,"gebraucht gut"]
["Diana",16,"4,5/.177","glatt",1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Stahl","Stahlblech","Stahlblech","Holz",null,"offen, Höhe einstellbar","Gesamte Waffe aus Stahlblech gefertigt",null,null,"stark gebraucht, Brünierung fehlt"]
["Diana",20,"4,5/.177","glatt",1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Messing","Stahlblech","Stahlblech","Holz",null,"offen, Höhe einstellbar","Gesamte Waffe aus Stahlblech gefertigt",null,null,"sehr stark gebraucht, wird überarbeitet"]
["Diana","22","4,5/.177","gezogen",1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Stahl",null,"Stahl","Holz",null,"offen, einstellbar",{"$nulls":3},"gebraucht, Schaft zerkratzt"]
["Diana","23","4,5/.177","gezogen",1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Stahl",null,"Stahl","Holz",null,"offen, einstellbar",{"$nulls":3},"gebraucht gut, Schaft überarbeitet"]
["Diana",25,"4,5/.177","gezogen",1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Stahl",null,"Stahl","Holz",null,"offen, einstellbar",{"$nulls":3},"gebraucht gut"]
["Diana",35,"4,5/.177","gezogen",1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Stahl",null,"Stahl","Holz",null,"offen, einstellbar",{"$nulls":3},"gebraucht, Schaft überarbeitet"]
["Diana","3?","4,5/.177","glatt",1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Stahl",null,"Stahl","Holz",null,"offen, fest","System Quackenbush",null,null,"sehr stark gebraucht, Schaft nachgefertigt"]
["Diana","60","4,5/.177","gezogen","1","Federdruck",null,"Seitenspanner","Ladeschacht",null,null,"Stahl","Stahl","Stahl","Holz",null,null,"Doppelkolbensystem zahnstangengekoppelt",null,null,"gebraucht"]
["Diana","75","4.5/.177","gezogen","1","Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Stahl","Kunststoff","Stahl",{"$nulls":3},"Doppelkolbensystem zahnstangengekoppelt",null,null,"gebraucht gut, Schaft fehlt"]
["Erma","ELG10","4,5/.177","gezogen","1","Federdruck",null,"LeverAction","Ladeschacht",null,null,"Stahl",null,"Stahl","Holz",null,null,"Einzellader im UHR-Style",null,"Winchester UHR","gebraucht, innerer Systemträger nach Bruch instandgesetzt"]
["Falke","70","4,5/.177","gezogen","1","Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Stahl",null,"Stahl","Holz",null,"offen, einstellbar",{"$nulls":3},"stark gebraucht"]
["Falke","80","4,5/.177","gezogen","1","Federdruck",null,"Unterlaufspanner","Ladewalze",null,null,"Stahl",null,"Stahl","Holz",null,"offen, einstellbar/ZF",{"$nulls":3},"gebraucht, leicht überarbeitet"]
["Feinwerbau",150,"4,5/.177","gezogen","1","Federdruck",null,"Seitenspanner","Ladeschacht",null,null,"Stahl",null,"Stahl","Holz",null,"Zielfernrohr","Prellschlagdämpfung durch Systemrücklauf",null,null,"stark gebraucht"]
["Feinwerbau","300","4,5/.177","gezogen","1","Federdruck",null,"Seitenspanner","Ladeschacht",null,null,"Stahl",null,"Stahl","Holz",null,"Diopter","Prellschlagdämpfung durch Systemrücklauf",null,null,"stark gebraucht"]
["FVM","Universal","5,5/.22","glatt","1","Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Aluminium","Stahlblech","Stahlblech","Holz",null,"offen, fest",{"$nulls":3},"gebraucht"]
["Haenel",310,"4,4 BRK","gezogen","6/8/12","Federdruck",null,"karabinerähnlicher Spannhebel","Magazin",null,null,"Stahl",null,"Stahl","Holz",null,"offen, einstellbar","Stoßrohr-Verdichter",null,null,"gebraucht sehr gut"]
["Haenel/Favorit?",null,"4,5/.177","gezogen",1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Stahl",null,"Stahl","Holz",null,null,"Laufverriegelung per Schwenkhebel",null,null,"stark gebraucht"]
["Hämmerli","Match","4,5/.177","gezogen","1","CO2","SA","zweiter Abzug","Ladeschieber",null,null,"Stahl","Stahl","Stahl","Holz",null,"Diopter",{"$nulls":3},"gebraucht "]
["Hämmerli",null,"4,4 BRK","gezogen","~60","CO2","SA","zweiter Abzug","Magazin",null,null,"Stahl",null,"Stahl","Holz",null,"offen, einstellbar",{"$nulls":3},"gebraucht"]
["Lion Brand/Umarex",null,"4,5/.177","gezogen","1","Federdruck",null,"Seitenspanner","Ladeschacht",null,null,"Stahl",null,"Stahl","Holz",{"$nulls":5},"gebraucht"]
["Mars",null,"4,5/.177","gezogen",1,"Federdruck",null,"Seitenspanner","Ladewalze",null,null,"Stahl",null,"Stahl","Holz",null,"Zielfernrohr",{"$nulls":3},"sehr stark gebraucht, Brünierung mit Fehlstellen"]
["Müller","Blitz","4,5/.177","gezogen","~12","Federdruck",null,"obenliegender Spannhebel","Kugelreservoir",null,null,"Stahl",null,"Stahl",null,null,"offen, einstellbar","Stoßrohr-Verdichter",null,null,"z.Zt. Zerlegt"]
["Neckermann","71/J","4,5/.177","gezogen","1","Federdruck",null,"Seitenspanner","Ladeschacht",null,null,"Stahl",null,"Stahl","Holz","Schieber","offen, einstellbar",{"$nulls":3},"stark gebraucht"]
["Neckermann","71/S","4,5/.177","gezogen","1","Federdruck",null,"Unterlaufspanner","Ladewalze",null,null,"Stahl",null,"Stahl","Holz",null,"offen, einstellbar",{"$nulls":3},"gebraucht, Schaft schlechter Zustand"]
["Relum","Tornado","5,5/.22","gezogen",1,"Federdruck",null,"Unterlaufspanner","Ladewalze",null,null,"Stahl",null,"Stahl","Holz",null,"offen, einstellbar","Lauf starr, Ladewalze",null,null,"gebraucht sehr gut"]
["Umarex","Panther","4,5/.177","gezogen",1,"Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Stahl",null,"Druckguss","Holz",null,"offen, einstellbar","basiert auf LuPi RO72",null,null,"gebraucht"]
["Weihrauch","HW35","4,5/.177","gezogen","1","Federdruck",null,"Knicklauf","Kipplauf-Hinterlader",null,null,"Stahl",null,"Stahl","Holz",{"$nulls":5},"Schrott "]
["Will?",null,"6,35/.25","glatt",1,"Federdruck",null,"Bügelspanner","Kipplauf-Hinterlader",null,null,"Stahl",null,"Stahl","Holz",null,"offen, einstellbar",{"$nulls":3},"sehr stark gebraucht"]
["Will?",null,"5,0/.20","gezogen",1,"Federdruck",null,"Bügelspanner","Kipplauf-Hinterlader",null,null,"Stahl",null,"Stahl","Holz",null,"offen, einstellbar",{"$nulls":3},"gebraucht  gut, Schaft überarbeitet"]