{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Info","Liste"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Info","index":0,"n_rows":23,"n_cols":3,"rows_kept":23,"flags":["formulas_cached_only"]}
["Farbkodierung: "]
[]
[]
[]
[null,null,"Erwerb in Arbeit"]
[]
[null,null,"noch aufzuarbeiten/zu reparieren"]
[]
[null,null,"nur teilweise vorhanden/nicht komplett"]
[]
[null,null,"kein Neukauf nötig"]
[]
[null,null,"Neukauf erforderlich, Belegstück, irreparabel"]
[]
[null,null,"Neukauf, falls billig und besser"]
[]
[null,null,"noch nicht vorhanden, aber dringend gesucht"]
[]
[null,null,"ausserhalb der Sammlung"]
[]
[null,null,"steht zum Verkauf"]
[]
[null,null,"keine Schreckschusswaffe (mehr)"]

{"sheet":"Liste","index":1,"n_rows":527,"n_cols":40,"rows_kept":527,"flags":["formulas_cached_only"]}
["PTB","Jahr","Typ","System","Hersteller","Modell","Herkunftsland","Kaliber","Schusszahl","Länge (mm)","Breite (mm)","Höhe (mm)","Lauflänge cm/Zoll","Gewicht","Ausschuss","Umbauschutz 1","Umbauschutz 2","Umbauschutz 3","Umbauschutz Trommel","Signal ?","Laufgewinde","Schloss","Bediensicherung","Fallsicherung","Laden","Entladen","Rahmen","Oberteil/Schlitten","Lauf","Trommel","Griff/Griffschalen","SN","Beschussamt","Jahr","Vorbild","Baugleichheiten","Bemerkung 1","Bemerkung 2","Zustand/Schäden","Verpackung"]
["5","69","Revolver",null,"Perfecta","S","Deutschland","6mm Flobert Platz","6","189","32","118","7,5/3",{"v":521,"d":"521 g"},"oben",{"$nulls":3},"Lager und Öffnung versetzt","n","n","SA/DA",null,"Hahnrückzug","Kipplauf","automatischer Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Nussbaum",{"$nulls":4},"alle Mayer/Perfecta Kipplaufrevolver",null,null,"gebraucht gut"]
["6","69","Revolver",null,"Perfecta","G","Deutschland","6mm Flobert Platz","6","189","32","118","7,5/3",{"v":549,"d":"549 g"},"vorn",{"$nulls":3},"Lager und Öffnung versetzt","j",null,"SA/DA",null,"Hahnrückzug","Kipplauf","automatischer Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",{"$nulls":4},"alle Mayer/Perfecta Kipplaufrevolver",null,null,"gebraucht gut"]
["7","69","Pistole","Repetierer","Perfecta/MaRie","S","Deutschland","6mm Flobert Platz","8",{"$nulls":4},{"v":244,"d":"244 g"},"oben","kein Lauf vorhanden","Lager und Lauf nicht parallel",null,null,"n","n","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Röhrenmagazin","automatisch nach oben","Druckguss verchromt","Druckguss verchromt",null,null,"Kunststoff weiss",{"$nulls":5},"Auswurf nach oben",null,"gebraucht"]
["7","69","Pistole","Repetierer","Perfecta/MaRie","S","Deutschland","6mm Flobert Platz","8",{"$nulls":4},{"v":243,"d":"243 g"},"oben","kein Lauf vorhanden","Lager und Lauf nicht parallel",null,null,"n","n","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Röhrenmagazin","automatisch nach oben","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":5},"Auswurf nach oben",null,"neuwertig","Pappschachtel"]
["8","69","Pistole","Repetierer","Perfecta/MaRie","G","Deutschland","6mm Flobert Platz","8",{"$nulls":4},{"v":259,"d":"259 g"},"vorn",null,"Lager und Lauf nicht parallel",null,null,"Zusatzlauf",null,"DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Röhrenmagazin","automatisch nach oben","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":5},"Auswurf nach oben",null,"gebraucht"]
["8","69","Pistole","Repetierer","Perfecta/MaRie","G","Deutschland","6mm Flobert Platz","8",{"$nulls":4},{"v":259,"d":"259 g"},"vorn",null,"Lager und Lauf nicht parallel",null,null,"Zusatzlauf",null,"DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Röhrenmagazin","automatisch nach oben","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":5},"Auswurf nach oben",null,"neuwertig"]
["8","69","Pistole","Repetierer","Perfecta/MaRie","G","Deutschland","6mm Flobert Platz","8",{"$nulls":4},{"v":264,"d":"264 g"},"vorn",null,"Lager und Lauf nicht parallel",null,null,"Zusatzlauf"," ","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Röhrenmagazin","automatisch nach oben","Druckguss verchromt","Druckguss verchromt",null,null,"Kunststoff weiss","1073",{"$nulls":4},"Auswurf nach oben",null,"neu"]
["8","69","Pistole","Repetierer","Perfecta/MaRie","G","Deutschland","6mm Flobert Platz","8",{"$nulls":4},{"v":262,"d":"262 g"},"vorn",null,"Lager und Lauf nicht parallel",null,null,"Zusatzlauf"," ","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Röhrenmagazin","automatisch nach oben","Druckguss vergoldet","Druck vergoldet",null,null,"Kunststoff weiss","973",{"$nulls":4},"Auswurf nach oben",null,"gebraucht gut","Pappschachtel"]
["9","69","Pistole","Repetierer","Walther","UP1","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":157,"d":"157 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf",null,"DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Alu-Druckguss brüniert","Alu-Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":7},"gebraucht gut"]
["9","69","Pistole","Repetierer","Walther","UP1","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":240,"d":"240 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf",null,"DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Alu-Druckguss verchromt","Druckguss verchromt",null,null,"Kunststoff weiss",{"$nulls":7},"gebraucht gut"]
["24","69","Revolver",null,"Em-Ge","22ST","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":388,"d":"388 g"},"oben","Lauf verschlossen",null,null,"vorderer Teil fest, hinterer Teil nur patronenlang","n","n","SA/DA",null,"Hahnrückzug","Ladeklappe","manueller Ausstosser","Druckguss verchromt",null,"Druckguss verchromt","Druckguss/Stahl verchromt","Kunststoff weiss",{"$nulls":7},"stark gebraucht, Verchromung abgegriffen"]
["25","69","Pistole","Repetierer","Em-Ge","6","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":249,"d":"249 g"},"oben",null,"Lager rechtwinklig zum Lauf",null,null,"n","n","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":7},"neu"]
["26","69","Pistole","Repetierer","Em-Ge","60","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"6/2,25",{"v":274,"d":"274 g"},"oben",null,"Lager rechtwinklig zum Lauf",null,null,"n","n","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":6},"1975 von Intersport an die BW geliefert","neu"]
["26","69","Pistole","Repetierer","Em-Ge","60","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"6/2,25",{"v":279,"d":"279 g"},"oben",null,"Lager rechtwinklig zum Lauf",null,null,"n","n","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff braun",{"$nulls":7},"gebraucht, Brünierung abgegriffen"]
["28","69","Pistole","Repetierer","Em-Ge","6d","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"6/2,25",{"v":269,"d":"269 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff braun",{"$nulls":7},"gebraucht gut"]
["29","69","Revolver",null,"Röhm","RG77","Deutschland",".22Knall","6",{"$nulls":4},{"v":345,"d":"345 g"},"vorn","Stahlbolzen",null,null,"keiner",null,null,"SA/DA",null,null,"Ladeklappe","manuell per Stift","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Kunststoff schwarz",{"$nulls":7},"gebraucht"]
["30","69","Revolver",null,"Röhm","RG6 ","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":337,"d":"337 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Umlaufende Nut","Zusatzlauf","M8*1,5","SA/DA",null,"Hahnrückzug","Ladeklappe","manuell per Stift","Druckguss verchromt",null,"Druckguss verchromt","Stahl brüniert","Kunststoff weiss",{"$nulls":5},"neues Modell",null,"neu","Pappschachtel"]
["31","69","Pistole","Repetierer","Röhm","RG2s","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":263,"d":"263 g"},"oben",null,"Lager rechtwinklig zum Lauf",null,null,"n","n","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":7},"neuwertig"]
["31","69","Pistole","Repetierer","Röhm","RG2s","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":277,"d":"277 g"},"oben",null,"Lager rechtwinklig zum Lauf",null,null,"n","n","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss verchromt","Druckguss verchromt",null,null,"Kunststoff weiss",{"$nulls":7},"neu"]
["32","69","Pistole","Repetierer","Röhm","RG3s","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":294,"d":"294 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":7},"gebraucht"]
["32","69","Pistole","Repetierer","Röhm","RG3s","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":296,"d":"296 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss verchromt","Druckguss verchromt",null,null,"Kunststoff weiss",{"$nulls":7},"neuwertig"]
["32","69","Pistole","Repetierer","Röhm","RG3s","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":297,"d":"297 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert, graviert",null,null,"Kunststoff schwarz",{"$nulls":7},"gebraucht"]
["33","69","Pistole","Repetierer","Röhm","RG5s","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":302,"d":"302 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":7},"neu"]
["33","69","Pistole","Repetierer","Röhm","RG5","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":302,"d":"302 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss verchromt","Druckguss verchromt",null,null,"Kunststoff weiss",{"$nulls":5},"PTB-Stempel sehr schwach, auf rechter Seite",null,"neuwertig"]
["34","69","Revolver",null,"Uniwerk","Volcanic 22 / V22  Type \"G\"","Italien","6mm Flobert Platz","6",{"$nulls":4},{"v":210,"d":"210 g"},"Vorn aus der Trommelattrappe","Lauf nicht durchbohrt",null,null,"Trommelattrappe steht fest, hinterer Teil nur patronenlang","n","n","DAO","keine","keine","Kipplauf","manuell per Hahnsporn","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff weiss",{"$nulls":7},"gebraucht"]
["36","69","Revolver",null,"ME","37","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"5/2",{"v":463,"d":"463 g"},"vorn","eingegossener Schlitz ",{"$nulls":3},"Zusatzlauf","M10","SA/DA","keine","Hahnrückzug","Schwenktrommel","manuell per Stift","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff schwarz",{"$nulls":5},"Trommelachsenstift dient als Ausstosser",null,"gebraucht gut"]
["37","69","Revolver",null,"ME","33","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"6/2,25",{"v":314,"d":"314 g"},"vorn","exzentrische Bohrung",null,null,"verjüngte Bohrung","Zusatzlauf","M8","SA/DA","keine","keine","Ladeklappe","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff schwarz",{"$nulls":5},"Trommelachsenstift dient als Ausstosser",null,"gebraucht gut"]
["38","69","Pistole","Automatik","Reck","P10 Startpistole","Deutschland","8mm Knall",{"$nulls":5},{"v":367,"d":"367 g"},"oben","Lauf nicht durchbohrt",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz","234969","München","71","früher auch als 6.35er Browning erhältlich, Reck P8",{"$nulls":3},"neu"]
["44","69","Pistole","Automatik","SM","Mod. 110","Deutschland","8mm Knall","6","118","24","86",null,{"v":328,"d":"328 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss verchromt?","Druckguss brüniert",null,"Kunststoff schwarz"," ",null," ","früher auch als 6.35er Browning erhältlich",{"$nulls":3},"gebraucht"]
["44","69a","Pistole","Automatik","SM","Mod. 110","Deutschland","8mm Knall","6","118","24","86",null,{"v":333,"d":"333 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","119694",null,"72","früher auch als 6.35er Browning erhältlich",{"$nulls":3},"gebraucht"]
["44","69b","Pistole","Automatik","SM","Mod. 110","Deutschland","8mm Knall","6","118","24","86",null,{"v":328,"d":"328 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","198512",null,"73","früher auch als 6.35er Browning erhältlich",{"$nulls":3},"gebraucht"]
["45","69","Pistole","Automatik","SM","Mod. 110A","Deutschland","8mm Knall","6","118","24","86",null,{"v":330,"d":"330 g"},"oben","Lauf nicht durchbohrt",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss verchromt","Druckguss verchromt","Druckguss verchromt",null,"Kunststoff schwarz","11832","München","69","früher auch als 6.35er Browning erhältlich",{"$nulls":3},"stark gebraucht","Pappschachtel"]
["45","69","Pistole","Automatik","SM","Mod. 110A","Deutschland","8mm Knall","6","118","24","86",null,{"v":328,"d":"328 g"},"oben","Lauf nicht durchbohrt","  ",null,null,"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","60022",null,"70","früher auch als 6.35er Browning erhältlich",{"$nulls":3},"gebraucht"]
["45","69a","Pistole","Automatik","SM","Mod. 110A","Deutschland","8mm Knall","6","118","24","86",null,{"v":329,"d":"329 g"},"oben","Lauf nicht durchbohrt",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","132860",null,"72","früher auch als 6.35er Browning erhältlich",{"$nulls":3},"neu"]
["45","69b","Pistole","Automatik","SM","Mod. 110A","Deutschland","8mm Knall","6","118","24","86",null,{"v":331,"d":"331 g"},"oben","Lauf nicht durchbohrt",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","178262",null,"72","früher auch als 6.35er Browning erhältlich",{"$nulls":3},"neuwertig"]
["46","69","Revolver",null,"Röhm","RG9","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":407,"d":"407 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Umlaufende Nut","Zusatzlauf",null,"SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss verchromt",null,"Druckguss verchromt","Stahl brüniert","Kunststoff weiss",{"$nulls":7},"neu","Pappschachtel"]
["48","69","Pistole","Automatik","Reck","P6","Deutschland","8mm Knall",{"$nulls":5},{"v":370,"d":"370 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","337350","München","72","früher auch als 6.35er Browning erhältlich, Reck P8",{"$nulls":3},"gebraucht"]
["48","69a","Pistole","Automatik","Reck","P6","Deutschland","8mm Knall",{"$nulls":5},{"v":341,"d":"341 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","391222",null,"73","früher auch als 6.35er Browning erhältlich, Reck P8",{"$nulls":3},"gebraucht"]
["48","69a","Pistole","Automatik","Reck","P6","Deutschland","8mm Knall",{"$nulls":5},{"v":375,"d":"375 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","448670",null,"75","früher auch als 6.35er Browning erhältlich, Reck P8",null,"Schlagbolzensicherung beim Zerlegen",null,"gebraucht"]
["48","69a","Pistole","Automatik","Reck","P6","Deutschland","8mm Knall",{"$nulls":5},{"v":375,"d":"375 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss vernickelt","Druckguss vernickelt","Druckguss vernickelt",null,"Kunststoff weiss","366354","Mellrichstadt","72","früher auch als 6.35er Browning erhältlich, Reck P8",{"$nulls":3},"gebraucht"]
["49","69","Revolver",null,"Em-Ge","38ST","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":520,"d":"520 g"},"oben","Lauf verschlossen",null,null,"vorderer Teil fest, hinterer Teil nur patronenlang","n","n","SA/DA",null,"Hahnrückzug","Ladeklappe","manueller Ausstosser","Druckguss brüniert",null,"Druck brüniert","Druckguss/Stahl brüniert","Kunststoff schwarz","3420",{"$nulls":6},"gebraucht gut"]
["70","69","Revolver",null,"Em-Ge","32ST","Deutschland",".320Knall/7mm Knall","6",{"$nulls":4},{"v":522,"d":"522 g"},"oben","Lauf verschlossen",null,null,"vorderer Teil fest, hinterer Teil nur patronenlang","n","n","SA/DA",null,"Hahnrückzug","Ladeklappe","manueller Ausstosser","Druckguss brüniert",null,"Druck brüniert","Druckguss/Stahl brüniert","Kunststoff schwarz","5047",null,"72",{"$nulls":4},"neu"]
["85","69","Revolver",null,"Mayer","S","Deutschland",".22Knall","6","192","30","110","7,5/3",{"v":494,"d":"494 g"},"vorn","Lauf verschlossen",null,null,"Lager und Öffnung versetzt","n",null,"SA/DA",null,null,"Kipplauf","automatischer Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun","710108-69","Köln",null,null,"alle Mayer/Perfecta Kipplaufrevolver",null,null,"stark gebraucht"]
["88","69","Revolver",null,"Mayer","G","Deutschland",".320Knall/7mm Knall","6","193","30","109","7,5/3",{"v":507,"d":"507 g"},"vorn","exzentrische Bohrung",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M8","SA/DA",null,null,"Kipplauf","automatischer Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,"Köln","72",{"$nulls":4},"neuwertig"]
["89","69","Revolver",null,"Arminius","HW1G","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":810,"d":"810 g"},"vorn","gewendelte Stahlplatte",null,null,"exzentrische Bohrung, HM-Stift","n","n","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Kunststoff schwarzbraun","916536",null,"76",null,null,"Weder Laufgewinde noch 15mm-Becher","Targetgriff","neuwertig"]
["89","69","Revolver",null,"Arminius","HW1G","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":730,"d":"730 g"},"vorn","gewendelte Stahlplatte",null,null,"exzentrische Bohrung, HM-Stift","n","n","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss verchromt",null,"Druckguss verchromt","Stahl verchromt","Kunststoff weiss",{"$nulls":5},"Weder Laufgewinde noch 15mm-Becher",null,"gebraucht gut"]
["90","69","Pistole",null,"FB Rekord","Weinberg u. Signal Pistole","Deutschland","6mm Flobert Platz","1",{"$nulls":4},{"v":150,"d":"150 g"},"vorn",null,"Lager winklig zum Lauf",null,null,"Zusatzlauf",null,"SA","keine","Hahnrast","Einzellader","automatischer Auswurf","Druckguss brüniert",null,"Druckguss brüniert",null,"Kunststoff schwarz",{"$nulls":3},"keins",null,"Verschluss durch Hahn",null,"gebraucht, Korrosionsspuren"]
["92","69","Pistole",null,"HS","Mod. 2","Deutschland","6mm Flobert Platz","1",{"$nulls":4},{"v":179,"d":"179 g"},"oben","Lauf nicht durchbohrt","Lager winklig zum Lauf",null,null,"n","n","SA",null,"keine","Einzellader","automatischer Auswurf","Stahl brüniert",null,"Stahl brüniert",null,"Kunststoff schwarz",{"$nulls":7},"neu","Pappschachtel"]
["93","69","Revolver",null,"NHM","Mod. S","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":545,"d":"545 g"},"seitlich und oben","Lauf nicht durchbohrt",null,null,"Lager und Öffnung versetzt","n","n","SA/DA",null,null,"Kipplauf","automatischer Ausstosser","Stahl brüniert",null,"Stahl brüniert","Stahl brüniert","Kunststoff dunkelbraun",{"$nulls":5},"Vollstahl",null,"gebraucht"]
["95","69","Pistole",null,"FB Rekord","B","Deutschland","6mm Flobert Platz","2",{"$nulls":4},{"v":182,"d":"182 g"},"vorn",null,"Lager winklig zum Lauf",null,null,"j, integriert","n","SA, Hahn mit stufenförmiger Schlagfläche","keine","keine","Einzellader","automatischer Auswurf","Druckguss brüniert",null,"Druckguss brüniert",null,"Kunststoff schwarz",{"$nulls":3},"keins",null,"Verschluss durch Hahn",null,"neuwertig"]
["99","69","Pistole","Automatik","HS","5S","Deutschland","8mm Knall","6","116","22","90",null,{"v":339,"d":"339 g"},"oben","Lauf nicht durchbohrt",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","39688","Mellrichstadt","71",null,null,"schlanker Abzugsbügel",null,"stark gebraucht"]
["99","69a","Pistole","Automatik","HS","5S","Deutschland","8mm Knall","6","116","22","90",null,{"v":336,"d":"336 g"},"oben","Lauf nicht durchbohrt",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","108717",null,"75",null,null,"schlanker Abzugsbügel","PTB auch auf Lauf/Griffstück","gebraucht"]
["100","69","Pistole","Automatik","HS","5A\"G\"","Deutschland","8mm Knall","6","116","22","90",null,{"v":338,"d":"338 g"},"vorn","rechteckiger Querschnitt",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","35779","Mellrichstadt","71",null,"ME 8 Detective PTB100/2","schlanker Abzugsbügel","PTB auch auf Lauf/Griffstück","gebraucht sehr gut"]
["100","69","Pistole","Automatik","HS","5A\"G\"","Deutschland","8mm Knall","6","116","22","90",null,{"v":335,"d":"335 g"},"vorn","rechteckiger Querschnitt",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","47809","Mellrichstadt","72",null,"ME 8 Detective PTB100/2","schlanker Abzugsbügel","PTB auch auf Lauf/Griffstück","stark gebraucht"]
["5","70","Revolver",null,"ME","70","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"5/2",{"v":303,"d":"303 g"},"vorn","Lauf nur geschraubt, Bohrung im Rahmen nur halbrund",null,null,"verjüngte Bohrung","j,  integriert","M8","SA/DA","keine","keine","Ladeklappe","manuell per Stift","Druckguss brüniert",null,"Stahl brüniert","Druckguss brüniert","Kunststoff schwarz",{"$nulls":5},"Lauf nur geschraubt, Trommelachsenstift dient als Ausstosser",null,"neuwertig"]
["5","70/A","Revolver",null,"ME","70/G","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"5/2",{"v":319,"d":"319 g"},"vorn","Lauf nur geschraubt, Bohrung im Rahmen nur halbrund","Lauf zur Trommelbohrung versetzt",null,"verjüngte Bohrung","j,  integriert","M8","SA/DA","keine","Hahnrückzug","Ladeklappe","manuell per Stift","Druckguss brüniert",null,"Stahl brüniert","Druckguss brüniert","Kunststoff schwarz",{"$nulls":5},"Lauf und Laufhülse nur geschraubt, Trommelachsenstift dient als Ausstosser",null,"gebraucht"]
["5","70/B","Revolver",null,"ME","70/G","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"5/2",{"v":317,"d":"317 g"},"vorn","exzentrische Bohrung","Lauf zur Trommelbohrung versetzt",null,"verjüngte Bohrung","Zusatzlauf","M12","SA/DA","keine","Hahnrückzug","Ladeklappe","manuell per Stift","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff schwarz",{"$nulls":5},"Trommelachse dient als Ausstosser",null,"neuwertig"]
["6","70","Revolver",null,"ME","80","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":436,"d":"436 g"},"vorn","Lauf nur geschraubt, Bohrung im Rahmen nur halbrund","Lauf zur Trommelbohrung versetzt",null,"verjüngte Bohrung","j, integiert","M8","SA/DA","keine","Hahnrückzug","Ladeklappe","manuell per Stift","Druckguss brüniert",null,"Stahl brüniert","Druckguss brüniert","Kunststoff schwarz",{"$nulls":5},"Lauf nur geschraubt, Trommelachsenstift dient als Ausstosser",null,"gebraucht gut","Pappschachtel"]
["6","70B","Revolver",null,"ME","80/G","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":437,"d":"437 g"},"vorn",null,"Lauf zur Trommelbohrung versetzt",null,"verjüngte Bohrung","j, integiert","M8","SA/DA","keine","Hahnrückzug","Ladeklappe","manuell per Stift","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff schwarz",{"$nulls":7},"gebraucht gut"]
["7","70","Revolver",null,"Arminius","HW1S","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":726,"d":"726 g"},"seitlich und oben","Stahlplatte längs im Lauf","Ausschuss durch 3 schräge Bohrungen, Lauf vorne zu",null,"exzentrische Bohrung, HM-Stift","n","n","SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Stahl brüniert","Stahl brüniert","Kunststoff schwarzbraun","375678",null,"72",null,"PTB 89-69",null,null,"neuwertig","Pappschachtel"]
["7","70A","Revolver",null,"Arminius","HW1S","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":692,"d":"692 g"},"seitlich","Lauf nicht durchbohrt",null,null,"exzentrische Bohrung","n","n","SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Stahl brüniert","Stahl brüniert","Kunststoff braun","1170398","Mellrichstadt","89",null,"PTB 89-69",null,null,"neuwertig","Pappschachtel mit Styroporeinschub"]
["10","70","Revolver",null,"NHM","S","Deutschland","6mm Flobert Platz","8",{"$nulls":4},{"v":412,"d":"412 g"},"oben","Lauf nicht durchbohrt",null,null,"Lager und Öffnung versetzt","n","n","SA/DA","keine","keine","Kipplauf","automatischer Ausstosser","Stahl brüniert",null,"Stahl brüniert","Stahl brüniert","Kunststoff schwarzbraun",{"$nulls":5},"Vollstahl",null,"neuwertig","Pappschachtel"]
["15","70","Revolver",null,"HS","121","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"14/5,5",{"v":1326,"d":"1,326 g"},"seitlich",{"$nulls":4},"n","n","SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss brüniert",null,"Stahl brüniert","Stahl brüniert","Holz",{"$nulls":3},"Colt SAA",{"$nulls":3},"gebraucht"]
["16","70","Revolver",null,"HS","121 A2","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"14/5,5",{"v":1260,"d":"1,260 g"},"seitlich",{"$nulls":4},"n","n","SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss brüniert",null,"Stahl brüniert","Stahl brüniert","Holz",null,"München","72","Colt SAA",{"$nulls":3},"gebraucht"]
["22","70","Pistole","Repetierer","Em-Ge","61","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":248,"d":"248 g"},"oben","fast kein Lauf vorhanden",{"$nulls":3},"n","n","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":7},"gebraucht, Brünierung abgegriffen"]
["28","70","Revolver",null,"Röhm","Mod. 60","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":322,"d":"322 g"},"vorn",{"$nulls":4},"Zusatzlauf",null,"SA/DA",null,null,"Ladeklappe","manueller Ausstosser","Druckguss brüniert",null,null,"Stahl brüniert","Kunststoff braun",{"$nulls":7},"gebraucht gut"]
["30","70","Pistole","Repetierer","Röhm","RG4s","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"0,5/0,2",{"v":310,"d":"310 g"},"oben","fast kein Lauf vorhanden",{"$nulls":3},"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff braun",{"$nulls":5},"Zusatzlauf wird OBEN in Waffe geschraubt",null,"neu"]
["32","70","Derringer",null,"Neumann","SI","Deutschland","6mm Flobert Platz","1",{"$nulls":4},{"v":182,"d":"182 g"},"oben","Ausschuss oben, Stahlstück im Lauf eingegossen",{"$nulls":3},"Zusatzlauf","M6","SA",null,"Hahnrast","Kipplauf","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert",null,"Kunststoff braun",{"$nulls":7},"gebraucht"]
["33","70","Derringer",null,"Reck","D5","Deutschland","6mm Flobert Platz","1",{"$nulls":4},{"v":184,"d":"184 g"},"oben","Ausschuss oben, Stahlstück im Lauf eingegossen",{"$nulls":3},"Zusatzlauf","M6","SA",null,"Hahnrast","Kipplauf","manueller Ausstosser","Druckguss vergoldet",null,"Druckguss brüniert",null,"Kunststoff braun",{"$nulls":7},"gebraucht gut"]
["34","70","Revolver",null,"Weber/L.T.F.","Valor","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":226,"d":"226 g"},"vorn",{"$nulls":3},"Umlaufende Nut","Zusatzlauf",null,"SA/DA",null,null,"Ladeklappe","manuell per Stift","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff weiss",{"$nulls":7},"neu","Pappschachtel"]
["38","70","Revolver",null,"Mayer+Söhne","Mod \"S\"","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},"487 g","vorn und oben","verjüngte Bohrung",null,null,"Stahlkern","Zusatzlauf","M8","SA/DA",null,"Hahnrückzug","Kipplauf","automatischer Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun","710114-151","Köln","71",null,"Alle Mayer&Söhne Kipplaufrevolver",null,null,"stark gebraucht"]
["1","71","Pistole","Repetierer","Em-Ge","62","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"6/2,25",{"v":286,"d":"286 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"j,  integriert","M12","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":5},"Becher an Lauf angeformt",null,"gebraucht"]
["3","71","Revolver",null,"Mayer","TG","Deutschland",".380Knall/9mm Knall","5","156","32","100","5/2",{"v":463,"d":"463 g"},"vorn und oben","exzentrische Bohrung",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M8","SA/DA",null,"Hahnrückzug","Kipplauf","automatischer Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun","711022-42","Köln","71",{"$nulls":4},"gebraucht gut"]
["4","71","Revolver",null,"Röhm","RG 76","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":422,"d":"422 g"},"vorn",{"$nulls":4},"j, integriert",null,"SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",{"$nulls":7},"gebraucht"]
["4","71","Revolver",null,"Röhm","RG 76","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":423,"d":"423 g"},"vorn",{"$nulls":4},"j, integriert",null,"SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",{"$nulls":7},"gebraucht gut"]
["5","71","Revolver",null,"Röhm","79","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":592,"d":"592 g"},"vorne und oben","Stahlbolzen seitlich im Lauf",null,null,"Übergrosse Öffnung, nicht rund","j,  integriert",null,"SA/DA",null,null,"Schwenktrommel","manuell per Ausstosser","Druckguss ehem. brüniert",null,"Druckguss ehem. brüniert","Druckguss ehem. brüniert","Kunststoff braun",null,"Ulm","72",{"$nulls":4},"stark gebraucht, Brünierung 0%, doppelte Ausschussbohrung, Auswerfer dreht in Trommel"]
["15","71","Revolver",null,"Mayer+Söhne","TS","Deutschland",".380Knall/9mm Knall","5","156","32","100","5/2",{"v":457,"d":"457 g"},"oben",{"$nulls":3},"Stahlkern","n",null,"SA/DA",null,"Hahnrückzug","Kipplauf","automatischer Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,null,"72",{"$nulls":4},"gebraucht gut","Pappschachtel"]
["3","72","Derringer",null,"Weber/L.T.F.","Derringer MK3","Deutschland","6mm Flobert Platz","2",{"$nulls":4},{"v":365,"d":"365 g"},"vorn","vor dem Lager tiefe Nut im Laufblock",{"$nulls":3},"j,  integriert","n","SA mit wechselseitig kippenden Schlagstück","keine","Hahnrast","Kipplauf","manuell per Schieber","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert",null,"Kunststoff weiss",{"$nulls":7},"neu","Pappschachtel"]
["4","72A","Revolver",null,"Arminius","HW 2 R","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":711,"d":"711 g"},"vorn und seitlich","exzentrische Bohrung",null,null,"exzentrische Bohrung","Zusatzlauf","M10","SA/DA",null,"Hahnrückzug","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Kunststoff braun","441829",null,"73",null,"Arminius HW 10GR PTB218, HW1G",null,null,"gebraucht gut"]
["5","72","Revolver",null,"HS","Mod. 21 C","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"12,5/5",{"v":781,"d":"781 g"},"vorn","längs eingegossener Schlitz ",null,null,"Hartmetallkern","j, integriert","n","SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz","1256",null,null,"Colt SAA","PTB 16, 258",null,null,"gebraucht"]
["7","72","Revolver",null,"HS","121 B","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"19,5/7,5",{"v":1221,"d":"1,221 g"},"vorn",{"$nulls":6},"SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss verchromt",null,"Stahl verchromt","Stahl verchromt","Holz",null,"München","76","Colt SAA","PTB 242",null,null,"gebraucht"]
["8","72","Pistole","Repetierer","MaRie/Aetna","Typ GII","Deutschland","6mm Flobert Platz","8",{"$nulls":4},{"v":264,"d":"264 g"},"vorn",null,"Lager und Lauf nicht parallel",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Röhrenmagazin","automatisch nach oben","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":5},"Auswurf nach oben",null,"neu"]
["17","72","Derringer",null,"C.Clauberg","K8","Deutschland","6mm Flobert Platz","2",{"$nulls":4},{"v":362,"d":"362 g"},"vorn","exzentrische Bohrung",{"$nulls":3},"j, integriert","n","SA",null,"Hahnrast","Kipplauf","manuell per Schieber","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert",null,"Kunststoff weiss",{"$nulls":4},"PTB 296",null,null,"gebraucht"]
["20","72","Pistole","Repetierer","MaRie/Aetna","G","Deutschland","6mm Flobert Platz","8",{"$nulls":4},{"v":258,"d":"258 g"},"vorn",null,"Lager und Lauf nicht parallel",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Röhrenmagazin","automatisch nach oben","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",{"$nulls":5},"Auswurf nach oben",null,"gebraucht gut","Pappschachtel"]
["2",null,"Selbstschussgerät",null,"Auber",null,null,".380Knall/9mm Knall","1",{"$nulls":4},{"v":386,"d":"386 g"},"vorn",{"$nulls":4},"n",null,null,"Fangbügel",null,"Verschraubung",null,"Aluguss blank",null,"Stahl",{"$nulls":4},"84",{"$nulls":4},"neu"]
["6",null,"Pistole","Repetierer","Em-Ge","62","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"6/2,25",{"v":287,"d":"287 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"j,  integriert","M12","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":5},"Becher an Lauf angeformt, vermutlich nachgestempelter Altbestand der PTB 1-71",null,"gebraucht"]
["6",null,"Pistole","Repetierer","Em-Ge","63","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"6/2,25",{"v":343,"d":"343 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"j,  integriert","M12","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":5},"neues Modell, runder Lauf",null,"gebraucht"]
["6",null,"Pistole","Repetierer","Em-Ge","63","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"6/2,25",{"v":335,"d":"335 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"j,  integriert","M12","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff braun",{"$nulls":5},"neues Modell, eckiger Lauf",null,"gebraucht","Styroporschachtel"]
["6",null,"Pistole","Repetierer","Em-Ge","63","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"6/2,25",{"v":332,"d":"332 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"j,  integriert","M12","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss verchromt","Druckguss verchromt",null,null,"Kunststoff braun",{"$nulls":5},"neues Modell, eckiger Lauf, ALLE Teile verchromt",null,"gebraucht gut"]
["11",null,"Revolver",null,"Mayer+Söhne","TGS","Deutschland",".380Knall/9mm Knall","5","157 (183)","32","101 (126)","5/2","615 m.Becher","vorne und oben","versetzte Bohrung",null,null,"Stahlkern","Zusatzlauf","M8","SA/DA",null,"Hahnrückzug","Kipplauf","automatischer Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,"Köln","73",null,null,"zweiter Abschussbecher wird oben auf den Lauf geklemmt",null,"gebraucht gut"]
["12",null,"Pistole","Automatik","Perfecta/MaRie","G5","Deutschland","8mm Knall",null,"134","23 (25)","101",null,{"v":414,"d":"414 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M8fein","Schlagbolzenschloss","Abzug, Schubknopf","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss verchromt","Druckguss brüniert",null,"Kunststoff schwarz",null,"Köln","75",null,"PTB 386,387, 619, 421, 12",null,null,"gebraucht, Abzug nicht einwandfrrei"]
["12",null,"Pistole","Automatik","Reck","Protector Automatik","Deutschland","8mm Knall",null,"134","23 (25)","101",null,{"v":425,"d":"425 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M8fein","Schlagbolzenschloss","Abzug, Schubknopf","keine","Magazin","automatischer Auswurf","Druckguss verchromt","Druckguss verchromt","Druckguss verchromt",null,"Kunststoff schwarz",null,"Köln","79",null,"PTB 386,387, 619, 421, 12",null,null,"stark gebraucht"]
["15",null,"Revolver",null,"HS","Mod. 21 C","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"12,5/5",{"v":825,"d":"825 g"},"vorn","längs eingegossener Schlitz ",{"$nulls":3},"Zusatzlauf",null,"SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Holz",{"$nulls":3},"Colt SAA","PTB 16, 258",null,null,"stark gebraucht"]
["16",null,"Revolver",null,"HS","Mod. 21 D","Deutschland","8mm Knall","6",{"$nulls":3},"12,5/5",{"v":778,"d":"778 g"},"vorn","längs eingegossener Schlitz ",null,null,"Hartmetallkern","Zusatzlauf",null,"SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,"München","73","Colt SAA",null,"verschiesst Pistolenmunition",null,"gebraucht"]
["19",null,"Selbstschussgerät",null,"Nimrod",null,"Deutschland","Kal.16 Alarm","1",{"$nulls":3},"4/1,6",{"v":1187,"d":"1,187 g"},"vorn","keiner","keiner",null,null,"n","n","Schnapphahn","Bohrung für Querstift",null,"Ladeschieber","manuell","Stahlguss",null,"Stahlguss",{"$nulls":9},"neuwertig"]
["19",null,"Selbstschussgerät",null,"Nimrod",null,"Deutschland","Kal.16 Alarm","1",{"$nulls":4},{"v":252,"d":"252 g"},"vorn","keiner","keiner",null,null,"n","n","Schlagbolzen","keine",null,"Einschraublauf","manuell","Aluprofil",null,"Aluminium",{"$nulls":8},"Wechsellauf .380Knall","gebraucht"]
["24",null,"Revolver",null,"ME","80GT","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"4/1,5",{"v":433,"d":"433 g"},"vorn","exzentrische Bohrung","Lauf zur Trommelbohrung versetzt",null,"Flutung vor dem Lager","j, integriert","n","SA/DA","keine","Hahnrückzug","Schwenktrommel mit Magazin","manuell per Stift","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff schwarz",{"$nulls":5},"Trommelachsenstift dient als Ausstosser",null,"gebraucht gut"]
["33",null,"Pistole","Repetierer","Röhm","RG3","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":333,"d":"333 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff braun",{"$nulls":7},"gebraucht, Laufgewinde M9*1 "]
["33",null,"Pistole","Repetierer","Röhm","RG3","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":333,"d":"333 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff braun",{"$nulls":6},"andere Beschriftungsvariante"]
["33",null,"Pistole","Repetierer","Röhm","RG3","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":327,"d":"327 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss verchromt","Druckguss verchromt",null,null,"Kunststoff braun",{"$nulls":7},"gebraucht gut"]
["33",null,"Pistole","Repetierer","Röhm","RG3","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":337,"d":"337 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss mattvernickelt","Druckguss mattvernickelt",null,null,"Kunststoff braun",null,null,"0734500",{"$nulls":4},"neu"]
["42",null,"Derringer",null,"Perfecta","G100 Maverick","Deutschland","6mm Flobert Platz","4",{"$nulls":4},{"v":366,"d":"366 g"},"vorn","exzentrische Bohrung",{"$nulls":3},"j, integriert","n","SA","keine","Hahnrast","verschiebbares Laufbündel","manueller Ausstosser","Druckguss vergoldet",null,"Druckguss brüniert",null,"Kunststoff schwarz",{"$nulls":3},"Sharps Derringer",{"$nulls":3},"gebraucht gut"]
["43/2",null,"Revolver",null,"Mayer","G2000","Deutschland",".380Knall/9mm Knall","5","189","32","112","7,5/3",{"v":518,"d":"518 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"eingegossene Sperre","Zusatzlauf","M8","SA/DA",null,null,"Kipplauf","automatischer Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,"Köln","81",null,"Mayer \"G\", PTB88-69",null,null,"gebraucht gut"]
["43/2",null,"Revolver",null,"Mayer","G2000","Deutschland",".380Knall/9mm Knall","5","189","32","112","7,5/3",{"v":524,"d":"524 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"eingegossene Sperre","Zusatzlauf","M8","SA/DA",null,null,"Kipplauf","automatischer Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,"Köln","80",null,"Mayer \"G\", PTB88-69",null,null,"stark gebraucht"]
["44",null,"Revolver",{"$nulls":3},"Deutschland",".380Knall/9mm Knall","5","158","32","101","5/2",{"v":485,"d":"485 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":5},"SA/DA",null,null,"Kipplauf","automatischer Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,"Köln","74",{"$nulls":4},"stark gebraucht"]
["53",null,"Revolver",null,"Röhm","RG59","Deutschland",".380Knall/9mm Knall","5",{"$nulls":3},"6/2,5",{"v":605,"d":"605 g"},"vorn","exzentrische Bohrung","Stahlbolzen in Laufwurzel",null,"Hartmetallkern","j, integriert","n","SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,"Ulm","75",{"$nulls":4},"stark gebraucht","Pappschachtel, Filzeinlage"]
["53",null,"Revolver",null,"Röhm","RG59","Deutschland",".380Knall/9mm Knall","5",{"$nulls":3},"6/2,5",{"v":610,"d":"610 g"},"vorn","exzentrische Bohrung","Stahlbolzen in Laufwurzel",null,"Hartmetallkern","j, integriert","n","SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,"Ulm","76",{"$nulls":4},"gebraucht","Pappschachtel"]
["55",null,"Revolver",null,"Arminius","HW6","Deutschland",".22Knall","8",{"$nulls":4},{"v":741,"d":"741 g"},"vorn","gewendelte Stahlplatte",{"$nulls":3},"Zusatzlauf","n","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Kunststoff braun","970329","Mellrichstadt","78",null,"PTB 89-69",null,null,"gebraucht"]
["55",null,"Revolver",null,"Arminius","HW6","Deutschland",".22Knall","8",{"$nulls":4},{"v":738,"d":"738 g"},"vorn","gewendelte Stahlplatte",{"$nulls":3},"Zusatzlauf","n","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Kunststoff braun","1127591","Mellrichstadt","83",null,"PTB 89-69",null,null,"neuwertig"]
["67",null,"Revolver",null,"Arminius","HW 2 R","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":700,"d":"700 g"},"vorn und seitlich","exzentrische Bohrung",null,null,"exzentrische Bohrung","Zusatzlauf","M10","SA/DA",null,"Hahnrückzug","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Kunststoff braun","490345",null,"75",null,"Arminius HW 10GR PTB218, HW1G",null,null,"stark gebraucht"]
["67",null,"Revolver",null,"Arminius","HW 2 R","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":710,"d":"710 g"},"vorn und seitlich","exzentrische Bohrung",null,null,"exzentrische Bohrung","Zusatzlauf","M10","SA/DA",null,"Hahnrückzug","Schwenktrommel","manueller Ausstosser","Druckguss verchromt",null,"Druckguss verchromt","Stahl verchromt","Kunststoff weiss","949498","München","77",null,"Arminius HW 10GR PTB218, HW1G",null,null,"stark gebraucht"]
["69/2",null,"Pistole","Automatik","Erma","EGP 75","Deutschland","8mm Knall",null,"157","25 (27)","115",null,{"v":540,"d":"540 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl blank",null,"Kunststoff braun","020186","München","77","Walther PPK",{"$nulls":3},"gebraucht"]
["69/3",null,"Pistole","Automatik","Erma","EGP 75","Deutschland","8mm Knall",null,"157","25 (27)","115",null,{"v":551,"d":"551 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl blank",null,"Kunststoff schwarz","031508","München","78","Walther PPK",{"$nulls":3},"gebraucht"]
["69/4",null,"Pistole","Automatik","Erma","EGP 75","Deutschland","8mm Knall",null,"157","25 (27)","115",null,{"v":567,"d":"567 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl blank",null,"Kunststoff schwarz","077113","München","84","Walther PPK",{"$nulls":3},"neu","Pappschactel, Styroporeinlage"]
["72",null,"Revolver",null,"ME","80GT/S","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"4/1,5",{"v":421,"d":"421 g"},"vorn","exzentrische Bohrung","Lauf zur Trommelbohrung versetzt",null,"Flutung vor dem Lager","j, integriert","M10","SA/DA","keine","Hahnrückzug","Schwenktrommel mit Magazin","manuell per Stift","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff schwarz",{"$nulls":5},"Trommelachsenstift dient als Ausstosser",null,"neuwertig"]
["73",null,"Revolver",null,"ME","70GS","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":313,"d":"313 g"},"vorn","exzentrische Bohrung","Lauf zur Trommelbohrung versetzt",null,"verjüngte Bohrung","j, integriert","n","SA/DA","keine","Hahnrückzug","Ladeklappe","manuell per Stift","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",{"$nulls":5},"Trommelachsenstift dient als Ausstosser","Alte Beschriftungsvariante","stark gebraucht"]
["73",null,"Revolver",null,"ME","70GS","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"3,75/1,5",{"v":312,"d":"312 g"},"vorn","exzentrische Bohrung","Lauf zur Trommelbohrung versetzt",null,"verjüngte Bohrung","j, integriert","n","SA/DA","keine","Hahnrückzug","Ladeklappe","manuell per Stift","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",{"$nulls":5},"Trommelachsenstift dient als Ausstosser","Neue Beschriftungsvariante","gebraucht"]
["75",null,"Pistole","Repetierer","IGI Tell","310","Italien","6mm Flobert Platz","6",{"$nulls":3},"6/2,5",{"v":238,"d":"238 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf",null,"DA-Repetiersystem","keine","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss schwarz lackiert","Druckguss schwarz lackiert",null,null,"Kunststoff braun",{"$nulls":7},"neuwertig","Pappschachtel"]
["76",null,"Signalgerät",null,"Erma","SG74","Deutschland","M9/15","1",{"$nulls":4},{"v":100,"d":"100 g"},"n","kein Lauf vorhanden",{"$nulls":3},"j",null,"Handdruck","keine","keine","Bechergewinde",null,"Kunststoff rot",{"$nulls":9},"1er und 6er Magazin"]
["78",null,"Pistole","Automatik","Reck","P6s","Deutschland","8mm Knall",null,"115","22","90",null,{"v":343,"d":"343 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","456187","München","75","früher auch als 6.35er Browning erhältlich, Reck P8",{"$nulls":3},"gebraucht"]
["78",null,"Pistole","Automatik","Reck","P6s","Deutschland","8mm Knall",null,"115","22","90",null,{"v":378,"d":"378 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss verchromt","Druckguss verchromt","Druckguss verchromt",null,"Kunststoff schwarz","482016","München","76","früher auch als 6.35er Browning erhältlich, Reck P8",{"$nulls":3},"gebraucht, Verchromung beschädigt"]
["78",null,"Pistole","Automatik","Reck","P6s","Deutschland","8mm Knall",null,"115","22","90",null,{"v":378,"d":"378 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,"München","78","früher auch als 6.35er Browning erhältlich, Reck P8",{"$nulls":3},"gebraucht"]
["78",null,"Pistole","Automatik","bonanza (Reck)","P6","Deutschland","8mm Knall",null,"115","22","90",null,{"v":378,"d":"378 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss verchromt","Druckguss verchromt","Druckguss verchromt",null,"Holz",null,"Köln","83","früher auch als 6.35er Browning erhältlich, Reck P8",{"$nulls":3},"gebraucht"]
["78",null,"Pistole","Automatik","Reck","P800","Deutschland","8mm Knall",null,"115","22","90",null,{"v":377,"d":"377 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M7fein","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",{"$nulls":3},"früher auch als 6.35er Browning erhältlich, Reck P8",{"$nulls":3},"gebraucht gut"]
["82",null,"Revolver",null,"Xythos",null,null,"2mm Berloque","6",{"$nulls":3},"1,6/1,125",{"v":12,"d":"12 g"},"vorn","keiner",null,null,"keiner","Zusatzlauf","M4fein aussen","DAO",null,"keine","Kipplauf mit Magazin","manuell per Stift","verchromt",null,"verchromt","verchromt","Kunststoff schwarz",{"$nulls":5},"kleinster Revolver",null,"gebraucht","Kunststoffbox"]
["83",null,"Pistole","Automatik","SM","Mod. 15","Deutschland","8mm Knall",null,"116","23","98",null,{"v":382,"d":"382 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","manueller Ausstosser","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun","1396","München","74",{"$nulls":4},"gebraucht gut"]
["83/2",null,"Pistole","Automatik","SM","Mod. 15","Deutschland","8mm Knall",null,"116","23","98",null,{"v":380,"d":"380 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M9x1","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","manueller Ausstosser","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun","150023","München","79",{"$nulls":4},"gebraucht gut"]
["83/2",null,"Pistole","Automatik","Luger","15","Deutschland","8mm Knall",null,"116","23","98",null,{"v":383,"d":"383 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","manueller Ausstosser","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun","5558","Mellrichstadt","97",{"$nulls":4},"gebraucht gut"]
["83/2",null,"Pistole","Automatik","SM","Mod. 15","Deutschland","8mm Knall",null,"116","23","98",null,{"v":380,"d":"380 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M9x1","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","manueller Ausstosser","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun","57801","München","76",{"$nulls":3},"WaA-Stempel mit Bundesadler","stark gebraucht"]
["100",null,"Pistole","Automatik","Mayer+Söhne","G8","Deutschland","8mm Knall","6","116","22","90",null,{"v":337,"d":"337 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","manueller Ausstosser","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff dunkelbraun",null,"Mellrichstadt","80",null,"ME 8 Detective PTB100/2, HS 5 PTB100","dicker Abzugsbügel",null,"stark gebraucht"]
["100",null,"Pistole","Automatik","Mayer+Söhne","G8","Deutschland","8mm Knall","6","116","22","90",null,{"v":336,"d":"336 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","manueller Ausstosser","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff dunkelbraun",null,"Mellrichstadt","80",null,"ME 8 Detective PTB100/2, HS 5 PTB100","dicker Abzugsbügel",null,"neuwert"]
["100",null,"Pistole","Automatik","HS","5A","Deutschland","8mm Knall","6","116","22","90",null,{"v":336,"d":"336 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","117951","Mellrichstadt","75",null,"ME 8 Detective PTB100/2","schlanker Abzugsbügel",null,"gebraucht"]
["100",null,"Pistole","Automatik","HS","5A","Deutschland","8mm Knall","6","116","22","90",null,{"v":339,"d":"339 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,"Mellrichstadt","77",null,"ME 8 Detective PTB100/2","dicker Abzugsbügel",null,"gebraucht gut"]
["100",null,"Pistole","Automatik","HS","5A","Deutschland","8mm Knall","6","116","22","90",null,{"v":339,"d":"339 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,"Mellrichstadt","77",null,"ME 8 Detective PTB100/2","dicker Abzugsbügel","Schlagbolzenfederlager als Zerlegehilfe verlängert und geriffelt","gebraucht gut"]
["100",null,"Pistole","Automatik","HS","5A","Deutschland","8mm Knall","6","116","22","90",null,{"v":341,"d":"341 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,"Mellrichstadt","88",null,"ME 8 Detective PTB100/2","dicker Abzugsbügel",null,"gebraucht gut"]
["100/2",null,"Pistole","Automatik","HS","5","Deutschland","8mm Knall","6","116","22","90",null,{"v":342,"d":"342 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,null,"94",null,"ME 8 Detective PTB100/2","dicker Abzugsbügel",null,"neu"]
["100/2",null,"Pistole","Automatik","ME","8 Detective","Deutschland","8mm Knall","6","116","22","90",null,{"v":345,"d":"345 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,null,"91",null,"HS 5 PTB100ff","dicker Abzugsbügel","gab es 8-schüssig als ME 8 Combat","neuwertig"]
["100/2",null,"Pistole","Automatik","ME","8 Detective II","Deutschland","8mm Knall","6","116","22","90",null,{"v":344,"d":"344 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M9fein","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,"Suhl","93",null,"HS 5 PTB100ff","dicker Abzugsbügel","gab es 8-schüssig als ME 8 Combat","neuwertig"]
["100/2",null,"Pistole","Automatik","ME","8 Detective II","Deutschland","8mm Knall","6","116","22","90",null,{"v":352,"d":"352 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M9fein","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss mattverchromt","Druckguss mattverchromt","Druckguss mattverchromt",null,"Kunststoff schwarz",null,"Suhl","94",null,"HS 5 PTB100ff","dicker Abzugsbügel","gab es 8-schüssig als ME 8 Combat","gebraucht gut"]
["101",null,"Pistole","Repetierer","FB Rekord","GP1","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":315,"d":"315 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf",null,"DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":3},"keins",{"$nulls":3},"stark gebraucht"]
["109",null,"Pistole","Repetierer","Reck","Mariner","Italien","6mm Flobert Platz","7",{"$nulls":4},{"v":356,"d":"356 g"},"oben",null,"Lager rechtwinklig zum Lauf",null,null,"n","n","DA-Repetiersystem","keine","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell","Druckguss schwarz lackiert","Druckguss schwarz lackiert",null,null,"Kunststoff braun",{"$nulls":5},"Griffstück mit PTB 214",null,"stark gebraucht"]
["113",null,"Pistole",null,"FB Rekord","Weinberg u. Signal Pistole","Deutschland","6mm Flobert Platz","1",{"$nulls":4},{"v":151,"d":"151 g"},"vorn",null,"Lager winklig zum Lauf",null,null,"Zusatzlauf",null,"SA","keine","Hahnrast","Einzellader","automatischer Auswurf","Druckguss brüniert",null,"Druckguss brüniert",null,"Kunststoff schwarz",{"$nulls":3},"keins",null,"Verschluss durch Hahn","Signalbecher geschraubt","gebraucht, Korrosionsspuren"]
["113",null,"Pistole",null,"FB Rekord","Weinberg u. Signal Pistole","Deutschland","6mm Flobert Platz","1",{"$nulls":4},{"v":174,"d":"174 g"},"vorn",null,"Lager winklig zum Lauf",null,null,"j, integriert","n","SA","keine","Hahnrast","Einzellader","automatischer Auswurf","Druckguss brüniert",null,"Druckguss brüniert",null,"Kunststoff orange",{"$nulls":3},"keins",null,"Verschluss durch Hahn","Signalbecher ist Teil des Spritzlings","neu"]
["124",null,"Revolver",null,"Em-Ge","38ST","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":530,"d":"530 g"},"oben","Lauf verschlossen",null,null,"vorderer Teil fest, hinterer Teil nur patronenlang","n","n","SA/DA",null,"Hahnrückzug","Ladeklappe","manueller Ausstosser","Druckguss brüniert",null,"Druck brüniert","Druckguss/Stahl brüniert","Kunststoff schwarz","9789",null,null,"keins",{"$nulls":3},"neuwertig"]
["132",null,"Revolver",null,"Perfecta","Mod. G/1","Deutschland",".380Knall/9mm Knall","5","189","32","112","7,5/3",{"v":510,"d":"510 g"},"vorn","enge Bohrung",null,null,"eingegossene Sperre","Zusatzlauf","M8","SA/DA",null,"Hahnrückzug","Kipplauf","automatischer Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun","0816059","Köln","77","keins","Mayer \"G\", PTB88-69",null,null,"stark gebraucht"]
["136",null,"Pistole",null,"FB Rekord","B1s","Deutschland","6mm Flobert Platz","2",{"$nulls":4},{"v":231,"d":"231 g"},"vorn",null,"Lager winklig zum Lauf",null,null,"j, integriert","n","SA, Hahn mit stufenförmiger Schlagfläche","keine","Hahnrast","Einzellader","automatischer Auswurf","Druckguss brüniert",null,"Druckguss brüniert",null,"Kunststoff schwarz",{"$nulls":3},"keins",null,"Verschluss durch Hahn","Signalbecher  mit Schraube befestigt","neu"]
["136",null,"Pistole",null,"FB Rekord","B1s","Deutschland","6mm Flobert Platz","2",{"$nulls":4},{"v":228,"d":"228 g"},"vorn",null,"Lager winklig zum Lauf",null,null,"j, integriert","n","SA, Hahn mit stufenförmiger Schlagfläche","keine","Hahnrast","Einzellader","automatischer Auswurf","Druckguss brüniert",null,"Druckguss brüniert",null,"Kunststoff schwarz",{"$nulls":3},"keins",null,"Verschluss durch Hahn","Signalbecher  mit Kerbstift befestigt","neuwertig"]
["136",null,"Pistole",null,"FB Rekord","B1s","Deutschland","6mm Flobert Platz","2",{"$nulls":4},{"v":232,"d":"232 g"},"vorn",null,"Lager winklig zum Lauf",null,null,"j, integriert","n","SA, Hahn mit stufenförmiger Schlagfläche","keine","Hahnrast","Einzellader","automatischer Auswurf","Druckguss brüniert",null,"Druckguss brüniert",null,"Kunststoff orange",{"$nulls":3},"keins",null,"Verschluss durch Hahn","Signalbecher unlösbar montiert","neu"]
["137",null,"Revolver",null,"Reck","GR 29","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"15/6",{"v":855,"d":"855 g"},"vorn","keiner",null,null,"Lager und Öffnung versetzt","n",null,"SA",null,"Hahnrast","Ladeklappe","manueller Ausstosser","Druckguss brüniert",null,"Stahl brüniert","Stahl brüniert","Kunststoff braun",null,"München","78",{"$nulls":4},"stark gebraucht, teilweise verschrammt"]
["140/2",null,"Revolver",null,"Röhm","RG 76","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":426,"d":"426 g"},"vorn",{"$nulls":4},"j, integriert",null,"SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",{"$nulls":5},"neues Modell",null,"stark gebraucht"]
["147",null,"Pistole",null,"HS","Mod. 2","Deutschland","6mm Flobert Platz","1",{"$nulls":4},{"v":170,"d":"170 g"},"vorn","keiner","Lager winklig zum Lauf",null,null,"Zusatzlauf",null,"SA",null,"keine","Einzellader","automatischer Auswurf","Stahl brüniert",null,"Stahl brüniert",null,"Kunststoff schwarz",{"$nulls":7},"neu","Pappschachtel"]
["154",null,"Pistole","Automatik","Röhm","RG8","Deutschland","8mm Knall",null,"135","23","96",null,{"v":443,"d":"443 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Abzug, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun",null,"Ulm","79",{"$nulls":4},"gebraucht","Pappschachtel"]
["154",null,"Pistole","Automatik","Röhm","RG8","Deutschland","8mm Knall",null,"135","23","96",null,{"v":443,"d":"443 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Abzug, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun",null,"Ulm","82",{"$nulls":4},"gebraucht gut","Pappschachtel"]
["155",null,"Revolver",null,"Em-Ge","G38","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":689,"d":"689 g"},"vorn","Stahleinsatz im lauf",null,null,"exzentrische Bohrung","j, integriert","n","SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Drcukguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Kunststoff braun","5003",null,"77",{"$nulls":4},"gebraucht"]
["162",null,"Revolver",null,"Erma","EGR66","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":566,"d":"566 g"},"vorn",{"$nulls":3},"Lager und Öffnung versetzt","Zusatzlauf",null,"SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert",null,"033081","München","80","S&W 36","EGR66x",null,null,"neu","Pappschachtel, Styroporeinlage"]
["162/2",null,"Revolver",null,"Erma","EGR66x","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":585,"d":"585 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M8fein","SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Edelstahl ",null,"Edelstahl","Edelstahl","Holz","038494","München",null,"S&W 36","EGR66",null,null,"neuwertig"]
["164",null,"Pistole","Automatik","SM","Mod. 110","Deutschland","8mm Knall","6","118","24","86",null,{"v":330,"d":"330 g"},"oben","Lauf nicht durchbohrt",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss verchromt","Druckguss verchromt","Druckguss verchromt",null,"Kunststoff grau",{"$nulls":3},"früher auch als 6.35er Browning erhältlich",null,null,"neue Version der SM110 PTB44-69ff","neuwertig"]
["165",null,"Pistole","Repetierer","M&S Aetna","G3","Deutschland","6mm Flobert Platz","8",{"$nulls":4},{"v":340,"d":"340 g"},"vorn","Lager und Lauf nicht parallel",{"$nulls":3},"j, integriert",null,"DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Röhrenmagazin","automatisch nach oben","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":5},"Auswurf nach oben",null,"neuwertig"]
["165",null,"Pistole","Repetierer","Perfecta","G3","Deutschland","6mm Flobert Platz","8",{"$nulls":4},{"v":333,"d":"333 g"},"vorn","Lager und Lauf nicht parallel",{"$nulls":3},"j, integriert",null,"DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Röhrenmagazin","automatisch nach oben","Druckguss verchromt","Druckguss verchromt",null,null,"Kunststoff schwarz",{"$nulls":5},"Auswurf nach oben",null,"neuwertig"]
["165",null,"Pistole","Repetierer","Perfecta","G3","Deutschland","6mm Flobert Platz","8",{"$nulls":4},{"v":343,"d":"343 g"},"vorn","Lager und Lauf nicht parallel",{"$nulls":3},"j, integriert",null,"DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Röhrenmagazin","automatisch nach oben","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":5},"Auswurf nach oben",null,"neu","Pappschachtel"]
["166",null,"Revolver",null,"Mayer+Söhne","600/1","Deutschland","6mm Flobert Platz","6","176","32","114","6,5/2,5",{"v":475,"d":"475 g"},"vorn",{"$nulls":4},"j, integriert",null,"SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun","1025",{"$nulls":3},"Perfecta 700 PTB193ff",null,null,"Korrosionsfraß Trommel/ Materialausbrechung Lauf"]
["A166/3",null,"Revolver",null,"Geco","360G","Deutschland","6mm Flobert Platz","6","176","32","114","6,5/2,5",{"v":491,"d":"491 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M8","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff schwarz",{"$nulls":4},"Perfecta 700 PTB193ff",null,null,"gebraucht gut"]
["166/4",null,"Revolver",null,"Perfecta","600","Deutschland","6mm Flobert Platz","6","176","32","114","6,5/2,5",{"v":474,"d":"474 g"},"vorn","schräger Stahlstift ",null,null,"Lager und Öffnung versetzt","j, integriert",null,"SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun","1025",{"$nulls":3},"Perfecta 700 PTB193ff",null,null,"neuwertig","Pappschachtel"]
["167",null,"Pistole","Repetierer","FB Rekord","GP1s","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":288,"d":"288 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff braun",{"$nulls":3},"keins",null,null,"Version mit altem Magazinschacht","gebraucht"]
["167",null,"Pistole","Repetierer","FB Rekord","GP1s","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":287,"d":"287 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff braun",{"$nulls":3},"keins",{"$nulls":3},"gebraucht"]
["170",null,"Signalgerät",null,"Xythos/Wischo",null,"Deutschland","6mm Flobert Platz","1",{"$nulls":4},{"v":58,"d":"58 g"},"n","kein Lauf vorhanden",{"$nulls":3},"j","M9x1","Handdruck","Verschraubung",null,"Bechergewinde",null,"Alu rot eloxiert/schwarz",{"$nulls":3},"Kunststoff schwarz",{"$nulls":7},"gebraucht","Plastikbeutel"]
["173",null,"Selbstschussgerät",null,"Wadie",null,"Deutschland",".380Knall/9mm Knall","1",{"$nulls":3},"0/0",null,"vorn","kein Lauf vorhanden",{"$nulls":3},"n","n","Schlagstift mit Rotationsauslösung","Splint","keine","Einzellader","manuell per Stift","Stahlguss grün lackiert",{"$nulls":3},"n.v.",{"$nulls":5},"Verschluss durch Schlagstück",null,"neu ","Pappschachtel"]
["176",null,"Pistole","Automatik","ME","ME 8 Pocket","Deutschland","8mm Knall","8","116","23","115",null,{"v":360,"d":"360 g"},"vorn","Hartmetallplatte länks im Lauf",{"$nulls":3},"Zusatzlauf","M10fein","Schlagbolzenschloss",null,null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz",null,"Mellrichstadt","79",null,null,"Spannzustandsanzeige, Zerlegeknopf","gab es 6-schüssig als ME 8 Detective","gebraucht gut","Pappschachtel"]
["176/2",null,"Pistole","Automatik","ME","ME 8 Combat","Deutschland","8mm Knall","8","116","29","115",null,{"v":373,"d":"373 g"},"vorn","Hartmetallplatte länks im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss",null,null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,"Mellrichstadt","94",{"$nulls":3},"gab es 6-schüssig als ME 8 Detective","neuwertig","Pappschachtel"]
["178",null,"Revolver",null,"Reck","Wildcat Leopard","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"10/4",{"v":903,"d":"903 g"},"vorn","trommelseitig 2 Stahlstifte neben der Bohrung",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M6","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Stahl brüniert, Aluschiene schwarz/blank","Stahl brüniert","Kunststoff braun",null,"München","78",null,null,"ventilierte Laufschiene, Trommel alte Bauform",null,"gebraucht sehr gut"]
["178",null,"Revolver",null,"Reck","Wildcat Panther","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"7,5/3",{"v":877,"d":"877 g"},"vorn","trommelseitig 2 Stahlstifte neben der Bohrung",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M8","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Stahl brüniert, Aluschiene schwarz/blank","Stahl brüniert","Kunststoff braun",null,"Köln","78",null,null,"ventilierte Laufschiene, Trommel neue Bauform",null,"gebraucht sehr gut","Pappschachtel, Schaumeinlage"]
["178/2",null,"Revolver",null,"Reck","GR90","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":987,"d":"987 g"},"vorn","trommelseitig 2 Stahlstifte neben der Bohrung",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M6","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Stahl brüniert","Stahl brüniert","Holz",null,"Köln","79",{"$nulls":4},"gebraucht gut"]
["178/2",null,"Revolver",null,"Reck","GR90","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":1003,"d":"1,003 g"},"vorn","trommelseitig 2 Stahlstifte neben der Bohrung",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M6","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Stahl brüniert","Stahl brüniert","Holz",null,"Köln","82",{"$nulls":4},"gebraucht gut"]
["179",null,"Revolver",null,"ME","220","Deutschland",".22Knall","6",{"$nulls":3},"5/2",{"v":450,"d":"450 g"},"vorn","eingegossener Schlitz ","Lauf zur Trommelbohrung versetzt",null,"Flutung vor dem Lager","Zusatzlauf","M8","SA/DA","keine","Hahnrückzug","Schwenktrommel","manuell per Stift","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff schwarz",null,null,"93",null,null,"Trommelachsenstift dient als Ausstosser",null,"gebraucht gut"]
["181",null,"Revolver",null,"Röhm","RG 77","Deutschland",".22Knall","6",{"$nulls":4},{"v":412,"d":"412 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Öffnung nicht rund","Zusatzlauf","M8","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,null,"80",{"$nulls":4},"stark gebraucht","Pappschachtel"]
["189",null,"Revolver",null,"HS","Mod. 121","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"12,5/5",{"v":1169,"d":"1,169 g"},"vorn","längs eingegossener Schlitz ",null,null,"Hartmetallkern","j, integriert","n","SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Messing/Holz",null,"München","80","Colt SAA",{"$nulls":3},"gebraucht"]
["193",null,"Revolver",null,"Mayer+Söhne","Mod.700/1","Deutschland",".22Knall","6","176","32","114","6,5/2,5",{"v":488,"d":"488 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Hartmetallkern","j, integriert",null,"SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,"Köln","82",null,"Mayer+Söhne 600/1 PTB166",null,null,"gebraucht"]
["A193/3",null,"Revolver",null,"Geco","322G","Deutschland",".22Knall","6","176","32","114","6,5/2,5",{"v":486,"d":"486 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Hartmetallkern","Zusatzlauf","M8","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff schwarz/weiss lackiert",null,null,"81",null,"Mayer+Söhne 600/1 PTB166",null,null,"stark gebraucht, Hahnfeder fehlt"]
["193/4",null,"Revolver",null,"Perfecta","700","Deutschland",".22Knall","6","176","32","114","6,5/2,5",{"v":479,"d":"479 g"},"vorn",{"$nulls":4},"j, integriert",null,"SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",{"$nulls":4},"Mayer+Söhne 600/1 PTB166",null,null,"neu, matte Brünierung links anpoliert"]
["195",null,"Pistole","Repetierer","Perfecta","G","Deutschland","6mm Flobert Platz","8",{"$nulls":4},{"v":256,"d":"256 g"},"vorn","Lager und Lauf nicht parallel",{"$nulls":3},"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Röhrenmagazin","automatisch nach oben","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":5},"Auswurf nach oben",null,"neuwertig","Pappschachtel"]
["196",null,"Pistole","Automatik","Reck","PK 800","Deutschland","8mm Knall","7","155","25","117",null,{"v":547,"d":"547 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl poliert",null,"Kunststoff schwarz",null,"Köln","79","Walther PPK","Perfecta ElAlamein PTB196/2 / Mauser Hsc84 PTB335ff","alte Schlosskonstruktion",null,"stark gebraucht"]
["196",null,"Pistole","Automatik","Reck","PK 800","Deutschland","8mm Knall","7","155","25","117",null,{"v":511,"d":"511 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen","keine","Magazin","automatischer Auswurf","Druckguss verchromt","Druckguss verchromt","Stahl verchromt",null,"Kunststoff schwarz",null,"Köln","82","Walther PPK","Perfecta ElAlamein PTB196/2 / Mauser Hsc84 PTB335ff","neue Schlosskonstruktion",null,"stark gebraucht"]
["196",null,"Pistole","Automatik","Reck","PK 800","Deutschland","8mm Knall","7","155","25","117",null,{"v":511,"d":"511 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen","keine","Magazin","automatischer Auswurf","Druckguss vergoldet","Druckguss vergoldet","Stahl vergoldet",null,"Kunststoff schwarz",null,"Köln","78","Walther PPK","Perfecta ElAlamein PTB196/2 / Mauser Hsc84 PTB335ff","alte Schlosskonstruktion",null,"gebraucht sehr gut","Pappschachtel, Schaumeinlage"]
["196",null,"Pistole","Automatik","Perfecta","El Alamein","Deutschland","8mm Knall","7","155","25","117",null,"541 g","vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun",null,"Köln","84","Walther PPK","Reck PK800 PTB196 / Mauser Hsc84 PTB335ff","nur Reck-Standardgriffschalen",null,"gebraucht gut"]
["196/2",null,"Pistole","Automatik","Reck","PK 800","Deutschland","8mm Knall","7","155","25","117",null,"536 g","vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M7fein","SA/DA","Schlagbolzen","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun",null,"Köln","96","Walther PPK","Perfecta ElAlamein PTB196/2 / Mauser Hsc84 PTB335ff","Schlitten gläzend",null,"gebraucht sehr gut, Schlitten neu"]
["196/2",null,"Pistole","Automatik","Reck","PK 800","Deutschland","8mm Knall","7","155","25","117",null,"534","vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M7fein","SA/DA","Schlagbolzen","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun",null,"Köln","90","Walther PPK","Perfecta ElAlamein PTB196/2 / Mauser Hsc84 PTB335ff","Schlitten matt",null,"neu, NOS","Pappschachtel, Schaumeinlage"]
["196/2",null,"Pistole","Automatik","Perfecta","El Alamein","Deutschland","8mm Knall","7","155","25","117",null,{"v":535,"d":"535 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun",null,"Köln","91","Walther PPK","Reck PK800 PTB196 / Mauser Hsc84 PTB335ff","Griffschalen mit Adlerdecor 3. Reich, aber ohne HK",null,"neuwertig"]
["196/2",null,"Pistole","Automatik","Perfecta","El Alamein","Deutschland","8mm Knall","7","155","25","117",null,{"v":535,"d":"535 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun",null,"Köln","89","Walther PPK","Reck PK800 PTB196 / Mauser Hsc84 PTB335ff","Griffschalen mit Adlerdecor 3. Reich, aber ohne HK",null,"neuwertig"]
["196/2",null,"Pistole","Automatik","Perfecta","FBI8000","Deutschland","8mm Knall","7","155","25","117",null,{"v":531,"d":"531 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,"Köln","85","Walther PPK","Reck PK800 PTB196 / Mauser Hsc84 PTB335ff",null,null,"gebraucht gut"]
["200",null,"Pistole","Repetierer","IGI","Protector Mod.600","Italien","6mm Flobert Platz","8",{"$nulls":4},{"v":237,"d":"237 g"},"vorn","Sperre im Lauf","Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","keine","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss schwarz lackiert","Druckguss schwarz lackiert","Druckguss schwarz lackiert",null,"Kunststoff braun",{"$nulls":7},"gebraucht","Pappschachtel"]
["201",null,"Revolver",null,"IGI","Protector","Italien","6mm Flobert Platz","8",{"$nulls":4},{"v":372,"d":"372 g"},"vorn","Sperre im Lauf",null,null,"Metallkern","Zusatzlauf","M8","SA/DA",null,"keine","Schwenktrommel","manueller Ausstoßer","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff braun","3?697","Italien",{"$nulls":5},"neu"]
["203",null,"Revolver",null,"ME","ME 380 Spezial","Deutschland",".380Knall/9mm Knall","5",{"$nulls":3},"5/2",{"v":609,"d":"609 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,null,"80",null,null,"mit Ausstosserstangengehäuse",null,"gebraucht"]
["203",null,"Revolver",null,"ME","ME 9 R","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":608,"d":"608 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,null,"83",null,null,"ohne Ausstosserstangengehäuse",null,"gebraucht"]
["203/2",null,"Revolver",null,"ME","ME 38 Marshal","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":602,"d":"602 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,null,"93",null,null,"ohne Ausstosserstangengehäuse",null,"gebraucht"]
["203/2",null,"Revolver",null,"ME","ME 38 Marshal","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":600,"d":"600 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff schwarz","106583",{"$nulls":4},"mit Ausstosserstangengehäuse",null,"gebraucht"]
["203/2",null,"Revolver",null,"HS","Undercover","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":602,"d":"602 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,null,"9/93",null,null,"kein Hahnsporn, mit Ausstosserstangengehäuse",null,"neuwertig"]
["204",null,"Revolver",null,"ME","76","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"5/2",{"v":329,"d":"329 g"},"vorn","Bohrung nicht rund",null,null,"Flutung vor dem Lager","Zusatzlauf","M8","SA/DA","keine","Hahnrückzug","Ladeklappe","manuell per Stift","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",{"$nulls":5},"Trommelachsenstift dient als Ausstosser",null,"neuwertig"]
["205",null,"Revolver",null,"ME","86","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":443,"d":"443 g"},"vorn","Bohrung nicht rund",null,null,"verjüngte Bohrung","Zusatzlauf","M8","SA/DA","keine","Hahnrückzug","Schwenktrommel mit Magazin","manuell per Stift","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",{"$nulls":5},"Trommelachse dient als Ausstosser",null,"gebraucht"]
["206",null,"Revolver",null,"H&R","900","USA",".380Knall/9mm Knall","6",{"$nulls":4},{"v":842,"d":"842 g"},"vorn","schräge Stahlbolzen im Lauf",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M6","SA/DA",null,null,"Kipplauf","manueller Ausstosser","Stahl brüniert",null,"Stahl brüniert","Stahl brüniert","Holz","AT162210",null,"80",{"$nulls":4},"neu"]
["208",null,"Pistole","Automatik","Erma","EGP 55","Deutschland","8mm Knall",null,"136","23 (25)","100","7/2,75",{"v":405,"d":"405 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff schwarz","000444","München","75","Walther TPH","PTB 399",null,"gilt als beste Kopie der Walther TPH","gebraucht"]
["208",null,"Pistole","Automatik","Erma","EGP 55","Deutschland","8mm Knall",null,"136","23 (25)","100","7/2,75",{"v":404,"d":"404 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff braun","006317","München","79","Walther TPH","PTB 399",null,"gilt als beste Kopie der Walther TPH","gebraucht gut"]
["209",null,"Pistole","Automatik","Erma","KGP 690","Deutschland","8mm Knall","6","187","32","126","9/3,5",{"v":781,"d":"781 g"},"vorn",{"$nulls":4},"Zusatzlauf",null,"Schlagbolzenschloss","Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz","008917","München","81","Luger P 08",null,null,"Massstab kleiner als Original, keine genaue Kopie","neuwertig"]
["210",null,"Revolver",null,"Arminius","HW1G","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":709,"d":"709 g"},"vorn","Öffnung nicht rund",null,null,"exzentrische Bohrung, HM-Stift","Zusatzlauf","M10","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss verchromt",null,"Druckguss verchromt","Stahl verchromt","Kunststoff braun","1165905",null,"89",null,"PTB 89-69",null,null,"neuwertig"]
["213",null,"Revolver",null,"Reck","Wildcat Tiger","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"15/6",{"v":1083,"d":"1,083 g"},"vorn","trommelseitig 2 Stahlstifte neben der Bohrung",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M6","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Stahl brüniert, Aluschiene schwarz/blank","Stahl brüniert","Holz",null,"Köln","82",null,null,"ventilierte Laufschiene, Trommel alte Bauform",null,"stark gebraucht"]
["213",null,"Revolver",null,"Reck","Wildcat Tiger","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"15/6",{"v":1082,"d":"1,082 g"},"vorn","trommelseitig 2 Stahlstifte neben der Bohrung",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M6","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Stahl brüniert, Aluschiene schwarz/blank","Stahl brüniert","Holz",null,null,"82",null,null,"ventilierte Laufschiene, Trommel neue Bauform",null,"gebraucht gut"]
["214",null,"Pistole","Repetierer","Mondial","REK-PROTECTOR","Italien","6mm Flobert Platz","6",{"$nulls":4},{"v":247,"d":"247 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf",null,"DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss schwarz lackiert","Druckguss schwarz lackiert",null,null,"Kunststoff braun","AZ17110",{"$nulls":4},"Mündung alte Bauweise, angedeutete Züge",null,"stark gebraucht"]
["214",null,"Pistole","Repetierer","Mondial","REK-PROTECTOR","Italien","6mm Flobert Platz","6",{"$nulls":4},{"v":251,"d":"251 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf",null,"DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss schwarz lackiert","Druckguss schwarz lackiert",null,null,"Kunststoff braun","CZ13766",{"$nulls":4},"Mündung neue Bauweise",null,"stark gebraucht"]
["214",null,"Pistole","Repetierer","Mondial","RECK-PROTECTOR","Italien","6mm Flobert Platz","6",{"$nulls":4},{"v":248,"d":"248 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss schwarz lackiert","Druckguss schwarz lackiert",null,null,"Kunststoff braun","Z64370",{"$nulls":6},"stark gebraucht","Pappschachtel"]
["215",null,"Pistole","Automatik","Reck","Baby Automatik","Deutschland","8mm Knall",null,"135","24","101",null,{"v":451,"d":"451 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun",null,"Köln","79",null,"PTB 12, 386, 387, 421",null,null,"gebraucht gut"]
["216",null,"Revolver",null,"Reck","San Francisco","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":617,"d":"617 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M10fein","SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Druckguss verchromt",null,"Druckguss verchromt","Druckguss verchromt","Holz",{"$nulls":6},"Auf linker Seite eingraviertes NRW-Wappen","gebraucht gut"]
["216",null,"Revolver",null,"Reck","Cobra","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":609,"d":"609 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M10fein","SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,null,"90",{"$nulls":4},"gebraucht gut"]
["216",null,"Revolver",null,"Mauser/Umarex","K50","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":617,"d":"617 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M10fein","SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,"Köln","93",{"$nulls":4},"gebraucht gut"]
["216",null,"Revolver",null,"Mauser/Umarex","K50","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":604,"d":"604 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M10fein","SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Druckguss mattverchromt",null,"Druckguss mattverchromt","Druckguss mattverchromt","Holz",null,"Köln","87",{"$nulls":4},"gebraucht"]
["217",null,"Revolver",null,"ME","900SA","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"12,5/5",{"v":755,"d":"755 g"},"vorn","Sperre",null,null,"Lager und Öffnung versetzt","Zusatzlauf",null,"SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Holz","044","Ulm","79","Colt SAA","HS 21 ",null,null,"stark gebraucht, Hahn rastet nicht ein"]
["217",null,"Revolver",null,"ME","900SA","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"12,5/5",{"v":816,"d":"816 g"},"vorn","Sperre",null,null,"Lager und Öffnung versetzt","Zusatzlauf",null,"SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Holz",null,"Ulm","87","Colt SAA","HS 21 ",null,null,"gebraucht gut"]
["217",null,"Revolver",null,"ME","900SAM","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"12,5/5",{"v":853,"d":"853 g"},"vorn","Sperre",null,null,"Lager und Öffnung versetzt","Zusatzlauf",null,"SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss brüniert",null,"Stahl brüniert","Stahl brüniert","Messing/Holz","078","Ulm","92","Colt SAA","HS 21 ",null,null,"neu"]
["218",null,"Revolver",null,"Arminius","HW10GR","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":670,"d":"670 g"},"vorn",{"$nulls":3},"exzentrische Bohrung, HM-Stift","Zusatzlauf",null,"SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Kunststoff braun",{"$nulls":4},"Geco 900G PTB410",null,null,"neu","Pappschachtel, Styroporeinschub"]
["222",null,"Pistole",null,"Xythos","Mini-Pistole",null,"2mm Berloque","1",{"$nulls":3},"1,6/1,125",{"v":10,"d":"10 g"},"vorn","keiner",{"$nulls":3},"Zusatzlauf","M4fein aussen","SA","keine","keine","Kipplauf","manuell per Stift","verchromt",null,"verchromt",null,"keine",{"$nulls":7},"gebraucht","Holzkiste, Schaumeinlage"]
["223",null,"Revolver",null,"Umarex","Sherlock Holmes","Italien",".22Knall","6",{"$nulls":4},{"v":403,"d":"403 g"},"vorn","Stahlplatte längs im Lauf","nur obere Hälfte offen",null,"Hartmetallkern, Öffnung nicht rund","Zusatzlauf","M12fein","SA/DA",null,"keine","Schwenktrommel","manueller Ausstosser","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Holz","BT54368",{"$nulls":6},"stark gebraucht"]
["224",null,"Revolver",null,"Mondial/Umarex","1917","Italien","6mm Flobert Platz","12",{"$nulls":4},{"v":341,"d":"341 g"},"vorn",{"$nulls":3},"keiner, nur verjüngte Bohrung","Zusatzlauf",null,"SA/DA",null,null,"Ladeklappe","manuell per Stift","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff braun","25655",null,null,"S&W 1917 ?",null,"Trommel alte Bauweise",null,"stark gebraucht"]
["224",null,"Revolver",null,"Mondial/Umarex","1917","Italien","6mm Flobert Platz","12",{"$nulls":4},{"v":340,"d":"340 g"},"vorn",{"$nulls":3},"Öffnung nicht rund","Zusatzlauf",null,"SA/DA",null,null,"Ladeklappe","manuell per Stift","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff braun","PZ1633",null,null,"S&W 1917 ?",null,"Trommel neue Bauweise",null,"gebraucht"]
["225",null,"Revolver",null,"Mondial/Umarex","999","Italien","6mm Flobert Platz","8",{"$nulls":4},{"v":287,"d":"287 g"},"vorn",{"$nulls":4},"Zusatzlauf",null,"SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff braun","U19558",{"$nulls":6},"neuwertig"]
["227",null,"Revolver",null,"MAM/Umarex","777","Italien","6mm Flobert Platz","8",{"$nulls":4},{"v":350,"d":"350 g"},"vorn","Öffnung nicht rund","Sperre waagrecht",null,"Öffnung nicht rund","Zusatzlauf","M10","SA/DA",null,"keine","Schwenktrommel","manueller Ausstosser","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff braun","54159",{"$nulls":5},"schrottig ab Werk","gebraucht"]
["228",null,"Revolver",null,"Geco","390G","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":588,"d":"588 g"},"vorn",null,"Hartmetallplatte längs im Lauf",null,"Hartmetallkern","Zusatzlauf","M10fein","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff schwarz",{"$nulls":4},"Reck Bodyguard, PTB453",null,null,"stark gebraucht"]
["228",null,"Revolver",null,"Perfecta","901","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":590,"d":"590 g"},"vorn",null,"Hartmetallplatte längs im Lauf",null,"Hartmetallkern","Zusatzlauf","M10fein","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,null,"88",null,"Reck Bodyguard, PTB453",null,null,"gebraucht","Kunststoffbox"]
["230",null,"Gewehr","Unterhebel","Erma","EG294","Deutschland",".22Knall",{"$nulls":5},{"v":2460,"d":"2,460 g"},"oben","Lauf nicht durchbohrt",{"$nulls":3},"n",null,"Unterhebelrepetierer",null,"Hahnrast","Röhrenmagazin","manueller Auswurf","Druckguss brüniert",null,"Stahl brüniert",null,"Holz","002109","München","88","Winnchester UHR",{"$nulls":3},"gebraucht sehr gut"]
["233",null,"Revolver",null,"Erma","EGR77","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"10/4",{"v":1052,"d":"1,052 g"},"vorn",{"$nulls":4},"Zusatzlauf",null,"SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Gummi braun","004263","München","81","S&W",{"$nulls":3},"gebraucht"]
["233",null,"Revolver",null,"Erma","EGR77","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"6,3/2,5",{"v":972,"d":"972 g"},"vorn",{"$nulls":4},"Zusatzlauf",null,"SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Gummi braun","018475","München","89","S&W",{"$nulls":3},"gebraucht"]
["234",null,"Revolver",null,"Orion/Hege",".357 Python","Italien","6mm Flobert Platz","6",{"$nulls":3},"10/4",{"v":1008,"d":"1,008 g"},"oben","Lauf verschlossen",null,null,"seitliche Bohrung","n",null,"SA/DA",null,"keine","Schwenktrommel","manueller Ausstosser","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff schwarz",{"$nulls":3},"Colt Python",null,"Startrevolver",null,"gebraucht"]
["237",null,"Revolvergewehr",null,"Reck","Wildcat Gepard","Deutschland",".380Knall/9mm Knall","6",{"$nulls":5},"vorn",{"$nulls":3},"Lager und Öffnung versetzt","Zusatzlauf",null,"SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Stahl brüniert, Aluschiene","Stahl brüniert","Holz",null,null,"80",null,null,"ventilierte Laufschiene",null,"gebraucht gut"]
["238",null,"Pistole","Automatik","Reck","Commander","Deutschland","8mm Knall",null,"157","32","114","8/3,25",{"v":596,"d":"596 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert","Holz",{"$nulls":3},"Colt Commander",null,null,"Massstab kleiner als Original, kein Beschussstempel sichtbar","gebraucht"]
["239",null,"Pistole","Repetierer","Perfecta","S","Deutschland","6mm Flobert Platz","8",{"$nulls":4},{"v":311,"d":"311 g"},"oben",null,"Lager und Lauf nicht parallel",null,null,"n","n","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Röhrenmagazin","automatisch nach oben","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":5},"Auswurf nach oben",null,"gebraucht gut"]
["240",null,"Pistole","Repetierer","Mayer+Söhne","G","Deutschland","6mm Flobert Platz","8",{"$nulls":4},{"v":324,"d":"324 g"},"vorn",null,"Lager und Lauf nicht parallel",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Röhrenmagazin","automatisch nach oben","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":5},"Auswurf nach oben",null,"gebraucht"]
["241",null,"Revolver",null,"HS","Texas Scout \"Frontier\" / Mod. 121","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"14/5,5",{"v":1089,"d":"1,089 g"},"vorn","längs eingegossener Schlitz ",null,null,"Hartmetallkern","j, integriert","n","SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,"Mellrichstadt","84","Colt SAA",{"$nulls":3},"gebraucht"]
["241",null,"Revolver",null,"HS","Texas Scout \"Frontier\" / Mod. 121","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"14/5,5",{"v":1133,"d":"1,133 g"},"vorn","längs eingegossener Schlitz ",null,null,"Hartmetallkern","j, integriert","n","SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss verchromt",null,"Druckguss verchromt","Stahl verchromt","Holz",null,"München","81","Colt SAA",{"$nulls":3},"gebraucht"]
["242",null,"Revolver",null,"HS","Texas Scout Army 1873 / Mod. 121","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"18,75/7,5",{"v":1236,"d":"1,236 g"},"vorn",{"$nulls":3},"Hartmetallkern","Zusatzlauf",null,"SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Stahl buntgehärtet",null,"Stahl brüniert","Druckguss brüniert","Holz",null,"Ulm","89","Colt SAA",{"$nulls":3},"neu","Pappschachtel"]
["242",null,"Revolver",null,"HS","Texas Scout \"Peacemaker\" / Mod. 121","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"18,75/7,5",{"v":1164,"d":"1,164 g"},"vorn",{"$nulls":3},"Hartmetallkern","Zusatzlauf",null,"SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss verchromt",null,"Stahl verchromt","Druckguss verchromt","Holz",null,"Ulm","86","Colt SAA",{"$nulls":3},"neu","Pappschachtel"]
["243",null,"Revolver",null,"Röhm","RG 79","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":626,"d":"626 g"},"vorn","Stahlbolzen schräg im Laufdach",null,null,"exzentrische Bohrung","Zusatzlauf","M10","SA/DA",null,"Hahnrückzug","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,"Ulm","83",{"$nulls":4},"gebraucht"]
["245",null,"Revolver",null,"ME-Import","Jaguar80","Italien",".380Knall/9mm Knall","5",{"$nulls":4},{"v":645,"d":"645 g"},"vorn",{"$nulls":4},"Zusatzlauf","M12","SA/DA",null,"keine","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz","01777",null,"80",{"$nulls":4},"gebraucht"]
["245",null,"Revolver",null,"ME-Import","Jaguar80","Italien",".380Knall/9mm Knall","5",{"$nulls":4},{"v":639,"d":"639 g"},"vorn",{"$nulls":4},"Zusatzlauf","M12","SA/DA",null,"keine","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz","124898","Köln","91",{"$nulls":4},"gebraucht"]
["245",null,"Revolver",null,"ME-Import","Jaguar80","Italien",".380Knall/9mm Knall","5",{"$nulls":4},{"v":641,"d":"641 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Hartmetallkern","Zusatzlauf","M12","SA/DA",null,"keine","Schwenktrommel","manueller Ausstosser","Druckguss verchromt",null,"Druckguss verchromt","Druckguss verchromt","Holz","192649","Italien"," ",{"$nulls":4},"gebraucht"]
["246",null,"Revolver",null,"Neumann Pedersoli","Western Army 1860","Italien",".380Knall/9mm Knall","6",{"$nulls":3},"20/8",{"v":1231,"d":"1,231 g"},"vorn und oben","Stahlsperre",null,null,"Lager und Öffnung versetzt","n",null,"SA",null,"Hahnrast","Öffnung im Rahmen","manuell","Messing blank",null,"Stahl brüniert","Stahl brüniert","Holz","4684","Mellrichstadt","84","Colt 1860 Army",null,"Originalrevolver umgebaut auf 9mm Knall",null,"neu","Pappschachtel mit Styroporeinschub"]
["249",null,"Pistole","Repetierer","Röhm","Mini1","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":131,"d":"131 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"j, integriert",null,"DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Kunststoff schwarz","Kunststoff schwarz","Kunststoff schwarz",null,"Kunststoff braun",{"$nulls":5},"Waffe ist bis auf Schlossteile und Laufeinsatz komplett aus Kunststoff",null,"gebraucht gut"]
["253",null,"Revolver",null,"ME","380 Police","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":668,"d":"668 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Hartmetallkern","Zusatzlauf","M10","SA/DA",null,"Hahnrückzug","Schwenktrmmel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",{"$nulls":4},"ME 38 Marshal",null,null,"stark gebraucht"]
["256",null,"Unterhebelrepetierer",null,"Reck","Lever Action","Deutschland",".22Knall","~10",{"$nulls":5},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M6","SA",null,"keine","Röhrenmagazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl brüniert",null,"Holz",{"$nulls":6},"munitionsempfindlich","gebraucht"]
["257",null,"Revolver",null,"Webley/Enfield / Orion","Mk?","Grossbritannien",".380Knall/9mm Knall","6",{"$nulls":4},{"v":805,"d":"805 g"},"vorn","Buchse",null,null,"Stahlbolzen zwischen den Kammern","Zusatzlauf","M10fein","DAO",null,"Hammerblock","Kipplauf","automatischer Ausstosser","Stahl brüniert",null,"Stahl brüniert","Stahl brüniert","Kunststoff schwarz","T4673",null,"82",null,null,"Originalstück auf .380Knall/9mm Knall geändert",null,"gebraucht"]
["258",null,"Revolver",null,"HS","Mod. 21 C","Deutschland","6mm Flobert Platz","6",{"$nulls":3},"12,5/5",{"v":880,"d":"880 g"},"vorn","längs eingegossener Schlitz ",null,null,"Hartmetallkern","Zusatzlauf",null,"SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",{"$nulls":3},"Colt SAA",{"$nulls":3},"gebraucht"]
["259",null,"Revolver",null,"HS","Texas Scout \"Buntline Special\" / Mod.121","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"40/16",{"v":2650,"d":"2,650 g"},"vorn","Hartmetallhalbmonde in Laufwurzel",null,null,"Hartmetallkern","Zusatzlauf","M12fein","SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss brüniert",null,"Stahl brüniert","Druckguss brüniert","Holz",null,"Mellrichstadt","83","Colt SAA Buntline",null,"Vorrichtung für Anschlagschaft, dieser vermutl. nicht original","restaurierter Schrott, Trommel von baugleichem PTB241-Revolver","gebraucht"]
["263",null,"Pistole","Automatik","ME","B.A.P.","Deutschland","8mm Knall",null,"113","24","73","5/2",{"v":234,"d":"234 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl brüniert",null,"Kunststoff schwarz",null,null,"88","FN Baby",null,"kleinste Automatikpistole, ohne Magazin ist Abzug ohne Funktion",null,"neuwertig","Pappschachtel"]
["265",null,"Revolver",null,"Arminius","Western Six Shooter","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"20/8",{"v":1084,"d":"1,084 g"},"vorn",{"$nulls":4},"j, integiert","n","SA","Hahhnrast","Hahnrast","Ladeklappe","manueller Ausstosser","Druckguss brüniert",null,"Stahl brüniert","Stahl brüniert","Holz","R1953","Mellrichstadt","86","Colt SAA",{"$nulls":3},"gebraucht gut","Pappschachtel, Styroporeinschub"]
["266",null,"Revolver",null,"Mayer+Söhne","22SA","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"12,5/5",{"v":827,"d":"827 g"},"vorn","Öffnung nicht rund",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M10","SA",null,"Hahnrast","Ladeklappe","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Holz",null,"Köln","82","Colt SAA","Geco 90SA PTB 324",null,null,"gebraucht"]
["267",null,"Pistole","Automatik","SM","80","Deutschland","8mm Knall",null,"153","27","119","8,5/3,25",{"v":640,"d":"640 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss verchromt","Druckguss verchromt","Druckguss verchromt",null,"Holz",null,"Mellrichstadt","82",null,null,"Zerlegehilfe",null,"neuwertig"]
["267",null,"Pistole","Automatik","SM","80","Deutschland","8mm Knall",null,"153","27","119","8,5/3,25",{"v":642,"d":"642 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss mattverchromt","Druckguss mattverchromt","Druckguss mattverchromt",null,"Kunststoff schwarz",null,"Mellrichstadt","91",null,null,"Zerlegehilfe",null,"gebraucht gut"]
["267",null,"Pistole","Automatik","SM","80","Deutschland","8mm Knall",null,"153","27","119","8,5/3,25",{"v":648,"d":"648 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz",null,"Mellrichstadt","94",null,null,"Zerlegehilfe",null,"neu","Pappschachtel"]
["272",null,"Pistole","Automatik","Reck","PK 800 Start","Deutschland","8mm Knall","7",{"$nulls":4},{"v":543,"d":"543 g"},"oben","Lauf nicht durchbohrt",{"$nulls":3},"n","n","SA/DA","Schlagbolzen","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff braun",null,"Köln","82","Walther PPK","Perfecta ElAlamein PTB196/2 / Mauser Hsc84 PTB335ff","alte Schlosskonstruktion","Startversion","neuwertig"]
["275",null,"Revolver",null,"Röhm","RG 69","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":709,"d":"709 g"},"vorn","Stahlbolzen schräg im Laufdach",null,null,"exzentrische Bohrung","Zusatzlauf","M10","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl Brüniert","Holz",null,"Ulm","82",null,"PTB 354",null,null,"gebraucht gut"]
["276",null,"Derringer",null,"Noris","Twi-Nine","Deutschland",".380Knall/9mm Knall","2",{"$nulls":4},{"v":377,"d":"377 g"},"vorn","Hartmetallplatte längs im Lauf","Lager leicht versetzt",null,null,"Zusatzlauf","M12","SA mit wechselseitig kippenden Schlagstück","Hahn, Drehhebel","Hahnrast","Kipplauf","manuell per Schieber","Druckguss brüniert",null,"Druckguss brüniert",null,"Kunststoff schwarz",null,"Ulm","91",null,null,"Laufachse geschraubt","Modell von Röhm, aber Alleinvertrieb von Noris","gebraucht gut","Pappschachtel, Schaumeinlage"]
["276",null,"Derringer",null,"Noris","Twi-Nine","Deutschland",".380Knall/9mm Knall","2",{"$nulls":4},{"v":371,"d":"371 g"},"vorn","Hartmetallplatte längs im Lauf","Lager leicht versetzt",null,null,"Zusatzlauf","M12","SA mit wechselseitig kippenden Schlagstück","Hahn, Drehhebel","Hahnrast","Kipplauf","manuell per Schieber","Druckguss brüniert",null,"Druckguss brüniert",null,"Kunststoff schwarz",null,"Ulm","84",null,null,"Laufachse verstiftet","Modell von Röhm, aber Alleinvertrieb von Noris","stark gebraucht, Scharnierstift locker","Pappschachtel, Schaumeinlage"]
["281",null,"Revolver",null,"Umarex","Dallas","Italien",".380Knall/9mm Knall","5",{"$nulls":4},{"v":537,"d":"537 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M8","SA/DA",null,"Hammerblock","Schwenktommel","manueller Ausstosser","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Holz",{"$nulls":3},"S&W 66, Chief Soecial",{"$nulls":3},"stark gebraucht"]
["281",null,"Revolver",null,"Umarex","Chief Special","Italien",".380Knall/9mm Knall","5",{"$nulls":4},{"v":509,"d":"509 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M8","SA/DA",null,"Hammerblock","Schwenktommel","manueller Ausstosser","Druckguss ",null,"Druckguss ","Druckguss","Holz","G02963",null,"AI","S&W 66, Chief Soecial",{"$nulls":3},"stark gebraucht, schwarze Lackierung nicht mehr vorhanden"]
["282/2",null,"Revolver",null,"Umarex","Police Python","Italien",".380Knall/9mm Knall","6",{"$nulls":3},"10/4",null,"vorn","Hartmetallplatte längs im Lauf",null,null,"exzentrische Bohrung","Zusatzlauf",null,"SA/DA",null,"keine","Schwenktrommel","manueller Ausstosser","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff schwarz",null,"Italien",null,"Colt Python",{"$nulls":3},"gebraucht"]
["282-3",null,"Revolver",null,"Umarex","Python","Italien",".380Knall/9mm Knall","6",{"$nulls":4},{"v":968,"d":"968 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"exzentrische Bohrung","Zusatzlauf",null,"SA/DA",null,"keine","Schwenktrommel","manueller Ausstosser","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff schwarz","392618","Italien",null,"Colt Python",{"$nulls":3},"gebraucht gut"]
["286",null,"Signalgerät",null,"IWS","P-2",null,"M10/15","1",{"$nulls":4},{"v":77,"d":"77 g"},"n","kein Lauf vorhanden",{"$nulls":3},"j","M10fein","Stift mit Klinke","Drehverriegelug",null,"Bechergewinde",null,"Blech verchromt",{"$nulls":11},"neuwertig"]
["287/2",null,"Revolver",null,"Neumann Pedersoli","Western Navy 1851","Italien",".380Knall/9mm Knall","6",{"$nulls":3},"19/7,5",{"v":1234,"d":"1,234 g"},"vorn","Stahlsperre",null,null,"Lager und Öffnung versetzt","Zusatzlauf",null,"SA",null,"Hahnrast","Öffnung im Rahmen","manuell","Messing blank",null,"Stahl brüniert","Stahl brüniert","Holz","13076","Mellrichstadt","92","Colt Navy 1851",null,"Originalrevolver umgebaut auf 9mm Knall",null,"neu","Pappschuber mit Styroporeinschub"]
["288/2",null,"Revolver",null,"Neumann Pedersoli","Western Sheriff 1851","Italien",".380Knall/9mm Knall","6",{"$nulls":3},"12,5/5",{"v":1124,"d":"1,124 g"},"vorn","Stahlsperre",null,null,"Lager und Öffnung versetzt","Zusatzlauf",null,"SA",null,"Hahnrast","Öffnung im Rahmen","manuell","Messing blank",null,"Stahl brüniert","Stahl brüniert","Holz","13348","Mellrichstadt","93","Colt Navy 1851",null,"Originalrevolver umgebaut auf 9mm Knall",null,"neu","Pappschuber mit Styroporeinschub"]
["289",null,"Revolver",null,"Neumann Pedersoli","Western Pocket 1849","Italien",".22Knall","6",{"$nulls":3},"15/6",{"v":692,"d":"692 g"},"vorn und oben","Stahlsperre",null,null,"Lager und Öffnung versetzt","n",null,"SA",null,"Hahnrast","Öffnung im Rahmen","manuell","Messing blank",null,"Stahl brüniert","Stahl brüniert","Holz","69767","Mellrichstadt","83","Colt 1849 Pocket, Baby Dragoon",null,"Originalrevolver umgebaut auf 9mm Knall",null,"neu","Pappschuber mit Schaumstoffeinschub"]
["293",null,"Revolver",null,"Em-Ge","39","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":702,"d":"702 g"},"vorn",{"$nulls":4},"Zusatzlauf","M10","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Holz","28916",{"$nulls":4},"sehr massiver 15mm-Zusatzlauf, Gewindeschutz",null,"neu"]
["295",null,"Pistole","Repetierer","Reck","PK 6000","Deutschland","6mm Flobert Platz","6",{"$nulls":4},{"v":394,"d":"394 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Drehflügel","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff schwarz",{"$nulls":3},"Walther TPH",null,"äusserlich Automatikpistole, aber Handrepetierer mit Kastenmagazin",null,"neu"]
["296",null,"Derringer",null,"Umarex","Derringer","Italien","6mm Flobert Platz","2",{"$nulls":4},{"v":365,"d":"365 g"},"vorn","exzentrische Bohrung",{"$nulls":3},"j, integriert","n","SA mit wechselseitig kippenden Schlagstück","keine","Hahnrast","Kipplauf","manuell per Schieber","Druckguss verchromt",null,"Druckguss verchromt",null,"Kunststoff schwarz","024197",{"$nulls":6},"neuwertig"]
["300",null,"Pistole","Automatik","Röhm","RG800","Deutschland","8mm Knall",null,"156","24","115",null,{"v":512,"d":"512 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff braun",null,"Ulm","85","Walther PPK",{"$nulls":3},"gebraucht gut"]
["303",null,"Revolver",null,"Neumann Pedersoli","Rogers & Spencer","Italien",".380Knall/9mm Knall","6",{"$nulls":3},"19/7,5",{"v":1023,"d":"1,023 g"},"vorn","Stahleinsatz im lauf",null,null,"Lager und Öffnung versetzt","n","n","SA",null,"Hahnrast","Öffnung im Rahmen","manuell","Stahl brüniert",null,"Stahl brüniert","Stahl brüniert","Holz","013468",null,null,"Rogers & Spencer",null,"Originalrevolver umgebaut auf 9mm Knall",null,"gebraucht"]
["304",null,"Revolver",null,"Neumann Pedersoli","Remington New Army","Italien",".380Knall/9mm Knall","6",{"$nulls":3},"20/8",{"v":1189,"d":"1,189 g"},"vorn","Stahlsperre",null,null,"Lager und Öffnung versetzt","n","n","SA",null,"Hahnrast","Öffnung im Rahmen","manuell","Messing blank",null,"Stahl brüniert","Stahl brüniert","Holz","12238","Mellrichstadt","92","Remington New Army",null,"Originalrevolver umgebaut auf 9mm Knall",null,"neu","Pappschuber mit Styroporeinschub"]
["308/2",null,"Pistole","Automatik","Umarex","Napoleon","Italien","8mm Knall",{"$nulls":5},{"v":1175,"d":"1,175 g"},"vorn","Platte im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA","keine","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz",{"$nulls":3},"Colt 1911","Me 8 General","Holzgriffschalen geklebt, dadurch Colt-Optik (2Schrauben, Waffe hat normal nur eine Schraube)",null,"gebraucht"]
["311",null,"Signalgerät",null,"Feistel","11010","Deutschland","RD 13/16,5mm","1",{"$nulls":4},{"v":30,"d":"30 g"},"n","kein Lauf vorhanden",{"$nulls":3},"j","M13rund aussen","Stift mit Klinke","Drehverriegelug",null,"Bechergewinde",null,"Kunststoff orange",{"$nulls":11},"neu"]
["313",null,"Pistole","Repetierer","Umarex","302","Italien","6mm Flobert Platz","7",{"$nulls":4},{"v":302,"d":"302 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf",null,"DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss schwarz lackiert","Druckguss schwarz lackiert",null,null,"Kunststoff braun","259570",{"$nulls":6},"neu"]
["315",null,"Revolver",null,"Weihrauch","HW 88 Airweight","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":381,"d":"381 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"verjüngte Bohrung","Zusatzlauf","M10","SA/DA",null,"Hahnrückzug","Schwenktrommel","manueller Ausstosser","Aludruckguss schwarz eloxiert",null,"Aludruckguss schwarz eloxiert","Stahl brüniert","Holz",null,null,"83","SW 66",{"$nulls":3},"gebraucht gut"]
["315",null,"Revolver",null,"Weihrauch","HW 88 Airweight","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":380,"d":"380 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"verjüngte Bohrung","Zusatzlauf","M10","SA/DA",null,"Hahnrückzug","Schwenktrommel","manueller Ausstosser","Aludruckguss mattverchromt",null,"Aludruckguss mattverchromt","Stahl mattverchromt","Holz","1422804","Mellrichstadt","91","SW 66",{"$nulls":3},"neu"]
["316",null,"Derringer",null,"Gun Toys/Umarex","Mini Derringer","Italien","6mm Flobert Platz","1",{"$nulls":4},{"v":175,"d":"175 g"},"vorn","exzentrische Bohrung",{"$nulls":3},"Zusatzlauf",null,"SA","keine","Hahnrast","Kipplauf","manuell per Schieber","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert",null,"Kunststoff weiss","001160",{"$nulls":4},"mit Ringöse",null,"gebraucht"]
["317",null,"Revolver",null,"Umarex","314","Italien","6mm Flobert Platz","7",{"$nulls":4},{"v":362,"d":"362 g"},"vorn","exzentrische Bohrung",null,null,"verjüngte Bohrung","Zusatzlauf",null,"SA/DA",null,null,"Schwenktommel","manueller Ausstosser","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff braun",{"$nulls":7},"gebraucht, Trommeltransport fehlt"]
["318",null,"Revolver",null,"Umarex",".44Magnum","Italien",".380Knall/9mm Knall","6",{"$nulls":3},"20/8",{"v":1045,"d":"1,045 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"exzentrische Bohrung","Zusatzlauf",null,"SA/DA",null,"keine","Schwenktrommel","manueller Ausstosser","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff schwarz",{"$nulls":3},"Colt Python",{"$nulls":3},"gebraucht"]
["319",null,"Revolver",null,"Umarex","343","Italien","6mm Flobert Platz","8",{"$nulls":4},{"v":307,"d":"307 g"},"vorn",{"$nulls":4},"Zusatzlauf",null,"SA/DA",null,null,"Kipplauf","manueller Ausstosser","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff braun","097590",{"$nulls":4},"Ab Werk sehr instabil"]
["319/2",null,"Revolver",null,"Umarex","343","Italien","6mm Flobert Platz","8",{"$nulls":4},{"v":310,"d":"310 g"},"vorn",{"$nulls":4},"Zusatzlauf",null,"SA/DA",null,null,"Kipplauf","manueller Ausstosser","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff braun","305720",{"$nulls":4},"Ab Werk sehr instabil"]
["320",null,"Revolver",null,"Umarex","Army .45","Italien",".380Knall/9mm Knall","6",{"$nulls":3},"12,5/5",{"v":875,"d":"875 g"},"vorn, seitlich","exzentrische Bohrung",null,null,"verjüngte Bohrung","Zusatzlauf","M10","SA",null,null,"Ladeklappe","manueller Ausstosser","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff schwarz","46206","Italien",null,"Colt SAA",{"$nulls":3},"gebraucht gut"]
["322",null,"Revolver",null,"Umarex","Rio 315","Italien",".380Knall/9mm Knall","6","180","39","130","6,5/2,5",{"v":756,"d":"756 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"verjüngte Bohrung","Zusatzlauf","M10fein","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff braun","0731157","Italien",{"$nulls":3},"mit Wechseltrommel .22Knall",null,"gebraucht"]
["322/3",null,"Revolver",null,"Umarex","Champion","Italien",".380Knall/9mm Knall","6","180","39","130","6,5/2,5",{"v":760,"d":"760 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"verjüngte Bohrung","Zusatzlauf","M10fein","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Kunststoff braun","307625",{"$nulls":3},"PTB596",null,null,"gebraucht gut"]
["323",null,"Pistolen-Signalgerät","Repetierer","Em-Ge","EM-GE 64 Stakkato","Deutschland","6mm Flobert Platz","8",{"$nulls":3},"0",{"v":523,"d":"523 g"},"oben","kein Lauf vorhanden","Lager senkrecht",null,null,"j","n","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff rot",{"$nulls":5},"PTB auf gemeinsamen Kastenmagazin für Patronen und Signalpatronen, Griffstück ohne PTB",null,"neu"]
["324",null,"Revolver",null,"Geco","90SA","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"15/6",{"v":908,"d":"908 g"},"vorn","Stahlbolzen",null,null,"Lager und Öffnung versetzt","Zusatzlauf",null,"SA",null,"Hahnrast","Ladeklappe","manueller Ausstosser","Druckguss brüniert",null,"Stahl brüniert","Stahl brüniert","Holz/Druckguss vergoldet","4021","Ulm","84","Colt SAA","ME 900 SAM",null,null,"gebraucht gut"]
["325",null,"Revolver",null,"Reck","Navy","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"18/7",{"v":1022,"d":"1,022 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Hartmetallkern","Zusatzlauf","M10","SA/DA",null,"Hahnrast, TransferBar","Ladeklappe","manuell per Stift","Druckguss vergoldet",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,"Köln","87","Colt 1848 Navy",null,"Entladestift in Ladepressenhebel, Original nur SA",null,"gebraucht, Korrosionsspuren","Pappschachtel, Schaumeinlage"]
["326",null,"Revolver",null,"Mauser/Umarex","L100","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":756,"d":"756 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Hartmetallkern","Zusatzlauf",null,"SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,null,"84",null,null,"ventilierte Laufschiene",null,"neuwertig"]
["327",null,"Pistole","Repetierer","Röhm","RG300","Deutschland","6mm Flobert Platz","10",{"$nulls":5},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf","M8","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss mattvernickelt","Druckguss mattvernickelt",null,null,"Kunststoff braun",{"$nulls":7},"gebraucht"]
["328",null,"Pistole","Automatik","ME","8 General","Italien","8mm Knall",{"$nulls":5},{"v":1062,"d":"1,062 g"},"vorn","2 Stahlbolzen senkrecht im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA",null,null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz",{"$nulls":3},"Colt 1911",null,"altes Modell der ME 800 General","Rahmen ist von der ME 800 General","stark gebraucht","Pappschachtel"]
["329",null,"Revolver",null,"ME","9 Agent","Italien",".380Knall/9mm Knall","5",{"$nulls":4},{"v":676,"d":"676 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M10","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Drcukguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff schwarz","3447",{"$nulls":3},"ME 80 Jaguar",null,null,"neu","Pappschachtel"]
["332",null,"Revolver",null,"HS","Ikarus","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":717,"d":"717 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"verjüngte Bohrung","Zusatzlauf","M12x1","SA/DA",null,"Hahnrückzug","Schwenktrommel","manueller Ausstoßer","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff hell",null,"Mellrichstadt","83",null,"Rahmen ME 380 Police",null,null,"stark gebraucht"]
["333",null,"Pistole","Automatik","HS","G.A.P. Mod.88","Deutschland","8mm Knall",null,"159","24","118","8,3/3,25",{"v":520,"d":"520 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert",null,null,"Holz, verschnitten",null,"Mellrichstadt","83",null,null,"Signalstift","Magazinboden Holz verschnitten","neu"]
["333",null,"Pistole","Automatik","ME","800 P","Deutschland","8mm Knall",null,"159","24","118","8,3/3,25",{"v":527,"d":"527 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M7fein","Schlagbolzenschloss","Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert",null,null,"Holz, verschnitten",null,"Mellrichstadt","85",null,null,"Sicherung im Schlitten","Magazinboden Holz verschnitten","neu"]
["334",null,"Revolver",null,"HS","Mod.45 Army 1873","Deutschland",".45short Knall","6",{"$nulls":3},"19.5/7,5",{"v":1230,"d":"1,230 g"},"vorn",{"$nulls":3},"Hartmetallkern","Zusatzlauf",null,"SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Stahl buntgehärtet",null,"Stahl brüniert","Druckguss brüniert","Holz",null,"Ulm","89","Colt SAA",{"$nulls":3},"neu"]
["335",null,"Pistole","Automatik","Mauser/Umarex","HSc. Mod.84","Deutschland","8mm Knall","7","157","28","117",null,{"v":543,"d":"543 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss vergoldet","Druckguss brüniert",null,"Holz","373","Köln","84","Mauser HSC","Reck PK800 und Perfecta \"El Alamein\" PTB196ff",null,null,"neuwertig"]
["335/2",null,"Pistole","Automatik","Mauser/Umarex","HSc. Mod.84","Deutschland","8mm Knall","7","157","28","117",null,{"v":537,"d":"537 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz","0132215","Köln","94","Mauser HSC","Reck PK800 und Perfecta \"El Alamein\" PTB196ff",null,null,"gebraucht","Kunststoffkoffer"]
["336",null,"Revolver",null,"Umarex","Space Raker Mod.201","Deutschland",".22Knall","6",{"$nulls":3},"15/6",{"v":618,"d":"618 g"},"vorn","verjüngte Bohrung",null,null,"Lager und Öffnung versetzt","Zusatzlauf",null,"SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Stahl brüniert","Druckguss brüniert","Kunststoff schwarz",null,null,"83",null,"PTB166, PTB193",null,"Anschussmöglichkeit für Modellraketen (nicht mehr vorhanden)","neu","Pappschachtel, Schaumeinlage"]
["340",null,"Revolver",null,"HS","Mod. 45 Frontier","Deutschland",".45short Knall","6",{"$nulls":3},"13,5/5,5",{"v":1059,"d":"1,059 g"},"vorn",{"$nulls":3},"Hartmetallkern","j, integriert","n","SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Druckguss brüniert",{"$nulls":3},"Holz",null,"Ulm","89","Colt SAA",{"$nulls":3},"gebraucht"]
["341",null,"Revolver",null,"Röhm","RG79","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"6/2,5",{"v":672,"d":"672 g"},"vorn","schräger Stahlbolzen im Laufdach",null,null,"Hartmetallkern","Zusatzlauf","M10","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,"Ulm","84",{"$nulls":4},"stark gebraucht"]
["341",null,"Revolver",null,"Röhm","RG79","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":671,"d":"671 g"},"vorn","schräger Stahlbolzen im Laufdach",null,null,"Hartmetallkern","Zusatzlauf","M10","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,"Ulm","87",{"$nulls":4},"gebraucht"]
["342",null,"Revolver",null,"Röhm","RG 77","Deutschland",".22Knall","6",{"$nulls":4},{"v":420,"d":"420 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M8","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,null,"85",{"$nulls":4},"gebraucht gut","Pappschachtel"]
["343",null,"Signalgerät",null,"Nico","Nicosignal","Deutschland","6/16x45","6",{"$nulls":4},{"v":93,"d":"93 g"},"n",{"$nulls":4},"j",null,"DA-Repetiersystem","Schieber","Schlagstück nicht an Patrone",null,null,"Kunststoff orange",null,null,"Kunststoff weiss",{"$nulls":8},"gebraucht"]
["345",null,"Revolver",null,"HS","45 Bulldog","Deutschland",".45short Knall","5",{"$nulls":4},{"v":736,"d":"736 g"},"vorn","Hartmetallsperre",null,null,"Hartmetallkern","Zusatzlauf","M10","SA/DA",null,"Hahnrückzug","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Stahl brüniert","Druckguss brüniert","Holz","1136559",null,"84",null,"Arminius HW 10GR PTB218",null,null,"neu","Pappschachtel"]
["346",null,"Pistole","Automatik","FN Browning/Umarex","GPDA 8","Deutschland","8mm Knall",null,"200","38","131","12/4,75",{"v":730,"d":"730 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M7feim","SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,null,"87","Browning Hi-Power",null,null,"auch als GPDA 9 in 9mm P.A.Knall erhältlich","gebraucht gut","Pappschachtel mit Schaumeinlage"]
["348",null,"Pistole","Repetierer","Röhm","RG600","Deutschland",".22Knall","10",{"$nulls":4},{"v":475,"d":"475 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"Zusatzlauf",null,"DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Kunststoff braun",null,null,"92",null,"Griffstück baugleich mit Röhm RG300",null,null,"gebraucht","Pappschachtel, Schaumeinlage"]
["349",null,"Revolver",null,"Röhm","Little Joe","Deutschland","6mm Flobert Platz","5",{"$nulls":4},{"v":131,"d":"131 g"},"vorn","Stahlbolzen seitlich im Lauf",null,null,"Hartmetallkern","Zusatzlauf",null,"SA",null,null,"Schwenktrommel","manuell per Stift","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",{"$nulls":7},"neuwertig","Pappschachtel, Schaumeinlage"]
["352",null,"Pistole","Automatik","Geco","Mod.1910","Deutschland","8mm Knall",null,"154","29","101",null,{"v":499,"d":"499 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M7fein","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff schwarz",null,"Mellrichstadt","84","FN 1910","PTB 386,387, 619, 12","Signalstift für Schlagbolzen",null,"neu","Pappschachtel"]
["354",null,"Revolver",null,"Röhm","RG99","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":763,"d":"763 g"},"vorn","Stahlbolzen schräg im Laufdach",null,null,"verjüngte Bohrung","Zusatzlauf","M10","SA/DA",null,"Transferbar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz braun",null,"Ulm","87",{"$nulls":4},"gebraucht"]
["365",null,"Revolver",null,"Röhm","Hubertus","Deutschland",".380Knall/9mm Knall","6","183","37","112","6,3/2,5","663/691","vorn",{"$nulls":4},"Zusatzlauf","M9","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert",null,"Kunststoff braun",null,"Ulm","84",{"$nulls":3},"Wechseltrommel .22Knall","gebraucht gut"]
["368",null,"Signalgerät",null,"Reimer","Komet150-S","Deutschland","M9/15","1",{"$nulls":4},{"v":21,"d":"21 g"},"n","Kein Lauf vorhanden",{"$nulls":3},"j","M9*1",null,null,"Rast","Verschraubung",null,"Kunststoff orange",{"$nulls":11},"neuwertig"]
["372",null,"Revolver",null,"ME","ME 453 ","Deutschland",".45short Knall","5",{"$nulls":3},"7,5/3",{"v":820,"d":"820 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"verjüngte Bohrung","Zusatzlauf","M10","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,null,"86",null,"Rahmen baugleich mit ME Revolvergewehr, PTB374",null,null,"gebraucht gut"]
["372",null,"Revolver",null,"ME","ME 454 Sergeant","Deutschland",".45short Knall","5",{"$nulls":3},"10/4","864g","vorn","Hartmetallplatte längs im Lauf",null,null,"verjüngte Bohrung","Zusatzlauf","M10","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff elfenbein",null,"Ulm","90",null,"Rahmen baugleich mit ME Revolvergewehr, PTB374",null,null,"neuwertig","Pappschachtel"]
["372",null,"Revolver",null,"ME","ME 45 Officer","Deutschland",".45short Knall","5",{"$nulls":3},"6/2,5",{"v":781,"d":"781 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"verjüngte Bohrung","Zusatzlauf","M10","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz","010067",null,"93",null,"Rahmen baugleich mit ME Revolvergewehr, PTB374",null,null,"neu"]
["372",null,"Revolver",null,"ME","ME 45 Officer","Deutschland",".45short Knall","5",{"$nulls":3},"6/2,5",{"v":779,"d":"779 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"verjüngte Bohrung","Zusatzlauf","M10","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss mattverchromt",null,"Druckguss mattverchromt","Druckguss mattverchromt","Holz",null,null,"94",null,"Rahmen baugleich mit ME Revolvergewehr, PTB374",null,null,"neu"]
["374",null,"Revolvergewehr",null,"ME","ME MARSHALL MOD. 1887","Deutschland",".45short Knall","5",{"$nulls":5},"vorn","ehemals Metallstift, wurde nur durch Vorderschaft gehalten","dünne, lose Stahlstange",null,null,"Zusatzlauf",null,"SA/DA","keine",null,"Schwenktrommel","manuell per Ausstosser","Druckguss brüniert",null,"Stahl brüniert","Stahl brüniert","Holz",null,null,"85",null,"Rahmen baugleich mit ME 45 Officer, PTB372",null,"Langwaffe ","neu","Pappschachtel"]
["380",null,"Revolver",null,"Röhm","Little Joe","Deutschland",".22Knall","5",{"$nulls":4},{"v":136,"d":"136 g"},"vorn","Stahlbolzen seitlich im Lauf",null,null,"Hartmetallkern","Zusatzlauf","M8","SA",null,null,"Schwenktrommel","manuell per Stift","Druckguss vergoldet",null,"Druckguss vergoldet","Druckguss vergoldet","Kunststoff braun",{"$nulls":3},"NAA ",null,null,"Sondermodell, Auflage 2000 Stück","neuwertig","Pappschachtel, Schaumeinlage"]
["385",null,"Pistole","Automatik","ME","ME 8 Police","Italien","8mm Knall",null,"152","28","114",null,{"v":664,"d":"664 g"},"vorn","Verschraubung,","Seitenrippen innen im Lauf",null,null,"Zusatzlauf",null,"SA","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","031032","Köln","90","Walther PPK",null,"Sicherungshebel an anderer Stelle als beim Original",null,"gebraucht, stark abgegriffen"]
["386",null,"Pistole","Automatik","Geco","Mod.Ultra","Deutschland","8mm Knall",null,"135","23","101",null,{"v":516,"d":"516 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Metall, florales Dekor",null,"Köln","91",null,"PTB 387, 619, 421, 12",null,null,"neu","Pappschachtel"]
["387",null,"Pistole","Automatik","Reck","Protector Automatik","Deutschland","8mm Knall",null,"134","23 (25)","101",null,{"v":417,"d":"417 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Schubknopf","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,"Köln","88",null,"PTB 386, 619, 421, 12",null,null,"gebraucht, teilweise Schäden in Brünierung"]
["387/2",null,"Pistole","Automatik","Perfecta","FBI8000","Deutschland","8mm Knall",null,"134","23 (25)","101",null,{"v":406,"d":"406 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Schubknopf","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","G028952","Köln","94",null,"PTB 386, 619, 421, 12","Alte Version, schlanker Abzugsbügel, runder Schlitten",null,"neuwertig"]
["387/2",null,"Pistole","Automatik","Perfecta","FBI8000","Deutschland","8mm Knall",null,"134","23 (25)","101",null,{"v":433,"d":"433 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Schubknopf","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","X01194","Köln","94",null,"PTB 386, 619, 421, 12","Neue Version, dicker Azugsbügel, kantiger Schlitten",null,"neu"]
["388",null,"Pistole","Automatik","Reck","P6","Deutschland","8mm Knall",null,"115","22","100",null,{"v":369,"d":"369 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,"Köln","90","früher auch als 6.35er Browning erhältlich, Reck P8",{"$nulls":3},"neuwertig"]
["388/2",null,"Pistole","Automatik","Reck","P6","Deutschland","8mm Knall",null,"115","22","100",null,{"v":369,"d":"369 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,"Köln","9x","früher auch als 6.35er Browning erhältlich, Reck P8",{"$nulls":3},"neuwertig","Kunststoffkoffer, Schaumeinlage"]
["389",null,"Pistole","Automatik","FN Browning/Umarex","GPDA 8","Deutschland","8mm Knall",null,"200","38","131","12/4,75",{"v":786,"d":"786 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M7fein","SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,"Köln","92","Browning Hi-Power",null,null,"auch als GPDA 9 in 9mm P.A.Knall erhältlich","neuwertig"]
["389/2",null,"Pistole","Automatik","FN Browning/Umarex","GPDA 8","Deutschland","8mm Knall",null,"200","38","131","12/4,75",{"v":755,"d":"755 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M7fein","SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,"Köln","92","Browning Hi-Power",null,null,"auch als GPDA 9 in 9mm P.A.Knall erhältlich","neuwertig"]
["389/2",null,"Pistole","Automatik","FN Browning/Umarex","GPDA 8","Deutschland","8mm Knall",null,"200","38","131","12/4,75",{"v":806,"d":"806 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M7fein","SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss verchromt","Druckguss verchromt","Druckguss brüniert",null,"Kunststoff schwarz","B132879","Köln","94","Browning Hi-Power",null,null,"auch als GPDA 9 in 9mm P.A.Knall erhältlich","gebraucht gut"]
["391",null,"Pistole","Automatik","Reck","Special Marines","Deutschland","8mm Knall","7","115 (230/296)","34","117 (127)",null,{"v":531,"d":"531 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10fein","SA/DA","Schlagbolzen","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz",null,"Köln","85","Walther PPK","Reck PK800 PTB196 / Mauser Hsc84 PTB335ff","Sondermodell, Abschussbecher mit Klappbajonett",null,"gebraucht sehr gut","Pappschachtel mit Schaumeinlage"]
["398",null,"Pistole","Automatik","Erma","EGP 45","Deutschland","8mm Knall",null,"157","28","114","8/3,25",{"v":584,"d":"584 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl poliert",null,"Kunststoff schwarz","023093","München","94","Colt Commander",null,null,"Massstab kleiner als Original","neu"]
["398",null,"Pistole","Automatik","IWC","Officer","Deutschland","8mm Knall",null,"157","28","114","8/3,25",{"v":585,"d":"585 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss verchromt","Druckguss verchromt","Stahl verchromt",null,"Kunststoff schwarz","22354","München","93","Colt Commander",null,null,"Massstab kleiner als Original","neu"]
["399",null,"Pistole","Automatik","Erma","EGP 55","Deutschland","8mm Knall",null,"136","23 (25)","100",null,{"v":413,"d":"413 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl poliert",null,"Kunststoff schwarz","030733","München","86","Walther TPH",null,null,"gilt als beste Kopie der Walther TPH","neuwertig"]
["400",null,"Pistole","Automatik","Erma","EGP 65","Deutschland","8mm Knall",null,"137","23","97",null,{"v":405,"d":"405 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M8","SA","keine","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","046010","München","92",{"$nulls":4},"neu","Pappschachtel, Styroporeinlage"]
["401",null,"Pistole","Automatik","Erma","EGP 75","Deutschland","8mm Knall",null,"157","25 (27)","115",null,{"v":564,"d":"564 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Steahl blank",null,"Kunststoff schwarz","108872","München","92","Walther PPK",{"$nulls":3},"neu","Pappschactel, Styroporeinlage"]
["402",null,"Pistole","Automatik","Erma","KGP 690","Deutschland","8mm Knall","6","187","32","126","9/3,5",{"v":772,"d":"772 g"},"vorn","Hartmetallplatte längs im Lauf","Lager und Öffnung versetzt",null,null,"Zusatzlauf","M8","Schlagbolzenschloss","Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss  mattvernickelt","Druckguss mattvernickelt","Druckguss mattvernickelt",null,"Holz","012952","München","97","Luger P 08",null,null,"Massstab kleiner als Original, keine genaue Kopie","neu"]
["407",null,"Pistole","Automatik","Mauser/Umarex","WTP","Deutschland","8mm Knall",null,"120","22","96","6,3/2,5",{"v":370,"d":"370 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA","Abzug, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",{"$nulls":3},"Tanfoglio PT27/PT28",null,"Sicherung und Zerlegehebel in einem",null,"neu","Pappschachtel, Schaumeinlage"]
["410",null,"Revolver",null,"Geco","900 G","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":691,"d":"691 g"},"vorn","Stahlkern mit rechteckiger Fräsung",null,null,"Bohrungen zwischen Öffnungen","Zusatzlauf",null,"SA/DA",null,"Hahnrast","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Kunststoff braun","1186773",null,"91",null,"Arminius HW 10GR PTB218",null,null,"neu","Pappschachtel, Styroporeinschub"]
["412",null,"Pistole","Automatik","Röhm","RG8","Deutschland","8mm Knall",null,"135","23","96",null,{"v":435,"d":"435 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Abzug, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun",{"$nulls":7},"neuwertig, aber Lagerspuren"]
["413",null,"Pistole","Automatik","Röhm","RG9","Deutschland","8mm Knall",null,"144","24","98",null,{"v":431,"d":"431 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M8","SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff braun",null,"Ulm","93","Walther TPH","Röhm RG90",null,null,"gebraucht"]
["413",null,"Pistole","Automatik","IWC","TP","Deutschland","8mm Knall",null,"144","25","98",null,{"v":431,"d":"431 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M8","SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Holz",null,"Ulm","94","Walther TPH","Röhm RG90",null,null,"neuwertig"]
["414",null,"Pistole","Automatik","Röhm","RG800","Deutschland","8mm Knall",null,"156","24","115",null,{"v":502,"d":"502 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff braun",null,"Ulm","93","Walther PPK",{"$nulls":3},"neuwertig"]
["414",null,"Pistole","Automatik","Röhm","RG800","Deutschland","8mm Knall",null,"156","24","115",null,{"v":515,"d":"515 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss Messing-Antik","Druckguss Messing-Antik","Stahl Messing-Antik",null,"Holz",null,null,"93","Walther PPK",null,null,"Sondermodell","gebraucht"]
["419",null,"Revolver",null,"ME-Import","Ranger","Italien",".380Knall/9mm Knall","6",{"$nulls":3},"14/5,25",{"v":968,"d":"968 g"},"vorn",{"$nulls":3},"Hartmetallkern","Zusatzlauf",null,"SA",null,null,"Ladeklappe","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz","16282","Italien",null,"Colt SAA",null,"Waffe wurde durch Hersteller überarbeitet, daher wieder neuwertig",null,"neu"]
["420",null,"Revolver",null,null,"Remington Pocket","Deutschland","VL-Zündhütchen","5",{"$nulls":3},"9/3,5",{"v":414,"d":"414 g"},"seitlich",{"$nulls":3},"Bohrung zur Trommelachse aufgefräst","n","n","SA",null,"Hahnrast",null,null,"Messing blank",null,"Stahl brüniert","Stahl brüniert","Holz",{"$nulls":3},"Remington Pocket Cal..31",null,"ehemals Vorderladerwaffe",null,"neuwertig"]
["421",null,"Pistole","Automatik","Geco","Mod.1910","Deutschland","8mm Knall",null,"154","29","101",null,{"v":496,"d":"496 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff schwarz",null,"Ulm","89","FN 1910","PTB 386,387, 619, 12","Signalstift für Schlagbolzen",null,"neuwertig","Pappschachtel"]
["425",null,"Signalgerät",null,"Mauser/Umarex","SG","Deutschland","R1/8-9mm","1",{"$nulls":3},"0/0","xx","n","kein Lauf vorhanden",{"$nulls":3},"j",null,"Stift mit Klinke",null,"keine","Bechergewinde",null,"Kunststoff schwarz",{"$nulls":10},"Signalgerät ist in Messerscheide integriert, entnehmbar","neuwertig"]
["428",null,"Pistole","Automatik","Walther/Umarex","P88 Compact/P88-8","Deutschland","8mm Knall",null,"182","34","139","10/4",{"v":959,"d":"959 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert",{"$nulls":3},"Kunststoff schwarz",{"$nulls":3},"Walther P88 Compact",null,null,"auch als P88-9 in 9mm P.A.Knall erhältlich","neuwertig"]
["430",null,"Revolver",null,"Geco","722 G","Deutschland",".22Knall","6",{"$nulls":4},{"v":427,"d":"427 g"},"vorn","exzentrische Bohrung",null,null,"Hartmetallkern","Zusatzlauf",null,"SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,null,"87",{"$nulls":4},"neuwertig","Pappschachtel"]
["437",null,"Pistole","Automatik","ME","ME 8 General","Italien","8mm Knall",{"$nulls":5},{"v":1165,"d":"1,165 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA","keine","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz",{"$nulls":3},"Colt 1911",null,"keine Sicherung, Schlittenfang nur manuell zu bedienen, \"nicht zerlegbar\"",null,"stark gebraucht"]
["437",null,"Pistole","Automatik","ME","ME 800 General","Italien","8mm Knall",{"$nulls":5},{"v":1082,"d":"1,082 g"},"vorn","Hartmetallplatte längs im Lauf","Verschraubung",null,null,"Zusatzlauf","M10","SA","keine","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz","53621","Köln","91","Colt 1911",null,"keine Sicherung, Schlittenfang nur manuell zu bedienen, \"nicht zerlegbar\"",null,"stark gebraucht"]
["438",null,"Revolver",null,"ME","Magnum","Italien",".380Knall/9mm Knall","6",{"$nulls":4},{"v":869,"d":"869 g"},"vorn, seitlich","Hartmetallplatte längs im Lauf",null,null,"Hartmetallkern","Zusatzlauf","M10","SA/DA",null,"keine","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff schwarz","69533",null,"91","Colt Python",null,null,"ab Werk nachträgliche Einfräsung an Laufwurzel, Nachträglich mit \"neu 538\" PTB-gestempelt","neu"]
["440",null,"Signalgerät",null,"Mauser/Umarex","SG","Deutschland","R1/8-9mm","1",{"$nulls":3},"0/0","xx","n","kein Lauf vorhanden",{"$nulls":3},"j",null,"Stift mit Klinke",null,"keine","Bechergewinde",null,"Kunststoff schwarz",{"$nulls":10},"Signalgerät ist in Messerscheide integriert, nicht entnehmbar","neuwertig"]
["444",null,"Revolver",null,"Em-Ge","42","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":720,"d":"720 g"},"vorn","schräger Stahlbolzen im Laufdach",null,null,"verjüngte Bohrung","j","M10","SA/DA",null,null,"Schwenktommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Holz",null,null,"92",{"$nulls":4},"neuwertig","Pappschachtel"]
["448",null,"Pistole","Automatik","ME","Combat Eagle","Italien","8mm Knall",null,"266","37 (39)","152","16/6,35",{"v":2029,"d":"2,029 g"},"vorn",{"$nulls":4},"Zusatzlauf","M10","SA","keine","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz","002270","Italien",null,"IMI Desert Eagle","technisch identisch mit ME 38 P","keine Sicherung, Schlittenfang nur manuell zu bedienen, \"nicht zerlegbar\"",null,"gebraucht"]
["448",null,"Pistole","Automatik","ME","Combat Eagle","Italien","8mm Knall",null,"226","37 (39)","152","16/6,25",{"v":2025,"d":"2,025 g"},"vorn",{"$nulls":4},"Zusatzlauf","M10","SA","keine","keine","Magazin","automatischer Auswurf","Druckguss poliert","Druckguss poliert","Druckguss poliert",null,"Holz",{"$nulls":3},"IMI Desert Eagle","technisch identisch mit ME 38 P","keine Sicherung, Schlittenfang nur manuell zu bedienen, \"nicht zerlegbar\"",null,"gebraucht"]
["450",null,"Revolver",null,"SM","2000","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"7/2,75",{"v":709,"d":"709 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",{"$nulls":5},"langer Lauf",null,"neu","Pappschachtel"]
["450",null,"Revolver",null,"SM","2000","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"10/4",{"v":772,"d":"772 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",{"$nulls":5},"kurzer Lauf",null,"neu","Pappschachtel"]
["451",null,"Revolver",null,"Röhm","RG 89","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":633,"d":"633 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"Hartmetallkern","Zusatzlauf","M10","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,"Ulm","92",null,"Röhm RG69, Kora 007",null,null,"gebraucht gut","Pappschachtel"]
["452",null,"Revolver",null,"Röhm","RG99","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"10/4",{"v":755,"d":"755 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"Hartmetallkern","Zusatzlauf","M10","SA/DA",null,"Transferbar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz","0378335","Ulm","2000",{"$nulls":4},"neuwertig","Pappschachtel"]
["453",null,"Revolver",null,"Reck","Bodyguard","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"6,35/2,5",{"v":609,"d":"609 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",{"$nulls":4},"Geco 390G, PTB228",null,null,"gebraucht"]
["456",null,"Pistole","Automatik","Geco","P35","Deutschland",".35Knall",null,"177","30","135","10/4",{"v":982,"d":"982 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA","keine","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff schwarz",null,null,"91","SigSauer P225",null,"Laufblock und Griffstück nur verstiftet",null,"neuwertig","Pappschachtel, Schaumeinlage"]
["456",null,"Pistole","Automatik","Geco","P35","Deutschland",".35Knall",null,"177","30","135","10/4",{"v":980,"d":"980 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA","keine","Hahnrast","Magazin","automatischer Auswurf","Druckguss hochglanzbrüniert","Druckguss hochglanzbrüniert","Stahl",null,"Kunststoff schwarz",{"$nulls":3},"SigSauer P225",null,"Laufblock und Griffstück nur verstiftet",null,"neuwertig","Pappschachtel, Schaumeinlage"]
["457",null,"Revolver",null,"Mauser/Umarex","Magnum","Deutschland",".45short Knall","5",{"$nulls":4},{"v":800,"d":"800 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA",null,null,"Kipplauf mit 2facher Verriegelung","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,null,"94",{"$nulls":4},"neu"]
["458",null,"Revolver",null,"Röhm","RG 69","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":715,"d":"715 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"exzentrische Bohrung","Zusatzlauf","M10","SA/DA",null,"Hahnrückzug","Schwenktrommel","manueller Ausstosser","Druckguss ehem. brüniert",null,"Druckguss ehem. brüniert","Stahl ehem. Brüniert","Holz",null,"Ulm","88",{"$nulls":4},"stark gebraucht, geschliffen, Brünierung stark beschädigt"]
["458",null,"Revolver",null,"Röhm","RG 69","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":726,"d":"726 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"exzentrische Bohrung","Zusatzlauf","M10","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss mattvernickelt",null,"Druckguss mattvernickelt","Stahl mattvernickelt","Holz",null,"Ulm","94",{"$nulls":4},"neuwertig"]
["459",null,"Pistole","Repetierer","Em-Ge","65","Deutschland",".22Knall","10",{"$nulls":3},"9,5/3,75",{"v":828,"d":"828 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"j,  integriert","n","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Holz",{"$nulls":5},"Laufblock abnehmbar, zur Verwendung mit Em-Ge Stakkato PTB323","PTB nur auf Laufblock, kurze -Version","neuwertig","Pappschachtel, Schaumeinlage"]
["459",null,"Pistole","Repetierer","Em-Ge","65","Deutschland",".22Knall","10",{"$nulls":3},"16/6,75",{"v":828,"d":"828 g"},"vorn",null,"Lager rechtwinklig zum Lauf",null,null,"j,  integriert","n","DA-Repetiersystem","Abzug, Schubknopf","Schlagstück nicht an Patrone","Kastenmagazin","Magazin manuell per Stift","Druckguss brüniert","Druckguss brüniert",null,null,"Holz",{"$nulls":5},"Laufblock abnehmbar, zur Verwendung mit Em-Ge Stakkato PTB323","PTB nur auf Laufblock, lange Version","neuwertig","Pappschachtel, Schaumeinlage"]
["464",null,"Pistole","Automatik","Beretta/Nuova Molgora","84","Italien","8mm Knall",null,"170","34","121","9,5/3,75",{"v":795,"d":"795 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,null," ","Beretta 84","Beretta 84","Lauf ist demontierbar",null,"gebraucht","Kunststoffkoffer"]
["467",null,"Pistole","Automatik","Weihrauch","HW 94","Deutschland",".380Knall/9mm Knall",{"$nulls":5},{"v":805,"d":"805 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun","001066","Mellrichstadt","89","Beretta",null,"verschiesst Revolvermunition",null,"neuwertig"]
["467",null,"Pistole","Automatik","Weihrauch","HW 94","Deutschland",".380Knall/9mm Knall",{"$nulls":5},{"v":807,"d":"807 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss vergoldet","Druckguss brüniert","Druckguss vergoldet",null,"Kunststoff schwarz","W0035",null,null,"Beretta",null,"verschiesst Revolvermunition","Sondermodell \"Für ein liberales Waffenrecht\"","neuwertig","Kunststoffkoffer, Schaumeinlage"]
["474",null,"Pistole","Automatik","SM","151A","Deutschland","8mm Knall",null,"116","23","98",null,{"v":388,"d":"388 g"},"oben","Hartmetallplatte längs im Lauf",{"$nulls":3},"n",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,"Mellrichstadt","93",{"$nulls":4},"neu","Pappschachtel"]
["475",null,"Pistole","Automatik","BBM/ME","ME 38 P","Italien","8mm Knall",null,"215","35","139","13/5",{"v":1061,"d":"1,061 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA","Abzug, Hebel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","02867","Köln","91","Walther P 38",null,"kein Spannabzug wie das Original",null,"stark gebraucht"]
["475",null,"Pistole","Automatik","BBM/ME","ME 38 P","Italien","8mm Knall",null,"215","35","139","13/5",{"v":1060,"d":"1,060 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA","Abzug, Hebel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","028613","Köln","91","Walther P 38",null,"kein Spannabzug wie das Original",null,"gebraucht sehr gut"]
["476",null,"Pistole","Automatik","Erma","EGP88","Deutschland","8mm Knall",null,"202","29 (34)","125","12,5/5",{"v":755,"d":"755 g"},"vorn",{"$nulls":4},"Zusatzlauf",null,"SA/DA",null,null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,null,"08693","München","94","Walther P38",{"$nulls":3},"gebraucht"]
["477",null,"Pistole","Automatik","Erma","EGP 88","Deutschland",".35Knall",null,"202","29 (34)","125","12,5/5",{"v":726,"d":"726 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","02877","München","88","Walther P 38",{"$nulls":3},"gebraucht"]
["478",null,"Pistole","Automatik","Brixia/ME","AP92","Italien","8mm Knall","18",{"$nulls":4},{"v":922,"d":"922 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel","kurzer Schlagbolzen","Magazin","automatischer Auswurf","Druckguss schwarz lackiert","Druckguss schwarz lackiert","Druckguss schwarz lackiert",null,"Kunststoff schwarz","A05183B",null,null,"Beretta 92 Army",{"$nulls":3},"gebraucht, Schlittenseiten blank","Pappschachtel, Plastikeinlage"]
["478",null,"Pistole","Automatik","Brixia/ME","AP92","Italien","8mm Knall","18",{"$nulls":4},{"v":897,"d":"897 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel","kurzer Schlagbolzen","Magazin","automatischer Auswurf","Druckguss schwarz lackiert","Druckguss schwarz lackiert","Druckguss schwarz lackiert",null,"Kunststoff schwarz",null,null,"88","Beretta 92 Army",{"$nulls":3},"gebraucht gut"]
["479",null,"Pistole","Automatik","ME","Mini Para","Deutschland","9mm P.A.Knall",null,"175","35","139","10/4",{"v":958,"d":"958 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA","Schlagbolzen/Drehflügel","kurzer Schlagbolzen","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff schwarz",null,null,"91",{"$nulls":4},"gebraucht, Federführung nicht komplett/defekt"]
["479",null,"Pistole","Automatik","ME","Mini Para","Deutschland","9mm P.A.Knall",null,"175","35","139","10/4",{"v":971,"d":"971 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA","Schlagbolzen/Drehflügel","kurzer Schlagbolzen","Magazin","automatischer Auswurf","Druckguss mattvernickelt","Druckguss mattvernickelt","Stahl mattvernickelt",null,"Kunststoff schwarz",null,"Ulm","94",{"$nulls":4},"gebraucht gut"]
["480",null,"Pistole","Automatik","FB Rekord","Rekord 08","Deutschland","8mm Knall","6","219","36","138","10,5/4,25",{"v":875,"d":"875 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M8","Schlagbolzenschloss","Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz",null,"Ulm","90","Luger P08","IWG Lange 08 PTB701","Kniegelenk ohne echte Funktion",null,"gebraucht","Holzkiste, Schaumeinlage"]
["481",null,"Pistole","Automatik","Reck","Miami Mod.92","Deutschland","8mm Knall","18",{"$nulls":4},"xx","vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M8","SA/DA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",{"$nulls":4},"90","Beretta 92",{"$nulls":3},"stark gebraucht, fehlende Kleinteile"]
["481/2",null,"Pistole","Automatik","Reck","Miami Mod.92","Deutschland","8mm Knall","18",{"$nulls":4},{"v":1137,"d":"1,137 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M8","SA/DA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","003 v. 150","Köln","92","Beretta 92",{"$nulls":3},"neuwertig","Lederkoffer mit Filzeinlage"]
["482",null,"Pistole","Automatik","Röhm","735","Deutschland",".35Knall","8","197","30 (34)","130","10,5/4,2",{"v":820,"d":"820 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff braun",null,null,"90",null,"Identisch mit RG725, nur längeres Patronenlager",null,null,"gebraucht gut","Pappschachtel"]
["486",null,"Revolver",null,"Umarex","UMA-Lady","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"5/2",{"v":573,"d":"573 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M10fein","SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,null,"91",null,"PTB 216",null,null,"gebraucht gut","Kunststoffkoffer"]
["486",null,"Revolver",null,"Umarex","UMA-Lady","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"5/2",{"v":591,"d":"591 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Hartmetallkern","Zusatzlauf","M10fein","SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Druckguss verchromt",null,"Druckguss verchromt","Druckguss verchromt","Holz",null,null,"90",null,"PTB 216",null,null,"neuwertig"]
["486",null,"Revolver",null,"Umarex","UMA-Lady","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"5/2",{"v":572,"d":"572 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Hartmetallkern","Zusatzlauf","M10fein","SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,null,"90",null,"PTB216",null,null,"gebraucht"]
["487",null,"Revolver",null,"Reck","R45 Magnum","Deutschland",".45short Knall","6",{"$nulls":3},"15/6",{"v":921,"d":"921 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA","Hahnrast","Hahnrast","Ladeklappe","manuell per Ausstosser","Druckguss verchromt",null,"Druckguss verchromt","Druckguss verchromt","Holz",null,"Köln","88",{"$nulls":4},"neuwertig, Rastnase am Abzug abgebrochen"]
["488",null,"Pistole","Automatik","Reck","Miami Mod.92F","Deutschland","9mm P.A.Knall","12",{"$nulls":4},"xx","vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M8?","SA/DA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",{"$nulls":5},"Beretta 92",{"$nulls":3},"stark gebraucht, Bodenfund, fehlende Kleinteile"]
["488/2",null,"Pistole","Automatik","Reck","Miami Mod.92F","Deutschland","9mm P.A.Knall","12",{"$nulls":4},{"v":1135,"d":"1,135 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M8","SA/DA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz","L057722","Köln","94","Beretta 92"]
["489/2",null,"Pistole","Automatik","Umarex","Brigadier Mod. 95","Italien","8mm Knall",{"$nulls":5},{"v":1109,"d":"1,109 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M7fein","SA",null,null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","025658",null,null,"Beretta 95","PTB 493, entfernt auch ME 8 General",null,null,"gebraucht"]
["490",null,"Derringer",null,"Pedersoli/Neumann","Las Vegas","Italien",".22Knall","1",{"$nulls":3},"6/2,5",{"v":226,"d":"226 g"},"vorn","geschlitzter Stahleinsatz im Lauf",{"$nulls":3},"n","n","SA","keine","Hahnrast","Drehlauf",null,"Messing blank",null,"Messing blank",null,"Holz",{"$nulls":5},"ehemals Vorderladerwaffe",null,"gebraucht"]
["493",null,"Pistole","Automatik","Umarex","Brigadier Mod. 95","Italien","8mm Knall",{"$nulls":5},{"v":1111,"d":"1,111 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA",null,null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,null,"90","Beretta 95","Umarex Brigadier 95, entfernt auch ME 8 General",null,null,"gebraucht"]
["493/2",null,"Pistole","Automatik","Umarex","Brigadier Mod. 96","Italien","9mm P.A.Knall",{"$nulls":5},{"v":1110,"d":"1,110 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA",null,null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","095654",null,null,"Beretta 95","Umarex Brigadier 95, entfernt auch ME 8 General",null,null,"gebraucht"]
["494",null,"Pistole","Automatik","Reck","Miami Mod.93","Deutschland","8mm Knall","25",{"$nulls":4},{"v":1275,"d":"1,275 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","C069774",null,"94","Beretta MP",null,"anschraubbarer Zusatzgriff und Laufverlängerung",null,"gebraucht"]
["496",null,"Pistole","Automatik","SM","Action","Deutschland","9mm P.A.Knall",null,"153","27","119","8,5/3,25",{"v":616,"d":"616 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss",null,null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz",null,"München","93",{"$nulls":4},"neu","Pappschachtel"]
["497",null,"Pistole","Automatik","Geco","P35-2","Deutschland",".35Knall",null,"175","32","134","10/4",{"v":933,"d":"933 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA","keine","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff schwarz",{"$nulls":3},"Heckler+Koch P5",{"$nulls":3},"neuwertig","Pappschachtel"]
["497",null,"Pistole","Automatik","Geco","P35-2","Deutschland",".35Knall",null,"175","32","134","10/4",{"v":933,"d":"933 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA","keine","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff schwarz",{"$nulls":3},"Heckler+Koch P5",{"$nulls":3},"neuwertig","Pappschachtel"]
["501",null,"Revolver",null,"Reck","Agent","Deutschland",".45short Knall","5",{"$nulls":3},"6,35/2,5",{"v":681,"d":"681 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff schwarz",null,null,"94",null,"S&W Combat Magnum, PTB617",null,null,"neu"]
["502",null,"Pistole","Automatik","Walther/Umarex","PPK","Deutschland","8mm Knall","7","155","25","117",null,{"v":552,"d":"552 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M7fein","SA/DA","Schlagbolzen/Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","6380704","Köln","94","Walther PPK","Reck PK800 PTB196ff / Mauser Hsc84 PTB335ff",null,"Überlanges Magazin","neu","Kunststoffkoffer"]
["503",null,"Revolver",null,"Reck","Chief Special","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":496,"d":"496 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"Lager und Öffnung versetzt","Zusatzlauf","M10fein","SA/DA",null,"HammerBlock","Schwenktommel","manueller Ausstosser","Druckguss verchromt",null,"Druckguss verchromt","Druckguss verchromt","Holz weiss",null,null,"94","S&W 66, Chief Soecial",{"$nulls":3},"gebraucht gut"]
["503",null,"Revolver",null,"Reck","Chief Special","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":492,"d":"492 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"Lager und Öffnung versetzt","Zusatzlauf","M10fein","SA/DA",null,"HammerBlock","Schwenktommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",null,null,"93","S&W 66, Chief Soecial",{"$nulls":3},"neu"]
["513",null,"Pistole","Automatik","Reck","Double Eagle","Deutschland","8mm Knall",{"$nulls":5},{"v":1074,"d":"1,074 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M8","SA/DA","keine","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","E00237","Köln","94","Colt Double Eagle",null,"Schlittenfang ohne Funktion",null,"neu, Lagerspuren"]
["517",null,"Pistole","Automatik","FB Rekord","Rekord 08","Deutschland","8mm Knall","6","219","36","138","10,5/4,25","xx","vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M8","Schlagbolzenschloss","Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz",{"$nulls":3},"Luger P08","IWG Lange 08 PTB701","Kniegelenk ohne echte Funktion",null,"stark gebraucht, Ausbruch am Gabelende, Kniegelenk gebrochen, Riegelnut gebrochen"]
["517",null,"Pistole","Automatik","IWC/Enser","Parabellum 08","Deutschland","8mm Knall","6","219","36","138","10,5/4,25",{"v":868,"d":"868 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M8","Schlagbolzenschloss","Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz",null,"Köln","94","Luger P08","IWG Lange 08 PTB701","Kniegelenk ohne echte Funktion",null,"gebraucht"]
["518",null,"Pistole","Automatik","Valtro/ME","98 Civil","Italien","9mm P.A.Knall","12",{"$nulls":4},{"v":1097,"d":"1,097 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA","Hahn/Schlagbolzen, Drehflügel","Trägheitsschlagbolzen","Magazin","automatischer Auswurf","Druckgus brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","C01959",null,"91","Beretta 92",{"$nulls":3},"stark gebraucht, Sicherung leicht defekt"]
["519",null,"Pistole","Automatik","ME","ME 8 Police","Italien","8mm Knall",null,"152","28","114",null,{"v":673,"d":"673 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","075034","Köln","90","Walther PPK",null,"Sicherungshebel an anderer Stelle als beim Original",null,"gebraucht, stark abgegriffen"]
["520",null,"Pistole","Automatik","Valtro/ME","85 Combat","Italien","9mm P.A.Knall",{"$nulls":5},{"v":758,"d":"758 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Hahn/Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",{"$nulls":3},"Beretta 84F",null,"Schlagbolzen sehr bruchgefährdet",null,"gebraucht gut"]
["523",null,"Pistole","Automatik","IWC","Government","Deutschland","9mm P.A.Knall",{"$nulls":5},{"v":1000,"d":"1,000 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M8","SA","Hahn/Schlitten, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss verchromt","Druckguss verchromt","Druckguss verchromt",null,"Hartgummi weiss","4830","Köln","2003","Colt 1911","Reck Government",null,null,"neu"]
["527",null,"Revolver",null,"Röhm","RG59 Le Petit","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":458,"d":"458 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun","0518279","Ulm","2001",{"$nulls":4},"gebraucht gut"]
["529",null,"Gewehr","Automatik","Erma","EGG1","Deutschland","8mm Knall",{"$nulls":4},"44/17,5",{"v":2570,"d":"2,570 g"},"vorn","Stahleinsatz im lauf","Lager und Öffnung versetzt",null,null,"n",null,"Schlagbolzenschloss","Abzug, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert",null,"Stahl brüniert",null,"Holz","80","München","90","M1 Carbine",null,null,"Einziger Schreckschuss Hallbautomat","gebraucht"]
["531",null,"Pistole","Automatik","Reck","Government","Deutschland","8mm Knall",{"$nulls":5},{"v":1109,"d":"1,109 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA ","Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Hartgummi weiss",null,"Köln","91","Colt 1911",null,null,"Umbau mit SportClub-Teilen und Gürtelclip","gebraucht gut"]
["532",null,"Revolver",null,"Hege","Army 1873","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"19/7,5",{"v":1222,"d":"1,222 g"},"seitlich","Stahlstück, Lauf verschlossen",null,null,"Lager und Öffnung versetzt","n","n","SA",null,"Hahnrast","Ladeklappe","manuell per Schieber","Stahl buntgehärtet",null,"Stahl mitternachtsblau","Stahl mitternachtsblau","Staht mitternachtsblau, Holz","114491",null,null,"Colt SAA",null,null,"auch in anderen, auch scharfen Kalibern erhältlich","radiale Schäden in Laufbläuung","Pappschachtel"]
["533",null,"Pistole","Automatik","Brixia/ME","mod.92 Army","Italien","8mm Knall","18",{"$nulls":4},{"v":940,"d":"940 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel","kurzer Schlagbolzen","Magazin","automatischer Auswurf","Aludruckguss silber eloxiert","Druckguss schwarz lackiert","Aludruckguss silber eloxiert",null,"Kunststoff schwarz","A18518B","Köln","92","Beretta 92 Army",{"$nulls":3},"gebraucht gut"]
["537",null,"Pistole","Automatik","ME","ME 800 General","Italien","8mm Knall",{"$nulls":5},{"v":1165,"d":"1,165 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA","keine","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz, aktueller Satz Eigenbau","9C608",null,"92","Colt 1911",null,"keine Sicherung, Schlittenfang nur manuell zu bedienen, \"nicht zerlegbar\"",null,"neu","Pappschachtel"]
["537",null,"Pistole","Automatik","ME","ME 800 General","Italien","8mm Knall",{"$nulls":5},{"v":1145,"d":"1,145 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA","keine","keine","Magazin","automatischer Auswurf","Druckguss verchromt","Druckguss verchromt","Druckguss verchromt",null,"Holz","254666","Italien",null,"Colt 1911",null,"keine Sicherung, Schlittenfang nur manuell zu bedienen, \"nicht zerlegbar\"",null,"neu","Pappschachtel"]
["539",null,"Selbstschussgerät",null,"Kieferle",null,"Deutschland","Kal.16 Alarm","1",{"$nulls":4},{"v":1004,"d":"1,004 g"},"vorn",{"$nulls":4},"n",null,"Stift mit Klinke","Klappbügel",null,"Verschraubung",null,"Stahl gelb verzinkt",null,"Stahl geschwärzt",{"$nulls":9},"neu"]
["540",null,"Pistole","Automatik","ME","ME 9 PP","Deutschland","9mm P.A.Knall",{"$nulls":5},{"v":578,"d":"578 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M8","SA/DA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff schwarz","10429","Köln","94","Walther PP","IWG P900 PTB660",null,null,"gebraucht","Kunststoffkoffer"]
["541",null,"Pistole","Automatik","Heckler+Koch","SP 9","Deutschland","9mm P.A.Knall",null,"125","29","128","10/4",{"v":778,"d":"778 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Griffstück","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,"Köln","92","Heckler+Koch P7",{"$nulls":3},"gebraucht","Pappschachtel"]
["541",null,"Pistole","Automatik","IWG","SP 9","Deutschland","9mm P.A.Knall",null,"125","29","128","10/4",{"v":784,"d":"784 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Griffstück","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","6088","Köln","94","Heckler+Koch P7",{"$nulls":3},"gebraucht","Pappschachtel"]
["549",null,"Revolver",null,"Röhm","Little Joe","Deutschland","6mm Flobert Platz","5",{"$nulls":4},{"v":134,"d":"134 g"},"vorn","Stahlbolzen seitlich im Lauf",null,null,"Hartmetallkern","Zusatzlauf",null,"SA",null,"Hammerblock","Schwenktrommel","manuell per Stift","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun","0633903",null,null,"NAA ","PTB 349",null,null,"neu","Pappschachtel"]
["550",null,"Derringer",null,"Noris","Twinny","Deutschland",".380Knall/9mm Knall","2",{"$nulls":4},{"v":384,"d":"384 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M12","SA mit wechselseitig kippenden Schlagstück","Hahn, Drehhebel","Hahnrast","Kipplauf","manuell per Schieber","Druckguss brüniert",null,"Druckguss brüniert",null,"Kunststoff schwarz",{"$nulls":6},"Modell von Röhm, aber Alleinvertrieb von Noris","gebraucht gut","Pappschachtel"]
["551",null,"Pistole","Automatik","Röhm","725","Deutschland","9mm P.A.Knall","8","197","30 (34)","130","10,5/4,2",{"v":849,"d":"849 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss mattvernickelt","Druckguss mattvernickelt","Stahl",null,"Holz",{"$nulls":4},"Identisch mit RG735, nur kürzeres Patronenlager","Flächen der Holzgriffschalen sind überschliffen, dadurch heller",null,"gebraucht, Vernickelung des Laufes blättert ab","Pappschachtel, Schaumeinlage"]
["551",null,"Pistole","Automatik","Röhm","725","Deutschland","9mm P.A.Knall","8","197","30 (34)","130","10,5/4,2",{"v":854,"d":"854 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss mattvernickelt","Druckguss mattvernickelt","Stahl",null,"Holz",null,"Ulm","94",null,"Identisch mit RG735, nur kürzeres Patronenlager",null,null,"neu","Pappschachtel, Schaumeinlage"]
["551",null,"Pistole","Automatik","Röhm","725","Deutschland","9mm P.A.Knall","8","197","30 (34)","130","10,5/4,2",{"v":831,"d":"831 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M10","SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff schwarz","637","Ulm","94",null,"Identisch mit RG735, nur kürzeres Patronenlager",null,null,"neuwertig, werksüberholt","Pappschachtel, Schaumeinlage"]
["551",null,"Pistole","Automatik","Röhm","725","Deutschland","9mm P.A.Knall","8","197","30 (34)","130","10,5/4,2",{"v":869,"d":"869 g"},"vorn","Hartmetallplatte längs im Lauf","Laufbohrung versetzt zum Lager","Einfräsung unter der Mündung",null,"Zusatzlauf","M10","SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff schwarz","0201439","Ulm","97",{"$nulls":3},"Neue Version mit schmalem Magazinschacht","neu","Pappschachtel, Schaumeinlage"]
["556",null,"Revolver",null,"HS","Buffalo","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":873,"d":"873 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Hartmetallkern","Zusatzlauf","M10","SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstoßer","Druckguss mattverchromt",null,"Druckguss mattverchromt","Druckguss mattverchromt","Holz",null,"Ulm","93",null,"ME 45",null,null,"gebraucht gut"]
["560",null,"Pistole","Automatik","Erma","EGP 315","Deutschland",".315Knall",null,"137","23","97",null,{"v":432,"d":"432 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8","SA","keine","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff schwarz","000226","München","93",{"$nulls":4},"neu","Pappschachtel, Styroporeinlage"]
["560",null,"Pistole","Automatik","IWC","Lady","Deutschland",".315Knall",null,"137","23","97",null,{"v":424,"d":"424 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8","SA","keine","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Schichtholz graubraun","10224","München","93",{"$nulls":4},"gebraucht sehr gut, Laufwurzel poliert"]
["561",null,"Pistole","Automatik","ME","315 Mini","Deutschland",".315Knall",null,"123","22","100",null,{"v":413,"d":"413 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,null,"93",{"$nulls":3},"ME's erste .315er","gebraucht gut, Magazinlippen vorne etwas aufgebogen","Pappschachtel"]
["568",null,"Signalgerät",null,"Reimer","Komet TM-5","Deutschland","M9/15","5",{"$nulls":4},{"v":70,"d":"70 g"},"n","kein Lauf vorhanden",{"$nulls":3},"ja","M9","Stift mit Klinke",null,"Rast","Verschraubung",null,"Kunststoff orange",{"$nulls":11},"neuwertig"]
["569",null,"Pistole","Automatik","IWC","Mod. PP","Deutschland",".315Knall",{"$nulls":5},{"v":551,"d":"551 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf","dünner Lauf",null,"Zusatzlauf","M8","SA/DA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz",null,"Köln","93","Walther PP","ME 9 PP PTB540",null,null,"gebraucht gut"]
["570",null,"Pistole","Automatik","IWG","American","Deutschland","9mm P.A.Knall",null,"184","35","143","10/4",{"v":915,"d":"915 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel","kurzer Schlagbolzen","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","15578","Köln","98","S&W 59","IWG Americal",null,null,"neu","Pappschachtel"]
["570",null,"Pistole","Automatik","IWG","Mod. 59","Deutschland","9mm P.A.Knall",null,"184","35","143","10/4",{"v":915,"d":"915 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel","kurzer Schlagbolzen","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff blaumetallic",null,"Köln","95","S&W 59","IWG Americal",null,null,"neu","Pappschachtel"]
["570",null,"Pistole","Automatik","Akah","Defense 59","Deutschland","9mm P.A.Knall",null,"184","35","143","10/4",{"v":926,"d":"926 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel","kurzer Schlagbolzen","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz",null,"Köln","93","S&W 59","IWG Americal",null,null,"neu","Pappschachtel"]
["572",null,"Pistole","Automatik","IWG","Amazone","Deutschland","9mm P.A.Knall",null,"144","26","109","7,5/3",{"v":480,"d":"480 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss mattvernickelt","Druckguss mattvernickelt","Druckguss mattvernickelt",null,"Kunststoff schwarz",null,null,"98",null,null,"Signalstift für Schlagbolzen",null,"neuwertig","Kunststoffkoffer"]
["574",null,"Pistole","Automatik","Röhm","RG800","Deutschland",".315Knall",{"$nulls":5},{"v":443,"d":"443 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun",null,null,"2000",null,"PTB 154, 412",null,null,"neu","Pappschachtel"]
["575",null,"Pistole","Automatik","Röhm","RG90","Deutschland",".315Knall",null,"144","24","98",null,{"v":451,"d":"451 g"},"vorn","Hartmetallplatte längs im Lauf","unten eingefräster Schlitz",null,null,"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff braun",null,"Ulm","94",null,"Röhm RG9",null,null,"gebraucht"]
["576",null,"Pistole","Automatik","Röhm","RG 100","Deutschland",".315Knall",null,"156","24","115",null,{"v":532,"d":"532 g"},"vorn","Hartmetallplatte längs im Lauf","unten eingefräster Schlitz","Lager versetzt zum Lauf",null,"Zusatzlauf","M8","SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss vergoldet","Druckguss vergoldet","Stahl vergoldet",null,"Holz","011","Ulm","94","Walther PPK",null,null,"Sondermodell","neu","Pappschachtel"]
["577",null,"Pistole","Automatik","Reck","PK 800","Deutschland",".315Knall","7",{"$nulls":3},"8/3,25",{"v":539,"d":"539 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf",null,"SA/DA","Schlagbolzen","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun",null,null,"94","Walther PPK","Reck PK800 PTB196 / Mauser Hsc84 PTB335ff",null,null,"neuwertig"]
["579",null,"Pistole","Automatik","Perfecta","FBI8000","Deutschland",".315Knall",null,"134","23 (25)","101",null,{"v":419,"d":"419 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M7fein","Schlagbolzenschloss","Abzug, Schubknopf","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","G295050","Köln","94",null,"PTB 386, 619, 421, 12",null,null,"neu"]
["580",null,"Pistole","Automatik","Reck","P6s","Deutschland",".315Knall",{"$nulls":5},{"v":376,"d":"376 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M7fein","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","A0 6310","Köln","95","früher auch als 6.35er Browning erhältlich, Reck P8","Reck P6 PTB 388",null,null,"gebraucht sehr gut"]
["582",null,"Pistole","Automatik","Valtro/ME","mod. 8 Mini L","Italien",".315Knall",null,"133","25","99","7/2,75",{"v":461,"d":"461 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"n",null,"SA","Abzug","Trägheitsschlagbolzen","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","G01036","Köln","94","Beretta 950/3032","Bauform wird auch in 8mm Knall, 9mmPAK und .35Knall produziert (Auslandsvertrieb)",null,null,"neuwertig","Kunststoffkoffer"]
["583",null,"Signalgerät",null,"ME","3K","Deutschland","M9/15","3",{"$nulls":4},{"v":49,"d":"49 g"},"n","kein Lauf vorhanden",{"$nulls":3},"ja",null,"Stift mit Klinke",null,"Rast","Verschraubung",null,"Kunststoff orange",null,null,"Kunststoff schwarz",{"$nulls":8},"neuwertig","Plastikbeutel"]
["586",null,"Pistole","Automatik","Mauser","HSc 84","Deutschland",".315Knall",null,"157","32","114","8/3,25",{"v":569,"d":"569 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M7fein","SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert","Kunststoff braun","A004766","Köln","94",{"$nulls":4},"gebraucht sehr gut","Kunststoffkoffer, Schaumeinlage"]
["587",null,"Pistole","Automatik","Reck","Commander","Deutschland",".315Knall",null,"157","32","114","8/3,25",{"v":600,"d":"600 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M7fein","SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert","Holz","C229578","Köln","95","Colt Commander","Reck Commander PTB238",null,"Massstab kleiner als Original","gebraucht"]
["592",null,"Pistole","Automatik","FN Browning/Umarex","GPDA 9","Deutschland","9mm P.A.Knall",null,"200","38","131","12/4,75",{"v":831,"d":"831 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf","M7fein","SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",{"$nulls":3},"Browning Hi-Power",{"$nulls":3},"gebraucht gut"]
["593",null,"Revolver",null,"Holek/Umarex","ALFA 2","Tschechien",".380Knall/9mm Knall","6",{"$nulls":3},"5/2",{"v":689,"d":"689 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"Lager und Öffnung versetzt","ja","M10fein","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Holz","4201009018","Tschechien","94",null,"Kora 007 PTB628",null,"Brünierung eher grau, wirkt parkerisiert","neuwertig"]
["594",null,"Revolver",null,"Röhm","RG 89N","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"6,3/2,5",{"v":655,"d":"655 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"Lager und Öffnung versetzt","ja","M10","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braum","0486945","Ulm","2001",null,"PTB 597",null,null,"neu"]
["596",null,"Revolver",null,"Umarex","Champion","Italien",".380Knall/9mm Knall","6",{"$nulls":3},"8/3",{"v":766,"d":"766 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Hartmetallkern","Zusatzlauf","M10fein","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss schwarz lackiert",null,"Druckguss schwarz lackiert","Druckguss schwarz lackiert","Holz","534013",{"$nulls":6},"neuwertig"]
["597",null,"Revolver",null,"Röhm","RG99n","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"4/10",{"v":760,"d":"760 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"verjüngte exzentrisch Bohrung","Zusatzlauf","M10","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz","0495125","Ulm","2001",{"$nulls":3},"Beschriftung gelasert","neuwertig"]
["598",null,"Pistole","Automatik","Reck","G5","Deutschland","9mm P.A.Knall","4","134","23 (25)","101",null,{"v":420,"d":"420 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"n","n","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","23161","Köln","94",null,"PTB 12, 386, 387, 421",null,null,"neuwertig"]
["600",null,"Revolver",null,"Röhm","RG56","Deutschland","6mm Flobert Platz","7",{"$nulls":4},{"v":467,"d":"467 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"Lager und Öffnung versetzt","Zusatzlauf","M10","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun","0595098",{"$nulls":6},"neuwertig"]
["601",null,"Revolver",null,"Erma","EGR77","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"6,25/2,5",{"v":988,"d":"988 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"Lager und Öffnung versetzt","Zusatzlauf","M8","SA/DA",null,"Hahnrückzug","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Gummi schwarz","028125","München","95","S&W","PTB 233",null,null,"gebraucht"]
["602",null,"Revolver",null,"Walther","WR 50","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":626,"d":"626 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"Lager und Öffnung versetzt","Zusatzlauf","M10fein","SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Druckguss mattvernickelt",null,"Druckguss mattvernickelt","Druckguss mattvernickelt","Holz","M6241406","Köln","96",null,"PTB 216",null,null,"neu","Kunststoffkoffer"]
["605",null,"Revolver",null,"Colt/Umarex","Anaconda","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"10/4",null,"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"Hartmetallkern","Zusatzlauf","M10fein","SA/DA",null,null,"Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",{"$nulls":4},"PTB 326","ventilierte Laufschiene",null,"neu","Kunststoffkoffer"]
["606",null,"Revolver",null,"Umarex/Browning","BR 9","Deutschland",".380Knall/9mm Knall","6",{"$nulls":4},{"v":791,"d":"791 g"},"vorn","Hartmetallplatte längs im Lauf","Bohrung nicht mittig",null,"Hartmetallkern","Zusatzlauf",null,"SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Holz",{"$nulls":7},"neu","Kunststoffkoffer"]
["607",null,"Revolver",null,"Alpina Sport/Reck","Tiger","Deutschland",".380Knall/9mm Knall","5",{"$nulls":3},"6/2,5",{"v":715,"d":"715 g"},"vorn","Hartmetallplatte längs im Lauf",null,null,"Lager und Öffnung versetzt","Zusatzlauf","M10fein","SA/DA",null,"HammerBlock","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff schwarz",null,"Köln","2000",null,"Reck Agent 9mm",null,null,"starkgebaraucht, Reste metallicblauen Lacks"]
["610",null,"Pistole","Automatik","Reck","Miami Mod.92F","Deutschland","9mm P.A.Knall","12",{"$nulls":4},{"v":1157,"d":"1,157 g"},"vorn","Hartmetallplatte längs im Lauf","Bohrung nicht mittig",null,null,"Zusatzlauf","M7fein","SA/DA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss verchromt","Druckguss verchromt","Druckguss verchromt",null,"Holz",null,null,"95","Beretta 92","PTB 481, 488",null,null,"neuwertig","Kunststoffkoffer"]
["613",null,"Pistole","Automatik","Walther/Umarex","P88 Compact/P88-9","Deutschland","9mm P.A.Knall",null,"182","34","139","10/4",{"v":973,"d":"973 g"},"vorn","Hartmetallplatte längs im Lauf","Lager und Öffnung versetzt",null,null,"Zusatzlauf","M7fein","SA/DA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss mattvernickelt","Druckguss mattvernickelt","Druckguss mattvernickelt",null,"Kunststoff schwarz","403332","Köln","98","Walther P88 Compact",null,null,"auch als P88-8 in 8mmKnall erhältlich","neuwertig"]
["614",null,"Pistole","Automatik","Reck","Double Eagle Combat Commander","Deutschland","9mm P.A.Knall",{"$nulls":5},{"v":1047,"d":"1,047 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","keine","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","D7053640","Köln","97","Colt Double Eagle","PTB 513","Schlittenfang ohne Funktion",null,"neuwertig"]
["617",null,"Revolver",null,"S&W/Umarex","Combat Magnum","Deutschland",".45short Knall","5",{"$nulls":4},{"v":705,"d":"705 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,null,"Zusatzlauf",null,"SA/DA",null,"ja","Schwenktrommel","manueller Ausstosser","Druckguss mattvernickelt",null,"Druckguss mattvernickelt","Druckguss mattvernickelt","Holz","H8149708",null,"98","S&W Combat Magnum","Reck Agent, PTB501",null,"Beschriftung gelasert","neu"]
["619",null,"Pistole","Automatik","Reck","G5 Light","Deutschland",".315Knall",null,"134","23 (25)","101",null,{"v":260,"d":"260 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Kunststoff schwarz","Druckguss brüniert","Kunststoff schwarz",null,"Kunststoff schwarz","27667","Köln","94",null,"PTB 12, 386, 387, 421",null,null,"neu","Kunststoffkoffer"]
["619",null,"Pistole","Automatik","Reck","G5 Light","Deutschland",".315Knall",null,"134","23 (25)","101",null,{"v":262,"d":"262 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Kunststoff schwarz","Druckguss verchromt","Kunststoff schwarz",null,"Kunststoff schwarz","27486","Köln","94",null,"PTB 12, 386, 387, 421",null,null,"neuwertig"]
["621",null,"Pistole","Automatik","SM","Mod. 15s","Deutschland",".315Knall",null,"116","23","98",null,{"v":403,"d":"403 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M9","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","1641","Mellrichstadt","99",null,"PTB 83/2",null,null,"neuwertig"]
["624",null,"Pistole","Automatik","SM","Cop","Deutschland",".315Knall",null,"157","31","117","8,5/3,5",{"v":632,"d":"632 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8","SA/DA","Schlagbolzen, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,null,"01",null,"PTB 625",null,null,"neu","Pappschachtel"]
["625",null,"Pistole","Automatik","SM","Cop","Deutschland","9mm P.A.Knall",null,"157","31","117","8,5/3,5",{"v":613,"d":"613 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8","SA/DA","Schlagbolzen, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss matt verchromt","Druckguss matt verchromt","Druckguss matt verchromt",null,"Holz",null,null,"01",null,"PTB 624",null,null,"neu","Pappschachtel"]
["626",null,"Selbstschussgerät",null,"Kieferle",null,"Deutschland",".380Knall/9mm Knall","1",{"$nulls":3},"1/0,4",{"v":481,"d":"481 g"},"vorn","keiner","keiner",null,null,"n",null,"Schnapphahn","Stahlring","keine","Schraubverschluss","manuell","Stahl",null,"Stahl",{"$nulls":4},"2004",{"$nulls":4},"neu"]
["628",null,"Revolver",null,"Kora","007","Tschechien",".380Knall/9mm Knall","6",{"$nulls":4},{"v":725,"d":"725 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"n","n","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Holz","100234","Suhl","93",null,"Röhm RG69 (RG89,99)",null,null,"neuwertig"]
["629",null,"Pistole","Automatik","ME","315 Mini-L","Deutschland",".315Knall",null,"123","22","100",null,{"v":418,"d":"418 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8 fein","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,null,"94",null,"PTB561",null,null,"gebraucht gut, Magazinlippen vorne etwas aufgebogen"]
["629",null,"Pistole","Automatik","ME","315 Mini-L","Deutschland",".315Knall",null,"123","22","100",null,{"v":427,"d":"427 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8 fein","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss matt verchromt","Druckguss matt verchromt","Druckguss matt verchromt",null,"Kunststoff schwarz","109160",null,"94",null,"PTB561",null,null,"gebraucht gut"]
["630",null,"Pistole","Automatik","ME","8 Liberty-L","Deutschland",".315Knall",null,"148","26","118",null,{"v":502,"d":"502 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel","kurzer Schlagbolzen","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",null,"Köln","98",{"$nulls":4},"neu","Kunststoffkoffer"]
["633",null,"Pistole","Automatik","Röhm","RG70","Deutschland",".315Knall",null,"136","25 (27)","90",null,{"v":384,"d":"384 g"},"vorn","Hartmetallplatte längs im Lauf","unten eingefräster Schlitz",null,null,"Zusatzlauf",null,"SA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff braun",{"$nulls":7},"neu","Pappschachtel"]
["635",null,"Pistole","Automatik","Reck","Pobeda","Deutschland","9mm P.A.Knall",null,"170","26 (29)","114","10/4",{"v":650,"d":"650 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA",null,null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun","B257598","Köln","95","Makarov",null,null,"Beschriftung in kyrillischer Schrift","neu","Holzkiste, innen passend gefräst"]
["636",null,"Pistole","Automatik","Geco","225","Deutschland","9mm P.A.Knall",null,"180","33 (36)","132","9,5/3,75",{"v":996,"d":"996 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf",null,"SA/DA","Entspannhebel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","DN03716",null,null,"SigSauer P225",null,"Funktion des Schlittenfangs nicht wie Original",null,"neuwertig","Kunststoffkoffer"]
["637",null,"Pistole",null,"Walther/Umarex","P99","Deutschland","9mm P.A.Knall",null,"180","32","138","10/4",null,"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M10","SA/DA","Entspanntaste",null,"Magazin","automatischer Auswurf","Kunststoff schwarz","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",{"$nulls":3},"Walther P99",null,"nicht funktionstüchtig, Schlagkraft des Hahns unzureichend, Entspanntaste ohne Funktion","alte Version mit grossem Laufgewinde","gebraucht, defekt","Kunststoffkoffer"]
["638",null,"Pistole","Automatik","Walther","Big Bore","Deutschland","9mm P.A.Knall",{"$nulls":5},{"v":970,"d":"970 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8fein","SA","Hahn/Schlitten, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss mattvernickelt","Druckguss mattvernickelt","Druckguss mattvernickelt",null,"Hartgummi schwarz","6141937","Köln","96","Colt 1911",{"$nulls":3},"gebraucht","Kunststoffkoffer"]
["639",null,"Pistole","Automatik","Alpina Sport/Reck","Mod. Panther","Deutschland","9mm P.A.Knall","4","134","23 (25)","101",null,{"v":415,"d":"415 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","00486","Köln","98",null,"PTB 12, 386, 387, 421, 598",null,null,"neuwertig"]
["640",null,"Pistole","Automatik","S&W/Umarex","Mod. 5904","Deutschland","9mm P.A.Knall",null,"184","35","143","10/4",{"v":925,"d":"925 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8fein","SA/DA","Schlagbolzen, Drehfügel","kurzer Schlagbolzen","Magazin","automatischer Ausstosser","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","P9243863","Köln","99","S&W 59","PTB 570",null,null,"gebraucht"]
["642",null,"Pistole","Automatik","BBM","Mini .315 Auto-L","Italien",".315Knall",null,"122","26","94","6,3/2,5",{"v":438,"d":"438 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA","Abzug, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz",{"$nulls":3},"Tanfoglio PT27/PT28","Gleiche Bauform wie Mauser WTP PTB407",null,null,"gebraucht","Kunststoffkoffer"]
["643",null,"Pistole","Automatik","Valtro/ME","9 Mini","Italien","9mm P.A.Knall",null,"133","25","99","7/2,75",{"v":475,"d":"475 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA","Abzug",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","F41287","Italien",null,"Beretta 950/3032","Bauform wird auch in 8mm Knall, .315Knall und .35Knall produziert (Auslandsvertrieb)",null,null,"neuwertig","Kunststoffkoffer"]
["644",null,"Pistole","Automatik","ME","ME 9 Mod. Para Sport","Deutschland","9mm P.A.Knall",null,"177","29","121","10/4",{"v":677,"d":"677 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss mattverchromt","Druckguss brüniert","Druckguss mattverchromt",null,"Holz","7350","Köln","94","Walther PP","Me 9 Falcon","schräge Schlitze in Schlitten, Magazinknopf aus Patronenboden","trotz anderem Schlitten gleiche PTB wie ME 9 Falcon","neu","Kunststoffkoffer"]
["644",null,"Pistole","Automatik","ME","ME 9 Falcon","Deutschland","9mm P.A.Knall",null,"177","31","121","10/4",{"v":692,"d":"692 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss vergoldet","Druckguss brüniert",null,"Holz","423","Suhl","94",null,"M9 PP, ME 9 Para Sport",null,"trotz anderem Schlitten gleiche PTB wie ME 9 PP und 9 Para Sport","neuwertig"]
["645",null,"Pistole","Automatik","Erma","EGP 790","Deutschland","9mm P.A.Knall",null,"157","25 (27)","115",null,{"v":537,"d":"537 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf","Ausschuss außermittig",null,"Zusatzlauf","M8fein","SA/DA","Schlagbolzen, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl blank",null,"Holz","011494","München","95","Walther PPK",{"$nulls":3},"neu","Pappschachtel"]
["647",null,"Pistole","Automatik","Erma","EGP 490","Deutschland","9mm P.A.Knall",null,"160","29","126","8,5/3,25",{"v":570,"d":"570 g"},"vorn","Hartmetallplatte längs im Lauf","Bohrung nicht mittig",null,null,"Zusatzlauf","M8fein","SA/DA","Schlagbolzen, Drehflügel","kurzer Schlagbolzen","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl blank",null,"Gummi schwarz","11891","Suhl","00",null,"Rahmen PTB 655",null,null,"neuwertig","Pappschachtel"]
["654",null,"Revolver",null,"SM","Chief","Deutschland",".380Knall/9mm Knall","6",{"$nulls":3},"7,5/3","684g","vorn","Hartmetallplatte längs im Lauf","Bohrung nicht mittig",null,"Lager und Öffnung versetzt","Zusatzlauf",null,"SA/DA",null,"Hammerblock","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Druckguss brüniert","Kunststoff braun",null,"Mellrichstadt","94",{"$nulls":4},"gebraucht"]
["655",null,"Pistole","Automatik","Erma","EGP 459","Deutschland","9mm P.A.Knall",null,"170","27","127","9,5/3,75",{"v":598,"d":"598 g"},"vorn","Hartmetallplatte längs im Lauf","Bohrung nicht mittig",null,null,"Zusatzlauf","M8fein","SA/DA","Schlagbolzen, Drehflügel","kurzer Schlagbolzen","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl blank",null,"Kunststoff schwarz","012434","München","95",null,"Rahmen PTB 647",null,null,"neuwertig","Pappschachtel"]
["658",null,"Pistole","Automatik","Valtro/ME","mod. 8 Mini L","Italien",".315Knall",null,"133","25","99","7/2,75",{"v":485,"d":"485 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA","Abzug","kurzer Schlagbolzen","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","C04375","Köln","94","Beretta 950/3032","Bauform wird auch in 8mm Knall, .315Knall und .35Knall produziert (Auslandsvertrieb)",null,null,"neuwertig","Kunststoffkoffer"]
["658",null,"Pistole","Automatik","Valtro/ME","mod. 8 Mini L","Italien",".315Knall",null,"133","25","99","7/2,75",{"v":483,"d":"483 g"},"vorn","Hartmetallplatte längs im Lauf",{"$nulls":3},"Zusatzlauf",null,"SA","Abzug","kurzer Schlagbolzen","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","G03875","Köln","94","Beretta 950/3032","Bauform wird auch in 8mm Knall, .9mmP.A.Knall und .35Knall produziert (Auslandsvertrieb)",null,null,"neuwertig","Kunststoffkoffer"]
["659",null,"Revolver",null,"Weihrauch","HW 88 Airweight","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":372,"d":"372 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"verjüngte Bohrung, Stahlbolzen","Zusatzlauf","M10","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Aludruckguss schwarz lackiert",null,"Aludruckguss schwarz lackiert","Stahl brüniert","Holz",{"$nulls":5},"Gewindeschutz, mit Alutrommel als SuperAirweight erhältlich",null,"gebraucht","Pappschachtel"]
["660",null,"Pistole","Automatik","IWG","P900","Deutschland","9mm P.A.Knall",null,"165","28","121","9,6/3,75",{"v":570,"d":"570 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M10fein","SA/DA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","10814",null,"96","Walther PP","ME 9 PP PTB540",null,null,"gebraucht gut"]
["668",null,"Pistole","Automatik","IWG","Gouverneur","Deutschland","9mm P.A.Knall",{"$nulls":5},{"v":965,"d":"965 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf","Ausschuss außermittig",null,"Zusatzlauf","M8","SA","Hahn/Schlitten, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss mattvernickelt","Druckguss brüniert","Druckguss mattvernickelt",null,"Hartgummi schwarz","10202","Köln","96","Colt 1911","Reck Government",null,null,"gebraucht","Kunststoffkoffer"]
["670",null,"Pistole","Automatik","Röhm","RG 88","Deutschland","9mm P.A.Knall",null,"158","27 (31)","114","9/3,5",{"v":586,"d":"586 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M10","SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl ",null,"Kunststoff schwarz","0266077","Ulm","98",{"$nulls":4},"stark gebraucht, Brünierung teils abgegriffen"]
["672",null,"Pistole","Automatik","Geco","P217","Deutschland","9mm P.A.Knall",null,"202","30","138","10,6/4,25",{"v":545,"d":"545 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M10","DAO",null,"DAO","Magazin","automatischer Auswurf","Kunststoff schwarz","Druckguss brüniert","Stahl blank",null,"Kunststoff schwarz","013703","München","95","Glock 17",null,"keine Abzugssicherung wie beim Vorbild",null,"neuwertig","Kunststoffkoffer"]
["672",null,"Pistole","Automatik","Geco","P217","Deutschland","9mm P.A.Knall",null,"202","30","138","10,6/4,25",{"v":529,"d":"529 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M10","DAO",null,"DAO","Magazin","automatischer Auswurf","Kunststoff schwarz","Druckguss brüniert","Stahl brüniert",null,"Kunststoff schwarz",{"$nulls":3},"Glock 17",null,"keine Abzugssicherung wie beim Vorbild",null,"neu","Kunststoffkoffer"]
["679",null,"Pistole","Automatik","ME","69 mod. Springfield","Deutschland","9mm P.A.Knall",null,"174","35","139","10/4",{"v":984,"d":"984 g"},"vorn","Hartmetallplatte längs im Lauf","Lager und Öffnung versetzt",null,null,"Zusatzlauf","M10","SA/DA","Schlagbolzen, Drehflügel","kurzer Schlagbolzen","Magazin","automatischer Auswurf","Druckguss mattvernickelt","Druckguss mattvernickelt","Stahl mattvernickelt",null,"Kunststoff schwarz","12126",null,"99",null,null,"neues Modell der ME 9 Mini Para PTB479",null,"gebraucht gut","Kunststoffkoffer"]
["689",null,"Pistole","Automatik","Valtro/ME","mod. 8000 F.S.","Italien","9mm P.A.Knall",{"$nulls":5},{"v":962,"d":"962 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf",null,"SA/DA","Drehflügel","kurzer Schlagbolzen","Magazin","automatischer Auswurf","Druckguss anthrazit verchromt, vergoldet","Druckguss anthrazit verchromt, vergoldet","Druckguss anthrazit verchromt",null,"Kunststoff schwarz","J01017","Italien",null,"Beretta Cougar",null,null,"Dekor hauptsächlich für Südosteuropa hergestellt","neu","Kunststoffkoffer"]
["693",null,"Revolver",null,"Holek","model 040","Tschechien",".380Knall/9mm Knall","6",{"$nulls":3},"4/10",{"v":800,"d":"800 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"verjüngte exzentrische Bohrung","Zusatzlauf","M10 fein","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss verchromt",null,"Druckguss verchromt","Stahl verchromt","Kunststoff schwarz","6040024163","Tschechien","96",null,"Röhm RG99n PTB 597, Mercury M2 PTB752",null,null,"gebraucht sehr gut","Pappschachtel"]
["694",null,"Revolver",null,"IWG","Special Force","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":665,"d":"665 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,"Lager und Öffnung versetzt","Zusatzlauf","M10fein","SA/DA",null,"HammerBlock","Schwendtrommel","manueller Ausstosser","Druckguss mattvernickelt",null,"Druckguss mattvernickelt","Druckguss mattvernickelt","Holz","18244",null,"98",null,null,"Trommelentriegelung über Druckknopf",null,"neu","Kunststoffkoffer"]
["696",null,"Pistole","Automatik","SigSauer","P239","Deutschland","9mm P.A.Knall",null,"172","31 (33)","131","9,5/3,75",{"v":888,"d":"888 g"},"vorn","Hartmetallplatte längs im Lauf","Lager und Öffnung versetzt",null,null,"Zusatzlauf","M10fein","SA/DA","Entspannhebel","Hahnrast","Magazin","automatischer Auswurf","Druckguss mattvernickelt","Druckguss mattvernickelt","Stahl mattvernickelt",null,"Kunststoff schwarz","12607",null,"99","SigSauer P239",{"$nulls":3},"neu"]
["698",null,"Revolver",null,"Luger","R94","Tschechien",".380Knall/9mm Knall","6",{"$nulls":3},"4/10",{"v":786,"d":"786 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"verjüngte exzentrische Bohrung","Zusatzlauf","M10 fein","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss verchromt",null,"Druckguss verchromt","Stahl verchromt","Kunststoff braun","8040033077","Tschechien","98",null,"Röhm RG99n PTB 597, Mercury M2 PTB752",null,null,"neuwertig"]
["699",null,"Pistole","Automatik","Röhm","RG96","Deutschland","9mm P.A.Knall",null,"187","30 (36)","133","10/4",{"v":799,"d":"799 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8fein","SA/DA","Schloss, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Kunststoff grün","Druckguss grün lackiert","Stahl",null,"Kunststoff grün","0579954","Ulm","2002","Heckler+Koch",null,null,"Sondermodell in grün incl. Sicherheitskompensator","neu","Kunststoffkoffer"]
["699",null,"Pistole","Automatik","Röhm","RG96","Deutschland","9mm P.A.Knall",null,"187","30 (36)","133","10/4",{"v":799,"d":"799 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8fein","SA/DA","Schloss, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Kunststoff schwarz","Druckguss glanzbrüniert","Stahl",null,"Kunststoff schwarz",null,"Ulm","1996","Heckler+Koch",null,null,"Altes Modell","stark gebraucht"]
["700",null,"Pistole","Automatik","IWG","Parabellum 08","Deutschland",".315Knall","6","219","36","138","10,5/4,25",{"v":826,"d":"826 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M10fein","Schlagbolzenschloss","Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz",null,"Köln",null,"Luger P 08","FB Rekord 08 PTB480","Kniegelenk ohne echte Funktion",null,"neuwertig"]
["701",null,"Pistole","Automatik","IWG","Lange 08","Deutschland",".315Knall","6","285","36","138","13,5/5,5",{"v":898,"d":"898 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M10fein","Schlagbolzenschloss","Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz","03515","Köln","97","Lange Luger P 08","FB Rekord 08 PTB480","Kniegelenk ohne echte Funktion",null,"neuwertig"]
["701",null,"Pistole","Automatik","IWG","Lange 08","Deutschland",".315Knall","6","284","36","138","13,5/5,5",{"v":907,"d":"907 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M10fein","Schlagbolzenschloss","Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Holz","03661","Köln","97","Lange Luger P 08","FB Rekord 08 PTB480","Kniegelenk ohne echte Funktion","Anschlagbrett","neu"]
["720",null,"Revolver",null,"Wadie","P1","Deutschland","9mm P.A.Knall","5",{"$nulls":4},{"v":541,"d":"541 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"verjüngte Bohrung","Zusatzlauf","M10","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss mattverchromt",null,"Druckguss mattverchromt","Stahl mattverchromt","Holz",null,"Mellrichstadt","97",null,"Rahmen HW37","Gewindeschutz","verschießt Pistolenmunition","gebraucht gut","Kunststoffkoffer"]
["722",null,"Pistole","Automatik","Mauser/Röhm","HSc Mod. 90","Deutschland","9mm P.A.Knall","7","158","27 (31)","114","9/3,5",{"v":606,"d":"606 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8fein","SA/DA","Schlagbolzen, Drehflügel mit Entspannfunktion","keine","Magazin","automatischer Auswurf","Druckguss mattvernickelt","Druckguss mattvernickelt","Stahl mattvernickelt",null,"Kunststoff schwarz","MW06225","Ulm","99",null,"Röhm RG88",null,null,"neu"]
["727",null,"Pistole","Automatik","IWG","Defender","Deutschland","9mm P.A.Knall",null,"186","31 (35)","138","10,5/4,2",{"v":902,"d":"902 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8","SA/DA","Schlagbolzen, Drehflügel","Trägheitsschlagbolzen","Magazin","automatischer Auswurf","Druckguss mattvernickelt","Druckguss mattvernickelt","Druckguss mattvernickelt",null,"Kunststoff schwarz","18243","Köln","98",null,"IWG American, Akah Defense 59",null,null,"gebraucht"]
["737",null,"Revolver",null,"Shield","RD6","Tschechien",".380Knall/9mm Knall","6",{"$nulls":3},"6/15",{"v":908,"d":"908 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"verjüngte exzentrisch Bohrung","Zusatzlauf","M10fein","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss brüniert",null,"Druckguss brüniert","Stahl brüniert","Kunststoff schwarz","8060036577","Tschechien","98",null,"Mercury, Alfa, Holek",null,null,"neuwertig","Kunststoffkoffer, Schaumeinlage"]
["744",null,"Pistole","Automatik","IWG","P315","Deutschland",".315Knall",null,"165","28","121","9,6/3,75",{"v":539,"d":"539 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss mattvernickelt","Druckguss mattvernickelt","Stahl mattvernickelt",null,"Kunststoff schwarz","71295","Köln","2000","Walther PP","ME 9 PP PTB540",null,null,"gebraucht gut"]
["745",null,"Pistole","Automatik","IWG ","SP15","Deutschland","9mm P.A.Knall",null,"175","30 (35)","128","9,5/3,75",{"v":635,"d":"635 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf",null,"SA/DA","Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Kunststoff schwarz","Druckguss mattvernickelt","Druckguss brüniert",null,"Kunststoff schwarz",null,"Köln","98","Heckler+Koch",{"$nulls":3},"gebraucht gut","Kunststoffkoffer"]
["748",null,"Pistole","Automatik","SM","Mod. 15-9","Deutschland","9mm P.A.Knall",null,"116","23","98",null,{"v":379,"d":"379 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M9x1","Schlagbolzenschloss","Abzug, Drehflügel","keine","Magazin","manueller Ausstosser","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff braun","1907","München","98",null,"SM 15 PTB 83/2",null,null,"gebraucht gut"]
["749",null,"Pistole","Automatik","Röhm","Vector CP1","Deutschland","9mm P.A.Knall","13","180","29","139","10/4",{"v":682,"d":"682 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf",null,"SA/DA",null,"Hahnrast","Magazin","automatischer Auswurf","Kunststoff schwarz","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","0284857","Ulm","98","Vector CP1",{"$nulls":3},"gebraucht, Brünierung am Schlitten teilweise fleckig"]
["751",null,"Revolver",null,"Mercury","M1 Lightning","Tschechien",".380Knall/9mm Knall","6",{"$nulls":3},"2/5",{"v":739,"d":"739 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"verjüngte exzentrisch Bohrung","Zusatzlauf","M10x1","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss verchromt",null,"Druckguss brüniert","Stahl verchromt","Holz","5020061468","Tschechien","2005",{"$nulls":4},"neu","Kunststoffkoffer, Schaumeinlage"]
["752",null,"Revolver",null,"Mercury","M2 Thunder","Tschechien",".380Knall/9mm Knall","6",{"$nulls":3},"4/10",{"v":827,"d":"827 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"verjüngte exzentrisch Bohrung","Zusatzlauf",null,"SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss verchromt",null,"Druckguss brüniert","Stahl verchromt","Gummi","1040051364","Tschechien","2001",null,"Röhm RG99n PTB 597",null,null,"neuwertig","Pappschachtel"]
["762",null,"Pistole",null,"Walther/Umarex","P99","Deutschland","9mm P.A.Knall",{"$nulls":5},{"v":647,"d":"647 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8fein","SA/DA","Entspanntaste",null,"Magazin","automatischer Auswurf","Kunststoff schwarz","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","B0139755",null,"2000","Walther P99",null,null,"neue Version mit kleinem Laufgewinde","gebraucht gut"]
["765",null,"Pistole","Automatik","Reck","PPK","Deutschland","9mm P.A.Knall",null,"171","28","111","10/4",{"v":575,"d":"575 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf","dünnes Laufröhrchen",null,"Zusatzlauf",null,"SA/DA","Schlagbolzen, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Stahl",null,"Kunststoff schwarz","G44936852","Köln","2004","Walther PP","IWG P900 PTB660",null,null,"gebraucht"]
["769",null,"Pistole","Automatik","Reck","Double Eagle","Deutschland","9mm P.A.Knall",{"$nulls":5},{"v":1143,"d":"1,143 g"},"vorn","sternförmige Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M9x1","SA/DA","keine","Hahnrast","Magazin","automatischer Auswurf","Druckguss mattvernickelt","Druckguss mattvernickelt","Druckguss mattvernickelt",null,"Kunststoff schwarz","D84247763","Köln","2003","Colt Double Eagle",null,"Schlittenfang ohne Funktion",null,"gebarucht gut, Vernickelung pickelig","Kunststoffkoffer"]
["774",null,"Pistole","Automatik","Umarex/Colt","1911","Deutschland","9mm P.A.Knall",{"$nulls":5},{"v":954,"d":"954 g"},"vorn","sternförmige Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8","SA","Hahn/Schlitten, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Hartgummi schwarz","D34949428","Köln","2003","Colt 1911","Reck Government",null,null,"gebraucht gut"]
["774",null,"Pistole","Automatik","Umarex/Colt","1911","Deutschland","9mm P.A.Knall",{"$nulls":6},"vorn","sternförmige Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8","SA","Hahn/Schlitten, Drehflügel","Hahnrast","Magazin","automatischer Auswurf","Druckguss mattvernickelt","Druckguss mattvernickelt","Druckguss mattvernickelt",null,null,"D45053428","Köln","2004","Colt 1911","Reck Government",null,null,"gebraucht gut"]
["775",null,"Pistole","Automatik","Reck","Defender","Deutschland","9mm P.A.Knall",null,"180","33 (36)","132","9,5/3,75",{"v":1004,"d":"1,004 g"},"vorn","Hartmetallstern im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M10fein","SA/DA","Entspannhebel","Hahnrast","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","I54307290","Köln","2005","SigSauer P225","Geco 225 PTB 636","Funktion des Schlittenfangs nicht wie Original",null,"neu","Kunststoffkoffer"]
["779",null,"Revolver",null,"Weihrauch","HW 37","Deutschland",".380Knall/9mm Knall","5",{"$nulls":4},{"v":524,"d":"524 g"},"vorn","Hartmetallplatte längs im Lauf","Lauf zur Trommelbohrung versetzt",null,"verjüngte Bohrung, Stahlbolzen","Zusatzlauf","M10","SA/DA",null,"TransferBar","Schwenktrommel","manueller Ausstosser","Druckguss verchromt",null,"Druckguss verchromt","Stahl verchromt","Hartgummi schwarz","1457871","Mellrichstadt","2003",{"$nulls":4},"neuwertig"]
["839",null,"Pistole","Automatik","Kimar/ME","Mod. 85 Auto","Italien","9mm P.A.Knall",{"$nulls":5},{"v":919,"d":"919 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8","SA/DA","Schloss, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss brüniert","Druckguss brüniert","Druckguss brüniert",null,"Kunststoff schwarz","C25474","Italien",null,"Beretta 85",{"$nulls":3},"neu","Kunststoffkoffer, Schaumeinlage"]
["845",null,"Pistole","Automatik","Kimar/ME","Mod.92 AUTO","Italien","9mm P.A.Knall",{"$nulls":5},{"v":1226,"d":"1,226 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8","SA/DA","Schlagbolzen, Drehflügel","keine","Magazin","automatischer Auswurf","Druckguss verchromt","Druckguss verchromt","Druckguss verchromt",null,"Kunststoff schwarz","C11983","Italien",null,"Beretta 92",{"$nulls":3},"neuwertig","Kunststoffkoffer, Schaumeinlage"]
["854",null,"Pistole","Automatik","Kimar/ME","Mod. 75 Auto","Italien","9mm P.A.Knall",null,"204","36 (39)","141","11,5/4,5",{"v":928,"d":"928 g"},"vorn","Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8fein","SA/DA","Schloss, Drehflügel",null,"Magazin","automatischer Auswurf","Druckguss mattverchromt","Druckguss mattverchromt","Druckguss mattverchromt",null,"Kunststoff schwarz","B87553","Italien","2003","CZ75",{"$nulls":3},"neu","Kunststoffkoffer, Schaumeinlage"]
["865",null,"Pistole","Automatik","Schmeisser","Mod.51","Ukraine","9mm P.A.Knall",null,"155","31","116",null,{"v":560,"d":"560 g"},"vorn","sternförmige Hartmetallplatte längs im Lauf","Lager versetzt zum Lauf",null,null,"Zusatzlauf","M8fein","SA/DA","Schlagbolzen, Drehflügel","Trägheitsschlagbolzen","Magazin","automatischer Auswurf","Druckguss verchromt","Druckguss verchromt","Stahl verchromt",null,"Kunststoff schwarz","000110","Köln","2005","Walther PPK",{"$nulls":3},"neu","Pappschachtel"]